{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["EFLH","C&HLH","SC Test Runs","Original Schedule","BINs","HVAC Calculator","Warning","Appendix E (Ref. Table)","Change Log"],"not_rendered":{"charts":11,"images":10,"macros":1,"external_links":0,"defined_names":10,"comments":5,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"EFLH","index":0,"n_rows":2273,"n_cols":31,"rows_kept":2273,"cut":false,"hidden":true,"merged":[[1155,0,1157,0],[1158,0,1160,0],[1102,0,1102,19],[1124,0,1124,1],[1125,0,1127,0],[1128,0,1130,0],[1132,0,1132,19],[1154,0,1154,1],[1095,0,1097,0],[1098,0,1100,0],[982,0,982,19],[1012,0,1012,19],[1042,0,1042,19],[1072,0,1072,19],[1064,0,1064,1],[1065,0,1067,0],[1068,0,1070,0],[1094,0,1094,1],[973,0,973,1],[974,0,976,0],[977,0,979,0],[1034,0,1034,1],[1035,0,1037,0],[1038,0,1040,0],[1004,0,1004,1],[1005,0,1007,0],[1008,0,1010,0],[906,0,906,13],[923,0,923,1],[924,0,926,0],[927,0,929,0],[931,0,931,13],[948,0,948,1],[949,0,951,0],[952,0,954,0],[956,0,956,13],[852,0,854,0],[856,0,856,13],[873,0,873,1],[874,0,876,0],[877,0,879,0],[881,0,881,13],[898,0,898,1],[899,0,901,0],[902,0,904,0],[797,0,799,0],[800,0,802,0],[804,0,804,13],[821,0,821,1],[822,0,824,0],[825,0,827,0],[831,0,831,13],[848,0,848,1],[849,0,851,0],[746,0,746,1],[747,0,749,0],[750,0,752,0],[754,0,754,13],[771,0,771,1],[772,0,774,0],[775,0,777,0],[779,0,779,13],[796,0,796,1],[679,0,679,13],[696,0,696,1],[697,0,699,0],[700,0,702,0],[704,0,704,13],[721,0,721,1],[722,0,724,0],[725,0,727,0],[729,0,729,13],[625,0,627,0],[629,0,629,13],[646,0,646,1],[647,0,649,0],[650,0,652,0],[654,0,654,13],[671,0,671,1],[672,0,674,0],[675,0,677,0],[571,0,573,0],[574,0,576,0],[578,0,578,13],[595,0,595,1],[596,0,598,0],[599,0,601,0],[604,0,604,13],[621,0,621,1],[622,0,624,0],[520,0,520,1],[521,0,523,0],[524,0,526,0],[528,0,528,13],[545,0,545,1],[546,0,548,0],[549,0,551,0],[553,0,553,13],[570,0,570,1],[453,0,453,13],[470,0,470,1],[471,0,473,0],[474,0,476,0],[478,0,478,13],[495,0,495,1],[496,0,498,0],[499,0,501,0],[503,0,503,13],[427,0,427,13],[444,0,444,1],[445,0,447,0],[448,0,450,0],[234,16,234,22],[231,16,231,26],[395,0,397,0],[398,0,400,0],[402,0,402,13],[419,0,419,1],[327,0,327,13],[344,0,344,1],[345,0,347,0],[348,0,350,0],[420,0,422,0],[423,0,425,0],[352,0,352,13],[369,0,369,1],[370,0,372,0],[373,0,375,0],[377,0,377,13],[394,0,394,1],[273,0,275,0],[277,0,277,13],[294,0,294,1],[295,0,297,0],[298,0,300,0],[302,0,302,13],[319,0,319,1],[320,0,322,0],[323,0,325,0],[0,17,0,30],[17,17,17,18],[18,17,20,17],[21,17,23,17],[227,0,227,13],[244,0,244,1],[194,0,196,0],[197,0,199,0],[201,0,201,13],[218,0,218,1],[69,0,71,0],[72,0,74,0],[51,0,51,13],[50,0,50,14],[76,0,76,13],[122,0,124,0],[126,0,126,13],[143,0,143,1],[144,0,146,0],[0,0,0,13],[42,0,42,1],[43,0,45,0],[46,0,48,0],[17,0,17,1],[18,0,20,0],[21,0,23,0],[25,0,25,12],[68,0,68,1],[1163,0,1163,13],[1180,0,1180,1],[1181,0,1183,0],[1184,0,1186,0],[93,0,93,1],[94,0,96,0],[97,0,99,0],[101,0,101,13],[118,0,118,1],[119,0,121,0],[147,0,149,0],[219,0,221,0],[222,0,224,0],[151,0,151,13],[168,0,168,1],[169,0,171,0],[172,0,174,0],[176,0,176,13],[193,0,193,1],[245,0,247,0],[248,0,250,0],[252,0,252,13],[269,0,269,1],[270,0,272,0],[1231,0,1233,0],[1234,0,1236,0],[1238,0,1238,13],[1255,0,1255,1],[1256,0,1258,0],[1259,0,1261,0],[1188,0,1188,13],[1205,0,1205,1],[1206,0,1208,0],[1209,0,1211,0],[1213,0,1213,13],[1230,0,1230,1],[1330,0,1330,1],[1331,0,1333,0],[1339,0,1339,13],[1343,16,1343,26],[1346,16,1346,22],[1356,0,1356,1],[1263,0,1263,13],[1280,0,1280,1],[1334,0,1336,0],[1281,0,1283,0],[1284,0,1286,0],[1288,0,1288,13],[1305,0,1305,1],[1306,0,1308,0],[1309,0,1311,0],[1313,0,1313,13],[1389,0,1389,13],[1406,0,1406,1],[1407,0,1409,0],[1410,0,1412,0],[1414,0,1414,13],[1431,0,1431,1],[1357,0,1359,0],[1360,0,1362,0],[1364,0,1364,13],[1381,0,1381,1],[1382,0,1384,0],[1385,0,1387,0],[1464,0,1464,13],[1481,0,1481,1],[1482,0,1484,0],[1485,0,1487,0],[1489,0,1489,13],[1506,0,1506,1],[1432,0,1434,0],[1435,0,1437,0],[1439,0,1439,13],[1456,0,1456,1],[1457,0,1459,0],[1460,0,1462,0],[1539,0,1539,13],[1556,0,1556,1],[1557,0,1559,0],[1560,0,1562,0],[1565,0,1565,13],[1582,0,1582,1],[1507,0,1509,0],[1510,0,1512,0],[1514,0,1514,13],[1531,0,1531,1],[1532,0,1534,0],[1535,0,1537,0],[1615,0,1615,13],[1632,0,1632,1],[1633,0,1635,0],[1636,0,1638,0],[1640,0,1640,13],[1657,0,1657,1],[1583,0,1585,0],[1586,0,1588,0],[1590,0,1590,13],[1607,0,1607,1],[1608,0,1610,0],[1611,0,1613,0],[1690,0,1690,13],[1707,0,1707,1],[1708,0,1710,0],[1711,0,1713,0],[1716,0,1716,13],[1733,0,1733,1],[1658,0,1660,0],[1661,0,1663,0],[1665,0,1665,13],[1682,0,1682,1],[1683,0,1685,0],[1686,0,1688,0],[1766,0,1766,13],[1783,0,1783,1],[1784,0,1786,0],[1787,0,1789,0],[1791,0,1791,13],[1808,0,1808,1],[1734,0,1736,0],[1737,0,1739,0],[1741,0,1741,13],[1758,0,1758,1],[1759,0,1761,0],[1762,0,1764,0],[1841,0,1841,13],[1858,0,1858,1],[1859,0,1861,0],[1862,0,1864,0],[1866,0,1866,13],[1883,0,1883,1],[1809,0,1811,0],[1812,0,1814,0],[1816,0,1816,13],[1833,0,1833,1],[1834,0,1836,0],[1837,0,1839,0],[1916,0,1916,13],[1933,0,1933,1],[1934,0,1936,0],[1937,0,1939,0],[1943,0,1943,13],[1960,0,1960,1],[1884,0,1886,0],[1887,0,1889,0],[1891,0,1891,13],[1908,0,1908,1],[1909,0,1911,0],[1912,0,1914,0],[1993,0,1993,13],[2010,0,2010,1],[2011,0,2013,0],[2014,0,2016,0],[2018,0,2018,13],[2035,0,2035,1],[1961,0,1963,0],[1964,0,1966,0],[1968,0,1968,13],[1985,0,1985,1],[1986,0,1988,0],[1989,0,1991,0],[2068,0,2068,13],[2085,0,2085,1],[2086,0,2088,0],[2089,0,2091,0],[2094,0,2094,19],[2116,0,2116,1],[2036,0,2038,0],[2039,0,2041,0],[2043,0,2043,13],[2060,0,2060,1],[2061,0,2063,0],[2064,0,2066,0],[2154,0,2154,19],[2176,0,2176,1],[2177,0,2179,0],[2180,0,2182,0],[2184,0,2184,19],[2267,0,2269,0],[2117,0,2119,0],[2120,0,2122,0],[2124,0,2124,19],[2146,0,2146,1],[2147,0,2149,0],[2150,0,2152,0],[2270,0,2272,0],[2206,0,2206,1],[2207,0,2209,0],[2210,0,2212,0],[2214,0,2214,19],[2236,0,2236,1],[2237,0,2239,0],[2240,0,2242,0],[2244,0,2244,19],[2266,0,2266,1]]}
["Scooper Office 8-17 wo setback intermittent",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EFLH Template"]
[null,131,2.3010000000000002,6326,3.7429999999999999]
[null,1751,5.1130000000000004,13597,9.577]
[null,524,2.101,4469,3.0209999999999999]
[null,1719,5.17,12939,9.3670000000000009]
[null,0,0,11445,10.28]
[null,335,2.891,6964,3.9620000000000002]
[null,2164,6.6920000000000002,15094,9.8360000000000003]
[null,645,2.6269999999999998,5145,3.4169999999999998]
[null,2142,6.7119999999999997,14396,10.077999999999999]
[null,0,0,13449,12.586]
[]
[null,131,1751,524,1719,0,335,2164,645,2142,0]
[null,2.3010000000000002,5.1130000000000004,2.101,5.17,0,2.891,6.6920000000000002,2.6269999999999998,6.7119999999999997,0]
[null,6326,13597,4469,12939,11445,6964,15094,5145,14396,13449]
[null,3.7429999999999999,9.577,3.0209999999999999,9.3670000000000009,10.28,3.9620000000000002,9.8360000000000003,3.4169999999999998,10.077999999999999,12.586]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total",null,null,null,null,null,null,"SYS18","SYS19","SYS20","SYS21","SYS22","SYS23","SYS24","SYS25","SYS26","SYS27","Total"]
["Heating","Ann kWh",131,1751,524,1719,0,335,2164,645,2142,0,9411,null,null,null,null,"Heating","Ann kWh",null,null,null,null,null,null,null,null,null,null,0]
[null,"Ann peak kW",2.3010000000000002,5.1130000000000004,2.101,5.17,0,2.891,6.6920000000000002,2.6269999999999998,6.7119999999999997,0,33.606999999999999,null,null,null,null,null,"Ann peak kW",null,null,null,null,null,null,null,null,null,null,0]
[null,"EFLH Heating",56.931768796175575,342.46039507138664,249.40504521656354,332.49516441005801,"",115.87685921826358,323.37118947997607,245.5272173582033,319.12991656734209,"","57-342",280.03094593388283,null,null,null,null,"EFLH Heating","","","","","","","","","","","0-0",{"$error":"#DIV/0!"}]
["Cooling","Ann kWh",6326,13597,4469,12939,11445,6964,15094,5145,14396,13449,103824,null,null,null,null,"Cooling","Ann kWh",null,null,null,null,null,null,null,null,null,null,0]
[null,"Ann peak kW",3.7429999999999999,9.577,3.0209999999999999,9.3670000000000009,10.28,3.9620000000000002,9.8360000000000003,3.4169999999999998,10.077999999999999,12.586,75.867000000000004,null,null,null,null,null,"Ann peak kW",null,null,null,null,null,null,null,null,null,null,0]
[null,"EFLH Cooling",1690.0881645738714,1419.7556646131357,1479.311486262827,1381.3387423935089,1113.3268482490273,1757.6981322564361,1534.5668971126474,1505.7067603160667,1428.4580273863862,1068.5682504369934,"1069-1758",1368.5001384000948,null,null,null,null,"EFLH Cooling","","","","","","","","","","","0-0",{"$error":"#DIV/0!"}]
[]
["Scooper Office 8-17 wo setback continuous"]
[null,128,2.202,7970,4.0590000000000002]
[null,1665,4.9219999999999997,16223,10.009]
[null,601,2.0950000000000002,5210,3.129]
[null,1741,5.0090000000000003,15472,9.7439999999999998]
[null,156,5.1120000000000001,12902,12.282999999999999]
[null,325,2.7839999999999998,8837,4.3109999999999999]
[null,2104,6.56,17841,10.531000000000001]
[null,676,2.6179999999999999,6031,3.5379999999999998]
[null,2189,6.5960000000000001,17227,10.468999999999999]
[null,402,5.6139999999999999,14981,13.805999999999999]
[]
[null,128,1665,601,1741,156,325,2104,676,2189,402]
[null,2.202,4.9219999999999997,2.0950000000000002,5.0090000000000003,5.1120000000000001,2.7839999999999998,6.56,2.6179999999999999,6.5960000000000001,5.6139999999999999]
[null,7970,16223,5210,15472,12902,8837,17841,6031,17227,14981]
[null,4.0590000000000002,10.009,3.129,9.7439999999999998,12.282999999999999,4.3109999999999999,10.531000000000001,3.5379999999999998,10.468999999999999,13.805999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",128,1665,601,1741,156,325,2104,676,2189,402,9987]
[null,"Ann peak kW",2.202,4.9219999999999997,2.0950000000000002,5.0090000000000003,5.1120000000000001,2.7839999999999998,6.56,2.6179999999999999,6.5960000000000001,5.6139999999999999,43.511999999999993]
[null,"EFLH Heating",58.128973660308809,338.27712312068269,286.87350835322195,347.57436614094627,30.516431924882628,116.73850574712644,320.73170731707319,258.2123758594347,331.86779866585812,71.606697541859631,"31-348",229.522890237176]
["Cooling","Ann kWh",7970,16223,5210,15472,12902,8837,17841,6031,17227,14981,122694]
[null,"Ann peak kW",4.0590000000000002,10.009,3.129,9.7439999999999998,12.282999999999999,4.3109999999999999,10.531000000000001,3.5379999999999998,10.468999999999999,13.805999999999999,81.878999999999991]
[null,"EFLH Cooling",1963.5378171963537,1620.8412428814067,1665.0687120485777,1587.8489326765189,1050.3948546771962,2049.8724193922526,1694.1411072072926,1704.6353872244206,1645.524882987869,1085.1079240909751,"1050-2050",1498.479463598725]
[]
["****Intermittent is default for remaining results"]
["SCooper Office 8-17 w setback - Baseline Design.SIM"]
[null,74,3.5339999999999998,4867,4.1379999999999999]
[null,186,7.7779999999999996,11076,10.724]
[null,169,4.43,3508,3.26]
[null,332,7.798,10153,9.9809999999999999]
[null,166,11.632999999999999,14511,13.787000000000001]
[null,130,4.5289999999999999,5344,4.3890000000000002]
[null,412,10.077999999999999,12598,11.766]
[null,270,5.3710000000000004,4088,3.6859999999999999]
[null,671,10.332000000000001,11242,10.801]
[null,446,17.670999999999999,16140,15.318]
[]
[null,74,186,169,332,166,130,412,270,671,446]
[null,3.5339999999999998,7.7779999999999996,4.43,7.798,11.632999999999999,4.5289999999999999,10.077999999999999,5.3710000000000004,10.332000000000001,17.670999999999999]
[null,4867,11076,3508,10153,14511,5344,12598,4088,11242,16140]
[null,4.1379999999999999,10.724,3.26,9.9809999999999999,13.787000000000001,4.3890000000000002,11.766,3.6859999999999999,10.801,15.318]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",74,186,169,332,166,130,412,270,671,446,2856]
[null,"Ann peak kW",3.5339999999999998,7.7779999999999996,4.43,7.798,11.632999999999999,4.5289999999999999,10.077999999999999,5.3710000000000004,10.332000000000001,17.670999999999999,83.153999999999996]
[null,"EFLH Heating",20.939445387662705,23.913602468500901,38.1489841986456,42.575019235701461,14.269749849565891,28.70390814749393,40.881127207779322,50.269968348538441,64.94386372435153,25.239092298115558,"14-65",34.345912403492314]
["Cooling","Ann kWh",4867,11076,3508,10153,14511,5344,12598,4088,11242,16140,93527]
[null,"Ann peak kW",4.1379999999999999,10.724,3.26,9.9809999999999999,13.787000000000001,4.3890000000000002,11.766,3.6859999999999999,10.801,15.318,87.85]
[null,"EFLH Cooling",1176.1720637989367,1032.8235732935473,1076.0736196319019,1017.2327422101994,1052.5132371074201,1217.5894281157439,1070.7122216556179,1109.0613130765057,1040.8295528191834,1053.6623580101841,"1017-1218",1064.6215139442231]
[]
["SCooper Office 7-19 w setback - Baseline Design.SIM"]
[null,99,3.65,5782,3.859]
[null,274,8.6189999999999998,13261,10.221]
[null,210,5.2690000000000001,4364,3.1360000000000001]
[null,354,8.6039999999999992,12870,10.327]
[null,116,12.613,20773,12.023999999999999]
[null,160,5.016,6420,4.0540000000000003]
[null,438,12.962999999999999,15003,11.217000000000001]
[null,263,6.782,5069,3.4849999999999999]
[null,607,12.518000000000001,14337,11.37]
[null,331,21.603999999999999,22887,14.301]
[]
[null,99,274,210,354,116,160,438,263,607,331]
[null,3.65,8.6189999999999998,5.2690000000000001,8.6039999999999992,12.613,5.016,12.962999999999999,6.782,12.518000000000001,21.603999999999999]
[null,5782,13261,4364,12870,20773,6420,15003,5069,14337,22887]
[null,3.859,10.221,3.1360000000000001,10.327,12.023999999999999,4.0540000000000003,11.217000000000001,3.4849999999999999,11.37,14.301]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",99,274,210,354,116,160,438,263,607,331,2852]
[null,"Ann peak kW",3.65,8.6189999999999998,5.2690000000000001,8.6039999999999992,12.613,5.016,12.962999999999999,6.782,12.518000000000001,21.603999999999999,97.637999999999991]
[null,"EFLH Heating",27.123287671232877,31.790230885253511,39.855760106282027,41.143654114365418,9.196860382145406,31.897926634768741,33.788474890071747,38.7791212031849,48.490174149225112,15.321236807998519,"9-48",29.20993875335423]
["Cooling","Ann kWh",5782,13261,4364,12870,20773,6420,15003,5069,14337,22887,120766]
[null,"Ann peak kW",3.859,10.221,3.1360000000000001,10.327,12.023999999999999,4.0540000000000003,11.217000000000001,3.4849999999999999,11.37,14.301,83.994]
[null,"EFLH Cooling",1498.3156258097954,1297.4268662557479,1391.5816326530612,1246.2477002033504,1727.6280771789754,1583.6211149481992,1337.5234019791387,1454.519368723099,1260.9498680738786,1600.3775959723096,"1246-1728",1437.7931757030265]
[]
["SCooper Office 7-22 w setback - Baseline Design.SIM"]
[null,104,3.7850000000000001,5280,3.9169999999999998]
[null,266,8.9629999999999992,12047,10.243]
[null,202,5.5309999999999997,3915,3.15]
[null,380,8.8930000000000007,11549,10.409000000000001]
[null,138,13.429,17525,12.407]
[null,171,5.0259999999999998,5835,4.1369999999999996]
[null,486,13.128,13662,11.234999999999999]
[null,282,6.9059999999999997,4550,3.5129999999999999]
[null,690,12.36,12765,11.451000000000001]
[null,384,22.835999999999999,19394,14.446]
[]
[null,104,266,202,380,138,171,486,282,690,384]
[null,3.7850000000000001,8.9629999999999992,5.5309999999999997,8.8930000000000007,13.429,5.0259999999999998,13.128,6.9059999999999997,12.36,22.835999999999999]
[null,5280,12047,3915,11549,17525,5835,13662,4550,12765,19394]
[null,3.9169999999999998,10.243,3.15,10.409000000000001,12.407,4.1369999999999996,11.234999999999999,3.5129999999999999,11.451000000000001,14.446]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",104,266,202,380,138,171,486,282,690,384,3103]
[null,"Ann peak kW",3.7850000000000001,8.9629999999999992,5.5309999999999997,8.8930000000000007,13.429,5.0259999999999998,13.128,6.9059999999999997,12.36,22.835999999999999,100.857]
[null,"EFLH Heating",27.47688243064729,29.677563315854069,36.521424697161457,42.730237265264812,10.276267778687915,34.02307998408277,37.020109689213896,40.834057341442225,55.825242718446603,16.815554387808724,"10-56",30.766332530216047]
["Cooling","Ann kWh",5280,12047,3915,11549,17525,5835,13662,4550,12765,19394,106522]
[null,"Ann peak kW",3.9169999999999998,10.243,3.15,10.409000000000001,12.407,4.1369999999999996,11.234999999999999,3.5129999999999999,11.451000000000001,14.446,84.908000000000001]
[null,"EFLH Cooling",1347.9703854991064,1176.1202772625206,1242.8571428571429,1109.5206071668747,1412.5090674619166,1410.4423495286442,1216.0213618157543,1295.1892968972388,1114.7498035106105,1342.5169597120309,"1110-1413",1254.5578744052386]
[]
["SCooper Office 6-21 7days w setback - Baseline Design.SIM"]
[null,318,3.9359999999999999,6630,3.7250000000000001]
[null,1042,8.968,14991,9.8170000000000002]
[null,581,4.5819999999999999,4837,3.052]
[null,1158,9.0410000000000004,14345,10.15]
[null,277,8.9600000000000009,20998,10.781000000000001]
[null,445,4.9870000000000001,7313,3.9769999999999999]
[null,1264,12.515000000000001,16789,10.157999999999999]
[null,666,5.8259999999999996,5550,3.4430000000000001]
[null,1548,12.327,15787,11.026]
[null,1232,20.896999999999998,23459,13.018000000000001]
[]
[null,318,1042,581,1158,277,445,1264,666,1548,1232]
[null,3.9359999999999999,8.968,4.5819999999999999,9.0410000000000004,8.9600000000000009,4.9870000000000001,12.515000000000001,5.8259999999999996,12.327,20.896999999999998]
[null,6630,14991,4837,14345,20998,7313,16789,5550,15787,23459]
[null,3.7250000000000001,9.8170000000000002,3.052,10.15,10.781000000000001,3.9769999999999999,10.157999999999999,3.4430000000000001,11.026,13.018000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",318,1042,581,1158,277,445,1264,666,1548,1232,8531]
[null,"Ann peak kW",3.9359999999999999,8.968,4.5819999999999999,9.0410000000000004,8.9600000000000009,4.9870000000000001,12.515000000000001,5.8259999999999996,12.327,20.896999999999998,92.039000000000016]
[null,"EFLH Heating",80.792682926829272,116.19090098126672,126.80052378873854,128.08317663975222,30.915178571428569,89.232003208341681,100.99880143827407,114.31513903192585,125.57799951326356,58.955830980523523,"31-128",92.688968806701496]
["Cooling","Ann kWh",6630,14991,4837,14345,20998,7313,16789,5550,15787,23459,130699]
[null,"Ann peak kW",3.7250000000000001,9.8170000000000002,3.052,10.15,10.781000000000001,3.9769999999999999,10.157999999999999,3.4430000000000001,11.026,13.018000000000001,79.146999999999991]
[null,"EFLH Cooling",1779.8657718120805,1527.0449220739533,1584.8623853211009,1413.3004926108374,1947.6857434375288,1838.8232335931607,1652.7859814924198,1611.9663084519314,1431.7975693814619,1802.0433246274388,"1413-1948",1651.3449656967416]
[]
["SCooper Office 6-19 7days w setback - Baseline Design.SIM"]
[null,289,4.3479999999999999,6259,3.7610000000000001]
[null,926,9.5730000000000004,14093,9.9130000000000003]
[null,533,5.15,4504,3.0790000000000002]
[null,1071,9.6140000000000008,13364,10.295999999999999]
[null,371,14.337999999999999,18936,11.000999999999999]
[null,443,5.9790000000000001,6862,4.0220000000000002]
[null,1196,13.641999999999999,15752,10.371]
[null,646,6.7329999999999997,5145,3.484]
[null,1517,13.452999999999999,14554,11.185]
[null,1310,23.187999999999999,21268,13.339]
[]
[null,289,926,533,1071,371,443,1196,646,1517,1310]
[null,4.3479999999999999,9.5730000000000004,5.15,9.6140000000000008,14.337999999999999,5.9790000000000001,13.641999999999999,6.7329999999999997,13.452999999999999,23.187999999999999]
[null,6259,14093,4504,13364,18936,6862,15752,5145,14554,21268]
[null,3.7610000000000001,9.9130000000000003,3.0790000000000002,10.295999999999999,11.000999999999999,4.0220000000000002,10.371,3.484,11.185,13.339]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",289,926,533,1071,371,443,1196,646,1517,1310,8302]
[null,"Ann peak kW",4.3479999999999999,9.5730000000000004,5.15,9.6140000000000008,14.337999999999999,5.9790000000000001,13.641999999999999,6.7329999999999997,13.452999999999999,23.187999999999999,106.018]
[null,"EFLH Heating",66.467341306347748,96.730387548312962,103.49514563106796,111.40004160599125,25.875296415120658,74.092657635056028,87.670429555783613,95.945343828902423,112.76295250130083,56.494738657926518,"26-113",78.307457224244942]
["Cooling","Ann kWh",6259,14093,4504,13364,18936,6862,15752,5145,14554,21268,120737]
[null,"Ann peak kW",3.7610000000000001,9.9130000000000003,3.0790000000000002,10.295999999999999,11.000999999999999,4.0220000000000002,10.371,3.484,11.185,13.339,80.450999999999993]
[null,"EFLH Cooling",1664.1850571656473,1421.6685160899829,1462.8126014939915,1297.9797979797981,1721.2980638123809,1706.1163600198904,1518.8506412110692,1476.7508610792192,1301.2069736253911,1594.4223704925407,"1298-1721",1500.7520105405777]
[]
["SCooper Office 5-23 7days w setback - Baseline Design.SIM"]
[null,386,3.286,7115,3.6840000000000002]
[null,1257,8.0079999999999991,16205,9.6910000000000007]
[null,684,4.1980000000000004,5260,3.024]
[null,1351,8.1059999999999999,15574,10.085000000000001]
[null,133,6.1509999999999998,24090,10.558999999999999]
[null,512,4.0179999999999998,7844,3.92]
[null,1490,10.236000000000001,18067,9.89]
[null,740,4.8609999999999998,6036,3.4079999999999999]
[null,1666,10.128,17214,10.936999999999999]
[null,1155,17.373999999999999,26662,12.637]
[]
[null,386,1257,684,1351,133,512,1490,740,1666,1155]
[null,3.286,8.0079999999999991,4.1980000000000004,8.1059999999999999,6.1509999999999998,4.0179999999999998,10.236000000000001,4.8609999999999998,10.128,17.373999999999999]
[null,7115,16205,5260,15574,24090,7844,18067,6036,17214,26662]
[null,3.6840000000000002,9.6910000000000007,3.024,10.085000000000001,10.558999999999999,3.92,9.89,3.4079999999999999,10.936999999999999,12.637]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",386,1257,684,1351,133,512,1490,740,1666,1155,9374]
[null,"Ann peak kW",3.286,8.0079999999999991,4.1980000000000004,8.1059999999999999,6.1509999999999998,4.0179999999999998,10.236000000000001,4.8609999999999998,10.128,17.373999999999999,76.366]
[null,"EFLH Heating",117.46804625684723,156.96803196803199,162.93473082420198,166.66666666666666,21.622500406437979,127.42658038825287,145.56467370066431,152.23205101830899,164.49447077409164,66.478646253021765,"22-167",122.75096247020926]
["Cooling","Ann kWh",7115,16205,5260,15574,24090,7844,18067,6036,17214,26662,144067]
[null,"Ann peak kW",3.6840000000000002,9.6910000000000007,3.024,10.085000000000001,10.558999999999999,3.92,9.89,3.4079999999999999,10.936999999999999,12.637,77.835000000000008]
[null,"EFLH Cooling",1931.3246471226926,1672.1700546899183,1739.4179894179895,1544.2736737729299,2281.4660479212048,2001.0204081632653,1826.7947421638016,1771.1267605633802,1573.923379354485,2109.8361952995174,"1544-2281",1850.9282456478445]
[]
["SCooper Office 24 7days w setback - Baseline Design.SIM"]
[null,576,2.7309999999999999,7741,3.67]
[null,1743,6.5640000000000001,17866,9.5609999999999999]
[null,919,3.6309999999999998,5817,3.0129999999999999]
[null,1816,6.6420000000000003,17260,10.067]
[null,7,1.41,29315,10.643000000000001]
[null,685,3.1819999999999999,8499,3.895]
[null,1999,7.9109999999999996,19764,9.6790000000000003]
[null,934,3.9220000000000002,6650,3.391]
[null,2034,7.8940000000000001,19039,10.891]
[null,1015,15.026999999999999,32071,12.669]
[]
[null,576,1743,919,1816,7,685,1999,934,2034,1015]
[null,2.7309999999999999,6.5640000000000001,3.6309999999999998,6.6420000000000003,1.41,3.1819999999999999,7.9109999999999996,3.9220000000000002,7.8940000000000001,15.026999999999999]
[null,7741,17866,5817,17260,29315,8499,19764,6650,19039,32071]
[null,3.67,9.5609999999999999,3.0129999999999999,10.067,10.643000000000001,3.895,9.6790000000000003,3.391,10.891,12.669]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",576,1743,919,1816,7,685,1999,934,2034,1015,11728]
[null,"Ann peak kW",2.7309999999999999,6.5640000000000001,3.6309999999999998,6.6420000000000003,1.41,3.1819999999999999,7.9109999999999996,3.9220000000000002,7.8940000000000001,15.026999999999999,58.913999999999994]
[null,"EFLH Heating",210.91175393628708,265.53930530164536,253.09832002203251,273.41162300511894,4.9645390070921991,215.27341294783156,252.68613323220833,238.14380418154002,257.66404864454017,67.545085512743725,"5-273",199.06983060053639]
["Cooling","Ann kWh",7741,17866,5817,17260,29315,8499,19764,6650,19039,32071,164022]
[null,"Ann peak kW",3.67,9.5609999999999999,3.0129999999999999,10.067,10.643000000000001,3.895,9.6790000000000003,3.391,10.891,12.669,77.478999999999999]
[null,"EFLH Cooling",2109.264305177112,1868.6329881811525,1930.6339196813808,1714.5127644779973,2754.3925584891476,2182.0282413350451,2041.9464820745943,1961.0734296667649,1748.140666605454,2531.4547320230481,"1715-2754",2116.9865382877942]
[]
[]
["SCooper Rest 9-18 w setback - Baseline Design.SIM"]
[null,131,2.1749999999999998,7611,6.1449999999999996]
[null,260,1.984,7044,6.1509999999999998]
[null,537,2.5489999999999999,6100,6.1989999999999998]
[null,386,2.5209999999999999,6754,7.056,null,null,null,null,null,null,null,null,null,null,null,"Restaurant Defaults do not estimate require ventilation, refrigeration, or cooking loads correctly!"]
[null,29,1.5349999999999999,3852,3.4249999999999998]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"From DOE Com Bldg Stocks Models.pdf"]
[]
[]
[]
[]
[null,131,260,537,386,29]
[null,2.1749999999999998,1.984,2.5489999999999999,2.5209999999999999,1.5349999999999999]
[null,7611,7044,6100,6754,3852]
[null,6.1449999999999996,6.1509999999999998,6.1989999999999998,7.056,3.4249999999999998]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",131,260,537,386,29,null,null,null,null,null,1343]
[null,"Ann peak kW",2.1749999999999998,1.984,2.5489999999999999,2.5209999999999999,1.5349999999999999,null,null,null,null,null,10.763999999999999]
[null,"EFLH Heating",60.229885057471272,131.04838709677421,210.67085131424088,153.11384371281238,18.892508143322477,"","","","","","19-211",124.76774433296173]
["Cooling","Ann kWh",7611,7044,6100,6754,3852,null,null,null,null,null,31361]
[null,"Ann peak kW",6.1449999999999996,6.1509999999999998,6.1989999999999998,7.056,3.4249999999999998,null,null,null,null,null,28.975999999999999]
[null,"EFLH Cooling",1238.5679414157853,1145.1796455860836,984.02968220680759,957.19954648526073,1124.6715328467153,"","","","","","957-1239",1082.3094975151851]
[]
["SCooper Rest 8-20 w setback - Baseline Design.SIM"]
[null,182,2.746,8504,5.9980000000000002]
[null,285,2.7989999999999999,7951,6.2729999999999997]
[null,552,2.968,7038,5.782]
[null,410,2.95,7642,6.9790000000000001]
[null,30,1.7310000000000001,4587,3.2469999999999999]
[]
[]
[]
[]
[]
[]
[null,182,285,552,410,30]
[null,2.746,2.7989999999999999,2.968,2.95,1.7310000000000001]
[null,8504,7951,7038,7642,4587]
[null,5.9980000000000002,6.2729999999999997,5.782,6.9790000000000001,3.2469999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",182,285,552,410,30,null,null,null,null,null,1459]
[null,"Ann peak kW",2.746,2.7989999999999999,2.968,2.95,1.7310000000000001,null,null,null,null,null,13.194000000000001]
[null,"EFLH Heating",66.27822286962855,101.82207931404074,185.98382749326146,138.9830508474576,17.331022530329289,"","","","","","17-186",110.58056692435954]
["Cooling","Ann kWh",8504,7951,7038,7642,4587,null,null,null,null,null,35722]
[null,"Ann peak kW",5.9980000000000002,6.2729999999999997,5.782,6.9790000000000001,3.2469999999999999,null,null,null,null,null,28.279]
[null,"EFLH Cooling",1417.8059353117706,1267.495616132632,1217.2258734002075,1094.9992835649807,1412.6886356636896,"","","","","","1095-1418",1263.1988401287174]
[]
["SCooper Rest 7-22 w setback - Baseline Design.SIM"]
[null,233,3.0030000000000001,9341,6.1159999999999997]
[null,333,3.274,8776,6.2469999999999999]
[null,562,4.0609999999999999,7826,5.6950000000000003]
[null,402,3.278,8469,6.4470000000000001]
[null,28,1.9019999999999999,5187,3.1720000000000002]
[]
[]
[]
[]
[]
[]
[null,233,333,562,402,28]
[null,3.0030000000000001,3.274,4.0609999999999999,3.278,1.9019999999999999]
[null,9341,8776,7826,8469,5187]
[null,6.1159999999999997,6.2469999999999999,5.6950000000000003,6.4470000000000001,3.1720000000000002]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",233,333,562,402,28,null,null,null,null,null,1558]
[null,"Ann peak kW",3.0030000000000001,3.274,4.0609999999999999,3.278,1.9019999999999999,null,null,null,null,null,15.518000000000001]
[null,"EFLH Heating",77.58907758907759,101.71044593769089,138.38955922186653,122.63575350823673,14.721345951629864,"","","","","","15-138",100.39953602268334]
["Cooling","Ann kWh",9341,8776,7826,8469,5187,null,null,null,null,null,39599]
[null,"Ann peak kW",6.1159999999999997,6.2469999999999999,5.6950000000000003,6.4470000000000001,3.1720000000000002,null,null,null,null,null,27.677]
[null,"EFLH Cooling",1527.3054283845652,1404.8343204738276,1374.1878841088674,1313.6342484876686,1635.2459016393441,"","","","","","1314-1635",1430.7547783358023]
[]
["SCooper Rest 9-22 7days w setback - Baseline Design.SIM"]
[null,72,2.4860000000000002,11522,6.101]
[null,94,1.92,10715,6.1829999999999998]
[null,297,6.5549999999999997,9774,5.7140000000000004]
[null,239,4.8369999999999997,10513,6.4450000000000003]
[null,1,0.76,6667,3.0459999999999998]
[]
[]
[]
[]
[]
[]
[null,72,94,297,239,1]
[null,2.4860000000000002,1.92,6.5549999999999997,4.8369999999999997,0.76]
[null,11522,10715,9774,10513,6667]
[null,6.101,6.1829999999999998,5.7140000000000004,6.4450000000000003,3.0459999999999998]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",72,94,297,239,1,null,null,null,null,null,703]
[null,"Ann peak kW",2.4860000000000002,1.92,6.5549999999999997,4.8369999999999997,0.76,null,null,null,null,null,16.558]
[null,"EFLH Heating",28.962188254223651,48.958333333333336,45.308924485125857,49.410791813107302,1.3157894736842106,"","","","","","1-49",42.456818456335306]
["Cooling","Ann kWh",11522,10715,9774,10513,6667,null,null,null,null,null,49191]
[null,"Ann peak kW",6.101,6.1829999999999998,5.7140000000000004,6.4450000000000003,3.0459999999999998,null,null,null,null,null,27.488999999999997]
[null,"EFLH Cooling",1888.5428618259302,1732.9775190037199,1710.5355267763387,1631.1869666408068,2188.7721602101119,"","","","","","1631-2189",1789.4794281348904]
[]
["SCooper Rest 8-22 7days w setback - Baseline Design.SIM"]
[null,161,3.5139999999999998,11938,6.093]
[null,161,3.2989999999999999,11159,6.3289999999999997]
[null,360,7.6390000000000002,10218,5.7160000000000002]
[null,296,6.4249999999999998,10927,6.4619999999999997]
[null,0,0,6947,3.0009999999999999]
[]
[]
[]
[]
[]
[]
[null,161,161,360,296,0]
[null,3.5139999999999998,3.2989999999999999,7.6390000000000002,6.4249999999999998,0]
[null,11938,11159,10218,10927,6947]
[null,6.093,6.3289999999999997,5.7160000000000002,6.4619999999999997,3.0009999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",161,161,360,296,0,null,null,null,null,null,978]
[null,"Ann peak kW",3.5139999999999998,3.2989999999999999,7.6390000000000002,6.4249999999999998,0,null,null,null,null,null,20.876999999999999]
[null,"EFLH Heating",45.816733067729089,48.802667474992425,47.126587249640004,46.070038910505836,"","","","","","","46-49",46.84581117976721]
["Cooling","Ann kWh",11938,11159,10218,10927,6947,null,null,null,null,null,51189]
[null,"Ann peak kW",6.093,6.3289999999999997,5.7160000000000002,6.4619999999999997,3.0009999999999999,null,null,null,null,null,27.601000000000003]
[null,"EFLH Cooling",1959.2975545708189,1763.153736767262,1787.6137158852343,1690.9625502940266,2314.8950349883371,"","","","","","1691-2315",1854.6067171479292]
[]
["SCooper Rest 5-23 7days w setback - Baseline Design.SIM"]
[null,294,6.3929999999999998,13333,6.0810000000000004]
[null,349,6.8620000000000001,12552,6.3460000000000001]
[null,481,8.359,11591,5.6539999999999999]
[null,376,7.609,12330,6.2130000000000001]
[null,0,0,7872,2.8]
[]
[]
[]
[]
[]
[]
[null,294,349,481,376,0]
[null,6.3929999999999998,6.8620000000000001,8.359,7.609,0]
[null,13333,12552,11591,12330,7872]
[null,6.0810000000000004,6.3460000000000001,5.6539999999999999,6.2130000000000001,2.8]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",294,349,481,376,0,null,null,null,null,null,1500]
[null,"Ann peak kW",6.3929999999999998,6.8620000000000001,8.359,7.609,0,null,null,null,null,null,29.222999999999999]
[null,"EFLH Heating",45.987799155326137,50.859807636257649,57.542768273716952,49.415166250492838,"","","","","","","46-58",51.329432296478799]
["Cooling","Ann kWh",13333,12552,11591,12330,7872,null,null,null,null,null,57678]
[null,"Ann peak kW",6.0810000000000004,6.3460000000000001,5.6539999999999999,6.2130000000000001,2.8,null,null,null,null,null,27.094000000000001]
[null,"EFLH Cooling",2192.5670120046043,1977.9388591238576,2050.0530597806865,1984.5485272815065,2811.4285714285716,"","","","","","1978-2811",2128.8108068206984]
[]
["SCooper Rest 24 7days w setback - Baseline Design.SIM"]
[null,22,2.2370000000000001,19114,6.6289999999999996]
[null,26,2.1269999999999998,18300,7.0289999999999999]
[null,73,5.15,17113,6.0860000000000003]
[null,25,2.4489999999999998,18066,6.968]
[null,0,0,10275,3.0369999999999999]
[]
[]
[]
[]
[]
[]
[null,22,26,73,25,0]
[null,2.2370000000000001,2.1269999999999998,5.15,2.4489999999999998,0]
[null,19114,18300,17113,18066,10275]
[null,6.6289999999999996,7.0289999999999999,6.0860000000000003,6.968,3.0369999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",22,26,73,25,0,null,null,null,null,null,146]
[null,"Ann peak kW",2.2370000000000001,2.1269999999999998,5.15,2.4489999999999998,0,null,null,null,null,null,11.962999999999999]
[null,"EFLH Heating",9.8345999105945463,12.223789374706159,14.174757281553397,10.208248264597795,"","","","","","","10-14",12.204296581125137]
["Cooling","Ann kWh",19114,18300,17113,18066,10275,null,null,null,null,null,82868]
[null,"Ann peak kW",6.6289999999999996,7.0289999999999999,6.0860000000000003,6.968,3.0369999999999999,null,null,null,null,null,29.748999999999999]
[null,"EFLH Cooling",2883.391160054307,2603.4997865983783,2811.8632928031548,2592.7095292766935,3383.2729667434969,"","","","","","2593-3383",2785.5726242898922]
[]
["SCooper Rest 10-23 7day Hol1 w setback - Baseline Design.SIM"]
[null,265,2.633,9702,6.3449999999999998]
[null,695,2.62,9415,5.9539999999999997]
[null,1002,2.649,8827,5.7590000000000003]
[null,703,2.6560000000000001,9285,6.3029999999999999]
[null,2,1.157,5661,3.089]
[]
[]
[]
[]
[]
[]
[null,265,695,1002,703,2]
[null,2.633,2.62,2.649,2.6560000000000001,1.157]
[null,9702,9415,8827,9285,5661]
[null,6.3449999999999998,5.9539999999999997,5.7590000000000003,6.3029999999999999,3.089]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",265,695,1002,703,2,null,null,null,null,null,2667]
[null,"Ann peak kW",2.633,2.62,2.649,2.6560000000000001,1.157,null,null,null,null,null,11.715]
[null,"EFLH Heating",100.64565134827193,265.26717557251908,378.25594563986408,264.68373493975901,1.7286084701815039,"","","","","","2-378",227.65685019206146]
["Cooling","Ann kWh",9702,9415,8827,9285,5661,null,null,null,null,null,42890]
[null,"Ann peak kW",6.3449999999999998,5.9539999999999997,5.7590000000000003,6.3029999999999999,3.089,null,null,null,null,null,27.45]
[null,"EFLH Cooling",1529.0780141843973,1581.2898891501513,1532.7313769751693,1473.1080437886721,1832.6319197151181,"","","","","","1473-1833",1562.4772313296903]
[]
["SCooper Rest 8-23 12-20 Hol2 w setback - Baseline Design.SIM"]
[null,191,2.3210000000000002,6311,5.1909999999999998]
[null,151,3.2210000000000001,5598,4.5430000000000001]
[null,335,5.3319999999999999,4878,3.8359999999999999]
[null,257,2.855,5456,4.6280000000000001]
[null,137,1.373,2085,2.1749999999999998]
[]
[]
[]
[]
[]
[]
[null,191,151,335,257,137]
[null,2.3210000000000002,3.2210000000000001,5.3319999999999999,2.855,1.373]
[null,6311,5598,4878,5456,2085]
[null,5.1909999999999998,4.5430000000000001,3.8359999999999999,4.6280000000000001,2.1749999999999998]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",191,151,335,257,137,null,null,null,null,null,1071]
[null,"Ann peak kW",2.3210000000000002,3.2210000000000001,5.3319999999999999,2.855,1.373,null,null,null,null,null,15.101999999999999]
[null,"EFLH Heating",82.292115467470907,46.879850977957155,62.828207051762945,90.017513134851143,99.781500364166064,"","","","","","47-100",70.917759237187141]
["Cooling","Ann kWh",6311,5598,4878,5456,2085,null,null,null,null,null,24328]
[null,"Ann peak kW",5.1909999999999998,4.5430000000000001,3.8359999999999999,4.6280000000000001,2.1749999999999998,null,null,null,null,null,20.373000000000001]
[null,"EFLH Cooling",1215.7580427663263,1232.2254017169271,1271.6371220020856,1178.9109766637857,958.62068965517244,"","","","","","959-1272",1194.1294851028322]
[]
[]
["SCooper Htl 9-18 w setback - Baseline Design.SIM"]
[null,355,5.2220000000000004,5280,4.03]
[null,1100,6.2469999999999999,3184,3.323]
[null,1270,6.2210000000000001,3212,3.5259999999999998]
[null,968,5.9219999999999997,4634,4.548]
[null,184,2.6019999999999999,734,0.95899999999999996]
[null,594,5.7469999999999999,8020,4.875]
[null,1099,6.3090000000000002,4672,4.2080000000000002]
[null,1186,6.3250000000000002,4897,4.5880000000000001]
[null,1164,6.4660000000000002,6970,5.9809999999999999]
[null,246,3.4849999999999999,713,1.0669999999999999]
[]
[null,355,1100,1270,968,184,594,1099,1186,1164,246]
[null,5.2220000000000004,6.2469999999999999,6.2210000000000001,5.9219999999999997,2.6019999999999999,5.7469999999999999,6.3090000000000002,6.3250000000000002,6.4660000000000002,3.4849999999999999]
[null,5280,3184,3212,4634,734,8020,4672,4897,6970,713]
[null,4.03,3.323,3.5259999999999998,4.548,0.95899999999999996,4.875,4.2080000000000002,4.5880000000000001,5.9809999999999999,1.0669999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",355,1100,1270,968,184,594,1099,1186,1164,246,8166]
[null,"Ann peak kW",5.2220000000000004,6.2469999999999999,6.2210000000000001,5.9219999999999997,2.6019999999999999,5.7469999999999999,6.3090000000000002,6.3250000000000002,6.4660000000000002,3.4849999999999999,54.546000000000006]
[null,"EFLH Heating",67.981616238988892,176.08452056987355,204.14724320848737,163.4582911178656,70.714834742505772,103.3582738820254,174.1955935964495,187.50988142292491,180.01855861429013,70.588235294117652,"68-204",149.70850291497084]
["Cooling","Ann kWh",5280,3184,3212,4634,734,8020,4672,4897,6970,713,42316]
[null,"Ann peak kW",4.03,3.323,3.5259999999999998,4.548,0.95899999999999996,4.875,4.2080000000000002,4.5880000000000001,5.9809999999999999,1.0669999999999999,37.105000000000004]
[null,"EFLH Cooling",1310.1736972704714,958.1703280168523,910.9472490073739,1018.9094107299912,765.38060479666319,1645.1282051282051,1110.2661596958174,1067.3496076721883,1165.3569637184416,668.22867853795697,"668-1645",1140.4392938957012]
[]
["SCooper Htl 8-21 w setback - Baseline Design.SIM"]
[null,683,5.218,5889,3.94]
[null,1456,6.1230000000000002,3612,3.0920000000000001]
[null,1632,6.1520000000000001,3645,3.2480000000000002]
[null,1329,6.0590000000000002,5212,4.46]
[null,249,2.5579999999999998,861,0.85799999999999998]
[null,844,6.3710000000000004,8983,4.8630000000000004]
[null,1422,6.7549999999999999,5285,3.9550000000000001]
[null,1507,6.9139999999999997,5532,4.3179999999999996]
[null,1405,6.9619999999999997,7721,5.9649999999999999]
[null,324,3.4329999999999998,856,0.97599999999999998]
[]
[null,683,1456,1632,1329,249,844,1422,1507,1405,324]
[null,5.218,6.1230000000000002,6.1520000000000001,6.0590000000000002,2.5579999999999998,6.3710000000000004,6.7549999999999999,6.9139999999999997,6.9619999999999997,3.4329999999999998]
[null,5889,3612,3645,5212,861,8983,5285,5532,7721,856]
[null,3.94,3.0920000000000001,3.2480000000000002,4.46,0.85799999999999998,4.8630000000000004,3.9550000000000001,4.3179999999999996,5.9649999999999999,0.97599999999999998]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",683,1456,1632,1329,249,844,1422,1507,1405,324,10851]
[null,"Ann peak kW",5.218,6.1230000000000002,6.1520000000000001,6.0590000000000002,2.5579999999999998,6.3710000000000004,6.7549999999999999,6.9139999999999997,6.9619999999999997,3.4329999999999998,56.545000000000009]
[null,"EFLH Heating",130.89306247604446,237.79193205944799,265.27958387516253,219.34312592837102,97.341673182173579,132.47527860618428,210.51073279052554,217.96355221290136,201.80982476299914,94.378094960675796,"94-265",191.9002564329295]
["Cooling","Ann kWh",5889,3612,3645,5212,861,8983,5285,5532,7721,856,47596]
[null,"Ann peak kW",3.94,3.0920000000000001,3.2480000000000002,4.46,0.85799999999999998,4.8630000000000004,3.9550000000000001,4.3179999999999996,5.9649999999999999,0.97599999999999998,35.674999999999997]
[null,"EFLH Cooling",1494.6700507614214,1168.1759379042689,1122.2290640394087,1168.6098654708521,1003.4965034965035,1847.2136541229693,1336.283185840708,1281.1486799444187,1294.3839061190276,877.04918032786884,"877-1847",1334.1555711282413]
[]
["SCooper Htl 9-22 7days w setback - Baseline Design.SIM"]
[null,802,5.4130000000000003,7077,3.843]
[null,1583,6.14,4459,3.0249999999999999]
[null,1756,6.109,4502,3.206]
[null,1481,7.02,6281,4.4189999999999996]
[null,292,1.8149999999999999,1081,0.748]
[null,727,5.61,10506,4.8650000000000002]
[null,1413,6.1740000000000004,6297,3.948]
[null,1487,6.1920000000000002,6601,4.3360000000000003]
[null,1449,7.6230000000000002,9022,5.9050000000000002]
[null,420,3.0609999999999999,1145,0.81899999999999995]
[]
[null,802,1583,1756,1481,292,727,1413,1487,1449,420]
[null,5.4130000000000003,6.14,6.109,7.02,1.8149999999999999,5.61,6.1740000000000004,6.1920000000000002,7.6230000000000002,3.0609999999999999]
[null,7077,4459,4502,6281,1081,10506,6297,6601,9022,1145]
[null,3.843,3.0249999999999999,3.206,4.4189999999999996,0.748,4.8650000000000002,3.948,4.3360000000000003,5.9050000000000002,0.81899999999999995]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",802,1583,1756,1481,292,727,1413,1487,1449,420,11410]
[null,"Ann peak kW",5.4130000000000003,6.14,6.109,7.02,1.8149999999999999,5.61,6.1740000000000004,6.1920000000000002,7.6230000000000002,3.0609999999999999,55.156999999999996]
[null,"EFLH Heating",148.16183262516165,257.81758957654722,287.44475364216731,210.96866096866097,160.88154269972452,129.59001782531195,228.86297376093293,240.1485788113695,190.08264462809916,137.21006207121854,"130-287",206.8640426419131]
["Cooling","Ann kWh",7077,4459,4502,6281,1081,10506,6297,6601,9022,1145,56971]
[null,"Ann peak kW",3.843,3.0249999999999999,3.206,4.4189999999999996,0.748,4.8650000000000002,3.948,4.3360000000000003,5.9050000000000002,0.81899999999999995,35.114000000000004]
[null,"EFLH Cooling",1841.5300546448088,1474.0495867768595,1404.2420461634435,1421.3622991627067,1445.1871657754011,2159.5066803699897,1594.9848024316109,1522.3708487084871,1527.8577476714647,1398.0463980463981,"1398-2160",1622.4582787492166]
[]
["SCooper Htl 8-22 7days w setback - Baseline Design.SIM"]
[null,1018,6.0389999999999997,7262,3.8279999999999998]
[null,1785,6.3730000000000002,4606,2.96]
[null,1969,6.9870000000000001,4656,3.1480000000000001]
[null,1707,7.5659999999999998,6439,4.4009999999999998]
[null,326,1.7569999999999999,1103,0.63700000000000001]
[null,1034,7.5860000000000003,10765,4.8639999999999999]
[null,1650,7.6879999999999997,6510,3.8149999999999999]
[null,1721,7.7859999999999996,6823,4.1379999999999999]
[null,1689,8.2989999999999995,9244,5.8959999999999999]
[null,483,2.99,1165,0.74099999999999999]
[]
[null,1018,1785,1969,1707,326,1034,1650,1721,1689,483]
[null,6.0389999999999997,6.3730000000000002,6.9870000000000001,7.5659999999999998,1.7569999999999999,7.5860000000000003,7.6879999999999997,7.7859999999999996,8.2989999999999995,2.99]
[null,7262,4606,4656,6439,1103,10765,6510,6823,9244,1165]
[null,3.8279999999999998,2.96,3.1480000000000001,4.4009999999999998,0.63700000000000001,4.8639999999999999,3.8149999999999999,4.1379999999999999,5.8959999999999999,0.74099999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",1018,1785,1969,1707,326,1034,1650,1721,1689,483,13382]
[null,"Ann peak kW",6.0389999999999997,6.3730000000000002,6.9870000000000001,7.5659999999999998,1.7569999999999999,7.5860000000000003,7.6879999999999997,7.7859999999999996,8.2989999999999995,2.99,63.071000000000005]
[null,"EFLH Heating",168.57095545620138,280.08787070453474,281.80907399456134,225.61459159397305,185.54354012521344,136.30371737411019,214.62018730489075,221.03776008219884,203.51849620436198,161.53846153846152,"136-282",212.17358215344609]
["Cooling","Ann kWh",7262,4606,4656,6439,1103,10765,6510,6823,9244,1165,58573]
[null,"Ann peak kW",3.8279999999999998,2.96,3.1480000000000001,4.4009999999999998,0.63700000000000001,4.8639999999999999,3.8149999999999999,4.1379999999999999,5.8959999999999999,0.74099999999999999,34.428000000000004]
[null,"EFLH Cooling",1897.0741901776385,1556.081081081081,1479.0343074968234,1463.0765735060215,1731.5541601255886,2213.1990131578946,1706.4220183486239,1648.8641855969067,1567.842605156038,1572.199730094467,"1463-2213",1701.3186940862088]
[]
["SCooper Htl 5-23 7days w setback - Baseline Design.SIM"]
[null,1926,7.6929999999999996,7843,3.7869999999999999]
[null,2742,8.1750000000000007,5008,2.883]
[null,2933,8.1430000000000007,5069,3.0590000000000002]
[null,2647,8.0139999999999993,7015,4.3550000000000004]
[null,384,1.5509999999999999,1234,0.54700000000000004]
[null,1976,8.6110000000000007,11670,4.9089999999999998]
[null,2632,9.1709999999999994,7064,3.7330000000000001]
[null,2694,9.1029999999999998,7428,4.04]
[null,2558,8.8309999999999995,10057,5.88]
[null,609,2.4449999999999998,1282,0.65500000000000003]
[]
[null,1926,2742,2933,2647,384,1976,2632,2694,2558,609]
[null,7.6929999999999996,8.1750000000000007,8.1430000000000007,8.0139999999999993,1.5509999999999999,8.6110000000000007,9.1709999999999994,9.1029999999999998,8.8309999999999995,2.4449999999999998]
[null,7843,5008,5069,7015,1234,11670,7064,7428,10057,1282]
[null,3.7869999999999999,2.883,3.0590000000000002,4.3550000000000004,0.54700000000000004,4.9089999999999998,3.7330000000000001,4.04,5.88,0.65500000000000003]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",1926,2742,2933,2647,384,1976,2632,2694,2558,609,21101]
[null,"Ann peak kW",7.6929999999999996,8.1750000000000007,8.1430000000000007,8.0139999999999993,1.5509999999999999,8.6110000000000007,9.1709999999999994,9.1029999999999998,8.8309999999999995,2.4449999999999998,71.737000000000009]
[null,"EFLH Heating",250.3574678278955,335.41284403669721,360.1866633918703,330.29698028450213,247.58220502901355,229.47392869585411,286.99160396903284,295.94639129957159,289.66141999773527,249.07975460122702,"229-360",294.14388669724127]
["Cooling","Ann kWh",7843,5008,5069,7015,1234,11670,7064,7428,10057,1282,63670]
[null,"Ann peak kW",3.7869999999999999,2.883,3.0590000000000002,4.3550000000000004,0.54700000000000004,4.9089999999999998,3.7330000000000001,4.04,5.88,0.65500000000000003,33.847999999999999]
[null,"EFLH Cooling",2071.0324795352522,1737.0794311481095,1657.0774762994442,1610.792192881745,2255.9414990859232,2377.2662456712164,1892.3118135547816,1838.6138613861385,1710.3741496598641,1957.2519083969464,"1611-2377",1881.0564878279367]
[]
["SCooper Htl 24 7days w setback - Baseline Design.SIM"]
[null,2699,6.6130000000000004,8507,3.7610000000000001]
[null,3665,7.093,5386,2.9470000000000001]
[null,3844,7.056,5473,3.012]
[null,3476,6.9119999999999999,7613,4.3259999999999996]
[null,493,1.3129999999999999,1340,0.53]
[null,2564,6.7670000000000003,12744,4.9279999999999999]
[null,3468,7.3209999999999997,7570,3.7109999999999999]
[null,3498,7.2469999999999999,7993,4.0780000000000003]
[null,3182,6.9649999999999999,10966,5.8719999999999999]
[null,766,1.8129999999999999,1392,0.64900000000000002]
[]
[null,2699,3665,3844,3476,493,2564,3468,3498,3182,766]
[null,6.6130000000000004,7.093,7.056,6.9119999999999999,1.3129999999999999,6.7670000000000003,7.3209999999999997,7.2469999999999999,6.9649999999999999,1.8129999999999999]
[null,8507,5386,5473,7613,1340,12744,7570,7993,10966,1392]
[null,3.7610000000000001,2.9470000000000001,3.012,4.3259999999999996,0.53,4.9279999999999999,3.7109999999999999,4.0780000000000003,5.8719999999999999,0.64900000000000002]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",2699,3665,3844,3476,493,2564,3468,3498,3182,766,27655]
[null,"Ann peak kW",6.6130000000000004,7.093,7.056,6.9119999999999999,1.3129999999999999,6.7670000000000003,7.3209999999999997,7.2469999999999999,6.9649999999999999,1.8129999999999999,59.099999999999994]
[null,"EFLH Heating",408.13549070013607,516.70661215282678,544.78458049886626,502.89351851851853,375.47600913937549,378.89759125166245,473.70577789919412,482.68248930591972,456.85570710696339,422.50413678985109,"375-545",467.93570219966165]
["Cooling","Ann kWh",8507,5386,5473,7613,1340,12744,7570,7993,10966,1392,68984]
[null,"Ann peak kW",3.7610000000000001,2.9470000000000001,3.012,4.3259999999999996,0.53,4.9279999999999999,3.7109999999999999,4.0780000000000003,5.8719999999999999,0.64900000000000002,33.813999999999993]
[null,"EFLH Cooling",2261.8984312682796,1827.621309806583,1817.0650730411687,1759.8243180767454,2528.3018867924525,2586.0389610389611,2039.8814335758557,1960.0294261893084,1867.5068119891009,2144.8382126348229,"1760-2586",2040.1017330099962]
[]
[]
["SCooper Rtl 9-18 w setback - Baseline Design.SIM"]
[null,538,13.055999999999999,14544,14.584]
[null,241,4.907,6096,5.8120000000000003]
[null,520,12.186,9946,10.263]
[null,373,10.472,10987,10.856999999999999]
[null,364,6.8440000000000003,5222,5.0380000000000003]
[null,781,14.692,16894,15.904999999999999]
[null,397,9.3190000000000008,2218,3.073]
[]
[]
[]
[]
[null,538,241,520,373,364,781,397]
[null,13.055999999999999,4.907,12.186,10.472,6.8440000000000003,14.692,9.3190000000000008]
[null,14544,6096,9946,10987,5222,16894,2218]
[null,14.584,5.8120000000000003,10.263,10.856999999999999,5.0380000000000003,15.904999999999999,3.073]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",538,241,520,373,364,781,397,null,null,null,3214]
[null,"Ann peak kW",13.055999999999999,4.907,12.186,10.472,6.8440000000000003,14.692,9.3190000000000008,null,null,null,71.475999999999999]
[null,"EFLH Heating",41.207107843137258,49.113511310372935,42.67191859510914,35.618792971734152,53.185271770894211,53.158181323169075,42.601137461100976,"","","","36-53",44.966142481392353]
["Cooling","Ann kWh",14544,6096,9946,10987,5222,16894,2218,null,null,null,65907]
[null,"Ann peak kW",14.584,5.8120000000000003,10.263,10.856999999999999,5.0380000000000003,15.904999999999999,3.073,null,null,null,65.531999999999996]
[null,"EFLH Cooling",997.25726823916625,1048.8644184445973,969.11234531813307,1011.9738417610758,1036.5224295355299,1062.1817038667086,721.7702570777742,"","","","722-1062",1005.7223951657206]
[]
["SCooper Rtl 8-20 w setback - Baseline Design.SIM"]
[null,464,10.923999999999999,17345,14.54]
[null,249,5.03,7099,5.6189999999999998]
[null,440,9.0340000000000007,11911,9.92]
[null,290,8.6440000000000001,13090,10.316000000000001]
[null,346,5.53,6114,5.0209999999999999]
[null,705,11.446,20148,16.899999999999999]
[null,360,8.5879999999999992,2623,2.5390000000000001]
[]
[]
[]
[]
[null,464,249,440,290,346,705,360]
[null,10.923999999999999,5.03,9.0340000000000007,8.6440000000000001,5.53,11.446,8.5879999999999992]
[null,17345,7099,11911,13090,6114,20148,2623]
[null,14.54,5.6189999999999998,9.92,10.316000000000001,5.0209999999999999,16.899999999999999,2.5390000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",464,249,440,290,346,705,360,null,null,null,2854]
[null,"Ann peak kW",10.923999999999999,5.03,9.0340000000000007,8.6440000000000001,5.53,11.446,8.5879999999999992,null,null,null,59.195999999999998]
[null,"EFLH Heating",42.475283778835596,49.502982107355862,48.704892627850342,33.549282739472467,62.56781193490054,61.593569806045778,41.918956683744767,"","","","34-63",48.212717075478075]
["Cooling","Ann kWh",17345,7099,11911,13090,6114,20148,2623,null,null,null,78330]
[null,"Ann peak kW",14.54,5.6189999999999998,9.92,10.316000000000001,5.0209999999999999,16.899999999999999,2.5390000000000001,null,null,null,64.855000000000004]
[null,"EFLH Cooling",1192.9160935350758,1263.3920626445988,1200.7056451612902,1268.9026754556028,1217.6857199761005,1192.189349112426,1033.0838912957856,"","","","1033-1269",1207.7711818672421]
[]
["SCooper Rtl 7-22 w setback - Baseline Design.SIM"]
[null,473,12.275,20225,14.228]
[null,290,6.7380000000000004,8056,5.5940000000000003]
[null,379,11.101000000000001,13949,9.7810000000000006]
[null,297,10.682,15199,10.175000000000001]
[null,344,7.2430000000000003,6987,4.8959999999999999]
[null,637,13.071,23262,17.079000000000001]
[null,316,9.4939999999999998,3058,2.508]
[]
[]
[]
[]
[null,473,290,379,297,344,637,316]
[null,12.275,6.7380000000000004,11.101000000000001,10.682,7.2430000000000003,13.071,9.4939999999999998]
[null,20225,8056,13949,15199,6987,23262,3058]
[null,14.228,5.5940000000000003,9.7810000000000006,10.175000000000001,4.8959999999999999,17.079000000000001,2.508]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",473,290,379,297,344,637,316,null,null,null,2736]
[null,"Ann peak kW",12.275,6.7380000000000004,11.101000000000001,10.682,7.2430000000000003,13.071,9.4939999999999998,null,null,null,70.604000000000013]
[null,"EFLH Heating",38.533604887983707,43.03947758978925,34.141068372218719,27.803782063284029,47.494132265635784,48.733838267921357,33.284179481777969,"","","","28-49",38.751345532830996]
["Cooling","Ann kWh",20225,8056,13949,15199,6987,23262,3058,null,null,null,90736]
[null,"Ann peak kW",14.228,5.5940000000000003,9.7810000000000006,10.175000000000001,4.8959999999999999,17.079000000000001,2.508,null,null,null,64.26100000000001]
[null,"EFLH Cooling",1421.4928310373912,1440.1144082946014,1426.1322973111132,1493.7592137592137,1427.0833333333333,1362.0235376778498,1219.2982456140351,"","","","1219-1494",1411.9917212617293]
[]
["SCooper Rtl 9-22 7days w setback - Baseline Design.SIM"]
[null,495,14.634,21288,13.891]
[null,258,6.4480000000000004,8322,5.3840000000000003]
[null,447,12.393000000000001,14630,9.657]
[null,318,12.013999999999999,15821,9.6229999999999993]
[null,368,7.0720000000000001,7316,4.8970000000000002]
[null,748,14.83,24256,17.027000000000001]
[null,379,9.2140000000000004,3307,3.0720000000000001]
[]
[]
[]
[]
[null,495,258,447,318,368,748,379]
[null,14.634,6.4480000000000004,12.393000000000001,12.013999999999999,7.0720000000000001,14.83,9.2140000000000004]
[null,21288,8322,14630,15821,7316,24256,3307]
[null,13.891,5.3840000000000003,9.657,9.6229999999999993,4.8970000000000002,17.027000000000001,3.0720000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",495,258,447,318,368,748,379,null,null,null,3013]
[null,"Ann peak kW",14.634,6.4480000000000004,12.393000000000001,12.013999999999999,7.0720000000000001,14.83,9.2140000000000004,null,null,null,76.605000000000004]
[null,"EFLH Heating",33.825338253382533,40.012406947890817,36.068748487049142,26.469119360745797,52.036199095022624,50.438300741739717,41.133058389407424,"","","","26-52",39.331636316167348]
["Cooling","Ann kWh",21288,8322,14630,15821,7316,24256,3307,null,null,null,94940]
[null,"Ann peak kW",13.891,5.3840000000000003,9.657,9.6229999999999993,4.8970000000000002,17.027000000000001,3.0720000000000001,null,null,null,63.551000000000002]
[null,"EFLH Cooling",1532.5030595349506,1545.6909361069836,1514.9632391011701,1644.081887145381,1493.9759036144578,1424.5609913666528,1076.4973958333333,"","","","1076-1644",1493.9182703655331]
[]
["SCooper Rtl 8-22 7days w setback - Baseline Design.SIM"]
[null,391,16.696999999999999,23942,14.032999999999999]
[null,212,6.3940000000000001,9248,5.6740000000000004]
[null,341,12.472,16524,9.6549999999999994]
[null,222,10.866,17838,10.137]
[null,309,6.6719999999999997,8128,4.819]
[null,567,18.352,26984,16.911999999999999]
[null,316,9.516,3709,3.1379999999999999]
[]
[]
[]
[]
[null,391,212,341,222,309,567,316]
[null,16.696999999999999,6.3940000000000001,12.472,10.866,6.6719999999999997,18.352,9.516]
[null,23942,9248,16524,17838,8128,26984,3709]
[null,14.032999999999999,5.6740000000000004,9.6549999999999994,10.137,4.819,16.911999999999999,3.1379999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",391,212,341,222,309,567,316,null,null,null,2358]
[null,"Ann peak kW",16.696999999999999,6.3940000000000001,12.472,10.866,6.6719999999999997,18.352,9.516,null,null,null,80.969000000000008]
[null,"EFLH Heating",23.417380367730733,33.156083828589303,27.341244387427839,20.430701270016566,46.312949640287769,30.895815170008717,33.207229928541402,"","","","20-46",29.122256666131481]
["Cooling","Ann kWh",23942,9248,16524,17838,8128,26984,3709,null,null,null,106373]
[null,"Ann peak kW",14.032999999999999,5.6740000000000004,9.6549999999999994,10.137,4.819,16.911999999999999,3.1379999999999999,null,null,null,64.368000000000009]
[null,"EFLH Cooling",1706.1212855412243,1629.89072964399,1711.444847229415,1759.6922166321397,1686.6569827765097,1595.5534531693472,1181.9630337794774,"","","","1182-1760",1652.5758140691025]
[]
["SCooper Rtl 5-23 7days w setback - Baseline Design.SIM"]
[null,413,9.9429999999999996,28511,14.887]
[null,341,3.5419999999999998,10750,5.4560000000000004]
[null,258,5.2350000000000003,19719,10.361000000000001]
[null,239,5.2539999999999996,21167,10.327999999999999]
[null,355,4.2080000000000002,9479,4.8680000000000003]
[null,529,8.7859999999999996,31868,16.942]
[null,199,6.258,4369,3.2090000000000001]
[]
[]
[]
[]
[null,413,341,258,239,355,529,199]
[null,9.9429999999999996,3.5419999999999998,5.2350000000000003,5.2539999999999996,4.2080000000000002,8.7859999999999996,6.258]
[null,28511,10750,19719,21167,9479,31868,4369]
[null,14.887,5.4560000000000004,10.361000000000001,10.327999999999999,4.8680000000000003,16.942,3.2090000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",413,341,258,239,355,529,199,null,null,null,2334]
[null,"Ann peak kW",9.9429999999999996,3.5419999999999998,5.2350000000000003,5.2539999999999996,4.2080000000000002,8.7859999999999996,6.258,null,null,null,43.225999999999999]
[null,"EFLH Heating",41.536759529317109,96.273291925465841,49.283667621776502,45.489151122953942,84.363117870722434,60.209424083769633,31.799296899968041,"","","","32-96",53.995280618146488]
["Cooling","Ann kWh",28511,10750,19719,21167,9479,31868,4369,null,null,null,125863]
[null,"Ann peak kW",14.887,5.4560000000000004,10.361000000000001,10.327999999999999,4.8680000000000003,16.942,3.2090000000000001,null,null,null,66.051000000000002]
[null,"EFLH Cooling",1915.1608786189292,1970.307917888563,1903.1946723289257,2049.4771494965144,1947.2062448644206,1881.0057844410342,1361.4833281396072,"","","","1361-2049",1905.5426867117833]
[]
["SCooper Rtl 24 7days w setback - Baseline Design.SIM"]
[null,56,7.4450000000000003,40898,14.154]
[null,147,3.044,14719,5.7839999999999998]
[null,5,1.605,28374,9.7230000000000008]
[null,4,1.1839999999999999,30254,10.612]
[null,149,4.6360000000000001,13126,4.8339999999999996]
[null,68,5.53,44760,17.18]
[null,3,0.39200000000000002,5612,1.915]
[]
[]
[]
[]
[null,56,147,5,4,149,68,3]
[null,7.4450000000000003,3.044,1.605,1.1839999999999999,4.6360000000000001,5.53,0.39200000000000002]
[null,40898,14719,28374,30254,13126,44760,5612]
[null,14.154,5.7839999999999998,9.7230000000000008,10.612,4.8339999999999996,17.18,1.915]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",56,147,5,4,149,68,3,null,null,null,432]
[null,"Ann peak kW",7.4450000000000003,3.044,1.605,1.1839999999999999,4.6360000000000001,5.53,0.39200000000000002,null,null,null,23.836000000000002]
[null,"EFLH Heating",7.5218267293485557,48.291721419185279,3.1152647975077881,3.3783783783783785,32.139775668679896,12.296564195298371,7.6530612244897958,"","","","3-48",18.123846282933375]
["Cooling","Ann kWh",40898,14719,28374,30254,13126,44760,5612,null,null,null,177743]
[null,"Ann peak kW",14.154,5.7839999999999998,9.7230000000000008,10.612,4.8339999999999996,17.18,1.915,null,null,null,64.201999999999998]
[null,"EFLH Cooling",2889.5012010739015,2544.7786998616875,2918.2351126195617,2850.9234828496042,2715.3496069507655,2605.3550640279395,2930.5483028720628,"","","","2545-2931",2768.4963085262143]
[]
["SCooper Rtl 10-23 7day Hol1 w setback - Baseline Design.SIM"]
[null,550,6.0860000000000003,20939,14.055]
[null,368,2.4820000000000002,8207,5.3710000000000004]
[null,416,4.2210000000000001,14892,9.9640000000000004]
[null,281,3.79,15820,10.055]
[null,421,2.5939999999999999,7491,4.7759999999999998]
[null,921,6.9089999999999998,24135,16.783000000000001]
[null,53,5.8390000000000004,3402,2.9550000000000001]
[]
[]
[]
[]
[null,550,368,416,281,421,921,53]
[null,6.0860000000000003,2.4820000000000002,4.2210000000000001,3.79,2.5939999999999999,6.9089999999999998,5.8390000000000004]
[null,20939,8207,14892,15820,7491,24135,3402]
[null,14.055,5.3710000000000004,9.9640000000000004,10.055,4.7759999999999998,16.783000000000001,2.9550000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",550,368,416,281,421,921,53,null,null,null,3010]
[null,"Ann peak kW",6.0860000000000003,2.4820000000000002,4.2210000000000001,3.79,2.5939999999999999,6.9089999999999998,5.8390000000000004,null,null,null,31.920999999999999]
[null,"EFLH Heating",90.371344068353594,148.26752618855761,98.55484482350154,74.142480211081789,162.2976098689283,133.30438558402085,9.0768967288919331,"","","","9-162",94.29529150089283]
["Cooling","Ann kWh",20939,8207,14892,15820,7491,24135,3402,null,null,null,94886]
[null,"Ann peak kW",14.055,5.3710000000000004,9.9640000000000004,10.055,4.7759999999999998,16.783000000000001,2.9550000000000001,null,null,null,63.959000000000003]
[null,"EFLH Cooling",1489.7901102810388,1528.0208527276111,1494.5804897631472,1573.3465937344606,1568.4673366834172,1438.0623249716975,1151.2690355329948,"","","","1151-1573",1483.5441454681904]
[]
["SCooper Rtl 9-24 10-18 Hol2 w setback - Baseline Design.SIM"]
[null,587,22.747,21863,13.738]
[null,247,7.52,8574,5.4359999999999999]
[null,622,20.158999999999999,15010,9.5]
[null,467,17.434999999999999,16206,9.7840000000000007]
[null,391,10.728,7579,4.8559999999999999]
[null,925,26.109000000000002,24907,16.914999999999999]
[null,508,11.65,3352,2.9359999999999999]
[]
[]
[]
[]
[null,587,247,622,467,391,925,508]
[null,22.747,7.52,20.158999999999999,17.434999999999999,10.728,26.109000000000002,11.65]
[null,21863,8574,15010,16206,7579,24907,3352]
[null,13.738,5.4359999999999999,9.5,9.7840000000000007,4.8559999999999999,16.914999999999999,2.9359999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",587,247,622,467,391,925,508,null,null,null,3747]
[null,"Ann peak kW",22.747,7.52,20.158999999999999,17.434999999999999,10.728,26.109000000000002,11.65,null,null,null,116.34800000000001]
[null,"EFLH Heating",25.80560073855893,32.845744680851062,30.854705094498737,26.785202179523949,36.446681580909768,35.428396338427362,43.605150214592271,"","","","26-44",32.205108811496544]
["Cooling","Ann kWh",21863,8574,15010,16206,7579,24907,3352,null,null,null,97491]
[null,"Ann peak kW",13.738,5.4359999999999999,9.5,9.7840000000000007,4.8559999999999999,16.914999999999999,2.9359999999999999,null,null,null,63.164999999999999]
[null,"EFLH Cooling",1591.4252438491776,1577.2626931567329,1580,1656.3777596075224,1560.7495881383854,1472.4800472953002,1141.6893732970027,"","","","1142-1656",1543.4338636903349]
[]
[]
[]
["SCooper Sch 7-16 w setback - Baseline Design.SIM"]
[null,284,40.296999999999997,39267,39.896999999999998]
[null,249,21.283000000000001,15968,16.148]
[null,290,32.472000000000001,23662,24.460999999999999]
[null,262,31.268000000000001,24363,24.465]
[null,280,22.271999999999998,15474,16.135000000000002]
[null,492,50.73,39422,40.159999999999997]
[null,432,336.01100000000002,112411,122.387]
[]
[]
[]
[]
[null,284,249,290,262,280,492,432]
[null,40.296999999999997,21.283000000000001,32.472000000000001,31.268000000000001,22.271999999999998,50.73,336.01100000000002]
[null,39267,15968,23662,24363,15474,39422,112411]
[null,39.896999999999998,16.148,24.460999999999999,24.465,16.135000000000002,40.159999999999997,122.387]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",284,249,290,262,280,492,432,null,null,null,2289]
[null,"Ann peak kW",40.296999999999997,21.283000000000001,32.472000000000001,31.268000000000001,22.271999999999998,50.73,336.01100000000002,null,null,null,534.33299999999997]
[null,"EFLH Heating",7.0476710425093687,11.699478456984448,8.9307711258930773,8.3791735960086982,12.571839080459771,9.698403311649912,1.2856721952555124,"","","","1-13",4.2838454671525064]
["Cooling","Ann kWh",39267,15968,23662,24363,15474,39422,112411,null,null,null,270567]
[null,"Ann peak kW",39.896999999999998,16.148,24.460999999999999,24.465,16.135000000000002,40.159999999999997,122.387,null,null,null,283.65300000000002]
[null,"EFLH Cooling",984.20933904804872,988.85310874411698,967.33575896324771,995.8307786633967,959.03315773163922,981.62350597609566,918.4880747138177,"","","","918-996",953.86616746517745]
[]
["SCooper Sch 6-20 w setback - Baseline Design.SIM"]
[null,257,37.670999999999999,51898,39.636000000000003]
[null,227,20.407,20893,16.015000000000001]
[null,257,31.245999999999999,31263,24.367999999999999]
[null,242,29.45,31966,24.268999999999998]
[null,250,21.402000000000001,20395,16.015999999999998]
[null,430,45.616999999999997,52172,41.926000000000002]
[null,213,135.37700000000001,153900,122.56]
[]
[]
[]
[]
[null,257,227,257,242,250,430,213]
[null,37.670999999999999,20.407,31.245999999999999,29.45,21.402000000000001,45.616999999999997,135.37700000000001]
[null,51898,20893,31263,31966,20395,52172,153900]
[null,39.636000000000003,16.015000000000001,24.367999999999999,24.268999999999998,16.015999999999998,41.926000000000002,122.56]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",257,227,257,242,250,430,213,null,null,null,1876]
[null,"Ann peak kW",37.670999999999999,20.407,31.245999999999999,29.45,21.402000000000001,45.616999999999997,135.37700000000001,null,null,null,321.16999999999996]
[null,"EFLH Heating",6.822223991930132,11.123634047140687,8.2250528067592654,8.2173174872665538,11.681151294271563,9.4263103667492381,1.5733839573930577,"","","","2-12",5.8411433197372116]
["Cooling","Ann kWh",51898,20893,31263,31966,20395,52172,153900,null,null,null,362487]
[null,"Ann peak kW",39.636000000000003,16.015000000000001,24.367999999999999,24.268999999999998,16.015999999999998,41.926000000000002,122.56,null,null,null,284.79000000000002]
[null,"EFLH Cooling",1309.3652235341608,1304.5894473930689,1282.9530531845044,1317.1535703984507,1273.4140859140859,1244.3829604541334,1255.7114882506528,"","","","1244-1317",1272.8220794269462]
[]
["SCooper Sch 7-21 7days w setback - Baseline Design.SIM"]
[null,2150,138.78800000000001,55074,39.704999999999998]
[null,1413,55.405000000000001,22171,16.082000000000001]
[null,2028,80.305999999999997,33065,24.329000000000001]
[null,1810,81.611999999999995,33824,24.36]
[null,1544,54.033999999999999,21642,16.04]
[null,3356,146.637,55205,39.932000000000002]
[null,2911,358.00200000000001,160996,120.758]
[]
[]
[]
[]
[null,2150,1413,2028,1810,1544,3356,2911]
[null,138.78800000000001,55.405000000000001,80.305999999999997,81.611999999999995,54.033999999999999,146.637,358.00200000000001]
[null,55074,22171,33065,33824,21642,55205,160996]
[null,39.704999999999998,16.082000000000001,24.329000000000001,24.36,16.04,39.932000000000002,120.758]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",2150,1413,2028,1810,1544,3356,2911,null,null,null,15212]
[null,"Ann peak kW",138.78800000000001,55.405000000000001,80.305999999999997,81.611999999999995,54.033999999999999,146.637,358.00200000000001,null,null,null,914.78399999999988]
[null,"EFLH Heating",15.491252846067383,25.503113437415394,25.253405723109108,22.178111062098711,28.57460117703668,22.886447485968752,8.1312394902821765,"","","","8-29",16.629062161122192]
["Cooling","Ann kWh",55074,22171,33065,33824,21642,55205,160996,null,null,null,381977]
[null,"Ann peak kW",39.704999999999998,16.082000000000001,24.329000000000001,24.36,16.04,39.932000000000002,120.758,null,null,null,281.20599999999996]
[null,"EFLH Cooling",1387.0797128825086,1378.6220619325954,1359.0776439639935,1388.5057471264367,1349.2518703241897,1382.4752078533506,1333.2118783020587,"","","","1333-1389",1358.3529512172572]
[]
["SCooper Sch 8-22 7days 12mths w setback - Baseline Design.SIM"]
[null,2016,137.779,75436,42.99]
[null,1354,55.908999999999999,30272,17.166]
[null,1943,80.569999999999993,45659,26.625]
[null,1744,82.12,46392,26.143000000000001]
[null,1519,54.375,29794,17.658000000000001]
[null,3298,147.05600000000001,75406,44.994]
[null,2788,32.875,230243,132.851]
[]
[]
[]
[]
[null,2016,1354,1943,1744,1519,3298,2788]
[null,137.779,55.908999999999999,80.569999999999993,82.12,54.375,147.05600000000001,32.875]
[null,75436,30272,45659,46392,29794,75406,230243]
[null,42.99,17.166,26.625,26.143000000000001,17.658000000000001,44.994,132.851]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",2016,1354,1943,1744,1519,3298,2788,null,null,null,14662]
[null,"Ann peak kW",137.779,55.908999999999999,80.569999999999993,82.12,54.375,147.05600000000001,32.875,null,null,null,590.68399999999997]
[null,"EFLH Heating",14.632128263378309,24.217925557602534,24.115675809854785,21.237213833414515,27.935632183908044,22.426830595147425,84.806083650190118,"","","","15-85",24.822070684155996]
["Cooling","Ann kWh",75436,30272,45659,46392,29794,75406,230243,null,null,null,533202]
[null,"Ann peak kW",42.99,17.166,26.625,26.143000000000001,17.658000000000001,44.994,132.851,null,null,null,308.42700000000002]
[null,"EFLH Cooling",1754.7336589904628,1763.4859606198299,1714.8920187793428,1774.5476800673221,1687.2805527239777,1675.9123438680713,1733.0919601659002,"","","","1676-1775",1728.7786088766547]
[]
["SCooper Sch 5-23 7days 12 mths w setback - Baseline Design.SIM"]
[null,3094,137.46600000000001,87424,42.649000000000001]
[null,1845,56.027000000000001,34998,17.007999999999999]
[null,2734,80.265000000000001,52951,26.611000000000001]
[null,2421,82.462000000000003,53659,25.91]
[null,1964,53.948999999999998,34534,17.57]
[null,4287,52.698,87490,44.600999999999999]
[null,4259,49.420999999999999,267867,134.221]
[]
[]
[]
[]
[null,3094,1845,2734,2421,1964,4287,4259]
[null,137.46600000000001,56.027000000000001,80.265000000000001,82.462000000000003,53.948999999999998,52.698,49.420999999999999]
[null,87424,34998,52951,53659,34534,87490,267867]
[null,42.649000000000001,17.007999999999999,26.611000000000001,25.91,17.57,44.600999999999999,134.221]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",3094,1845,2734,2421,1964,4287,4259,null,null,null,20604]
[null,"Ann peak kW",137.46600000000001,56.027000000000001,80.265000000000001,82.462000000000003,53.948999999999998,52.698,49.420999999999999,null,null,null,512.28800000000001]
[null,"EFLH Heating",22.507383643955595,32.930551341317582,34.062169064972281,29.358977468409691,36.404752636749521,81.350335876124333,86.177940551587383,"","","","23-86",40.21956399525267]
["Cooling","Ann kWh",87424,34998,52951,53659,34534,87490,267867,null,null,null,618923]
[null,"Ann peak kW",42.649000000000001,17.007999999999999,26.611000000000001,25.91,17.57,44.600999999999999,134.221,null,null,null,308.57]
[null,"EFLH Cooling",2049.8487655044664,2057.7375352775166,1989.8162414039307,2070.9764569664221,1965.509391007399,1961.6152104212911,1995.7160205929026,"","","","1962-2071",2005.7782674919792]
[]
["SCooper Sch 24h 7days 12 mths w setback - Baseline Design.SIM"]
[null,3521,50.03,104376,43.619]
[null,1983,20.346,41701,17.405000000000001]
[null,2843,30.513000000000002,63229,27.105]
[null,2648,30.414999999999999,63979,26.533000000000001]
[null,2118,20.43,41203,17.888999999999999]
[null,4830,49.786000000000001,104546,45.459000000000003]
[null,5448,31.914999999999999,325270,138.07]
[]
[]
[]
[]
[null,3521,1983,2843,2648,2118,4830,5448]
[null,50.03,20.346,30.513000000000002,30.414999999999999,20.43,49.786000000000001,31.914999999999999]
[null,104376,41701,63229,63979,41203,104546,325270]
[null,43.619,17.405000000000001,27.105,26.533000000000001,17.888999999999999,45.459000000000003,138.07]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",3521,1983,2843,2648,2118,4830,5448,null,null,null,23391]
[null,"Ann peak kW",50.03,20.346,30.513000000000002,30.414999999999999,20.43,49.786000000000001,31.914999999999999,null,null,null,233.435]
[null,"EFLH Heating",70.377773335998398,97.463874963137712,93.173401500999574,87.062304783823777,103.67107195301028,97.015225163700634,170.70343098856338,"","","","70-171",100.20348276822241]
["Cooling","Ann kWh",104376,41701,63229,63979,41203,104546,325270,null,null,null,744304]
[null,"Ann peak kW",43.619,17.405000000000001,27.105,26.533000000000001,17.888999999999999,45.459000000000003,138.07,null,null,null,316.08000000000004]
[null,"EFLH Cooling",2392.902175657397,2395.9207124389541,2332.7430363401586,2411.2991369238307,2303.2589859690315,2299.7866209111507,2355.8339972477729,"","","","2300-2411",2354.7962541128827]
[]
[]
["SCooper Tech Col 7-16 w setback - Baseline Design.SIM"]
[null,31,7.27,61058,52.493000000000002]
[null,26,7.8280000000000003,22154,18.727]
[null,54,21.878,60840,53.051000000000002]
[null,28,10.624000000000001,21446,17.814]
[null,12,11.909000000000001,94449,74.346000000000004]
[null,111,25.21,133678,110.014]
[null,71,18.835999999999999,48537,39.347999999999999]
[null,154,53.311,133054,112.672]
[null,65,19.422000000000001,46774,37.823999999999998]
[null,68,36.332000000000001,212062,161.36600000000001]
[null,234,45.58,66505,55.942999999999998]
[null,119,22.559000000000001,24432,19.945]
[null,308,65.278000000000006,66698,57.42]
[null,120,23.283999999999999,23586,19.227]
[null,419,96.379000000000005,103539,82.588999999999999]
[]
[null,31,26,54,28,12,111,71,154,65,68,234,119,308,120,419]
[null,7.27,7.8280000000000003,21.878,10.624000000000001,11.909000000000001,25.21,18.835999999999999,53.311,19.422000000000001,36.332000000000001,45.58,22.559000000000001,65.278000000000006,23.283999999999999,96.379000000000005]
[null,61058,22154,60840,21446,94449,133678,48537,133054,46774,212062,66505,24432,66698,23586,103539]
[null,52.493000000000002,18.727,53.051000000000002,17.814,74.346000000000004,110.014,39.347999999999999,112.672,37.823999999999998,161.36600000000001,55.942999999999998,19.945,57.42,19.227,82.588999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann kWh",31,26,54,28,12,111,71,154,65,68,234,119,308,120,419,1820]
[null,"Ann peak kW",7.27,7.8280000000000003,21.878,10.624000000000001,11.909000000000001,25.21,18.835999999999999,53.311,19.422000000000001,36.332000000000001,45.58,22.559000000000001,65.278000000000006,23.283999999999999,96.379000000000005,465.70000000000005]
[null,"EFLH Heating",4.2640990371389274,3.321410321921308,2.4682329280555808,2.6355421686746987,1.0076412797044252,4.4030146767155891,3.7693777872159697,2.8887096471647502,3.3467202141900936,1.8716283166354728,5.1338306274681882,5.2750565184626979,4.7182818101044761,5.1537536505755028,4.347420081138007,"1-5",3.9080953403478631]
["Cooling","Ann kWh",61058,22154,60840,21446,94449,133678,48537,133054,46774,212062,66505,24432,66698,23586,103539,1118812]
[null,"Ann peak kW",52.493000000000002,18.727,53.051000000000002,17.814,74.346000000000004,110.014,39.347999999999999,112.672,37.823999999999998,161.36600000000001,55.942999999999998,19.945,57.42,19.227,82.588999999999999,912.779]
[null,"EFLH Cooling",1163.1646124245137,1182.9978106477279,1146.8209835818363,1203.8845851577412,1270.3978694213542,1215.0998963768247,1233.5315645013725,1180.8967622834423,1236.622250423012,1314.1677924717721,1188.799313587044,1224.9686638255203,1161.5813305468478,1226.7124356373849,1253.665742411217,"1147-1314",1225.7205742025178]
[]
["SCooper Tech Col 6-20 w setback - Baseline Design.SIM"]
[null,37,8.0429999999999993,83743,51.756]
[null,29,7.0449999999999999,29345,18.187999999999999]
[null,59,18.010999999999999,83292,53.89]
[null,28,6.9710000000000001,29073,18.934999999999999]
[null,19,12.507,126885,71.245999999999995]
[null,119,25.81,181990,105.59399999999999]
[null,94,17.481000000000002,63990,37.814]
[null,191,47.591999999999999,181240,111.855]
[null,84,15.914,63133,38.74]
[null,127,36.832000000000001,278719,153.66900000000001]
[null,237,37.832000000000001,90767,54.948999999999998]
[null,129,18.568999999999999,32144,19.599]
[null,305,52.86,90671,57.79]
[null,120,17.617999999999999,31687,20.14]
[null,445,79.361000000000004,138573,81.480999999999995]
[]
[null,37,29,59,28,19,119,94,191,84,127,237,129,305,120,445]
[null,8.0429999999999993,7.0449999999999999,18.010999999999999,6.9710000000000001,12.507,25.81,17.481000000000002,47.591999999999999,15.914,36.832000000000001,37.832000000000001,18.568999999999999,52.86,17.617999999999999,79.361000000000004]
[null,83743,29345,83292,29073,126885,181990,63990,181240,63133,278719,90767,32144,90671,31687,138573]
[null,51.756,18.187999999999999,53.89,18.934999999999999,71.245999999999995,105.59399999999999,37.814,111.855,38.74,153.66900000000001,54.948999999999998,19.599,57.79,20.14,81.480999999999995]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann kWh",37,29,59,28,19,119,94,191,84,127,237,129,305,120,445,2023]
[null,"Ann peak kW",8.0429999999999993,7.0449999999999999,18.010999999999999,6.9710000000000001,12.507,25.81,17.481000000000002,47.591999999999999,15.914,36.832000000000001,37.832000000000001,18.568999999999999,52.86,17.617999999999999,79.361000000000004,402.44599999999991]
[null,"EFLH Heating",4.6002735297774464,4.1163946061036194,3.2757759147187833,4.0166403672356905,1.519149276405213,4.6106160402944596,5.3772667467536177,4.0132795427802996,5.2783712454442631,3.4480886185925281,6.2645379572848379,6.9470623081479888,5.7699583806280739,6.8112158020206612,5.6072882146142309,"2-7",5.026761354318344]
["Cooling","Ann kWh",83743,29345,83292,29073,126885,181990,63990,181240,63133,278719,90767,32144,90671,31687,138573,1505252]
[null,"Ann peak kW",51.756,18.187999999999999,53.89,18.934999999999999,71.245999999999995,105.59399999999999,37.814,111.855,38.74,153.66900000000001,54.948999999999998,19.599,57.79,20.14,81.480999999999995,895.64599999999996]
[null,"EFLH Cooling",1618.0346240049462,1613.4264350120959,1545.5928743737243,1535.410615262741,1780.9420879768691,1723.4880769740705,1692.2303908605279,1620.3120110857806,1629.659266907589,1813.7620469971171,1651.8407978307157,1640.0836777386601,1568.9738709119224,1573.3366434955312,1700.6786858285982,"1535-1814",1680.6327499927427]
[]
["SCooper Tech Col 9-21 7days w setback - Baseline Design.SIM"]
[null,472,9.7840000000000007,80567,50.261000000000003]
[null,522,4.7430000000000003,28290,17.908000000000001]
[null,1326,23.443000000000001,80150,53.466999999999999]
[null,513,12.196,28010,19.065999999999999]
[null,285,13.547000000000001,115955,66.674999999999997]
[null,1040,25.488,174978,104.065]
[null,927,10.427,61986,37.274999999999999]
[null,2881,37.292000000000002,174196,112.307]
[null,1061,20.536999999999999,60799,39.369999999999997]
[null,1068,32.814999999999998,253250,143.077]
[null,1378,45.655999999999999,88008,54.497]
[null,894,18.353000000000002,31202,19.460999999999999]
[null,2928,60.225999999999999,87783,58.338000000000001]
[null,1037,22.129000000000001,30599,20.492999999999999]
[null,3588,65.691999999999993,128132,77.153000000000006]
[]
[null,472,522,1326,513,285,1040,927,2881,1061,1068,1378,894,2928,1037,3588]
[null,9.7840000000000007,4.7430000000000003,23.443000000000001,12.196,13.547000000000001,25.488,10.427,37.292000000000002,20.536999999999999,32.814999999999998,45.655999999999999,18.353000000000002,60.225999999999999,22.129000000000001,65.691999999999993]
[null,80567,28290,80150,28010,115955,174978,61986,174196,60799,253250,88008,31202,87783,30599,128132]
[null,50.261000000000003,17.908000000000001,53.466999999999999,19.065999999999999,66.674999999999997,104.065,37.274999999999999,112.307,39.369999999999997,143.077,54.497,19.460999999999999,58.338000000000001,20.492999999999999,77.153000000000006]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann kWh",472,522,1326,513,285,1040,927,2881,1061,1068,1378,894,2928,1037,3588,19920]
[null,"Ann peak kW",9.7840000000000007,4.7430000000000003,23.443000000000001,12.196,13.547000000000001,25.488,10.427,37.292000000000002,20.536999999999999,32.814999999999998,45.655999999999999,18.353000000000002,60.225999999999999,22.129000000000001,65.691999999999993,402.32800000000003]
[null,"EFLH Heating",48.242027800490597,110.05692599620492,56.562726613488032,42.062971466054442,21.037868162692845,40.803515379786568,88.903807423036355,77.255175372734101,51.662852412718507,32.546091726344663,30.182232346241459,48.711382335313026,48.616876432105734,46.861584346332862,54.618522803385503,"21-110",49.511841084885958]
["Cooling","Ann kWh",80567,28290,80150,28010,115955,174978,61986,174196,60799,253250,88008,31202,87783,30599,128132,1423905]
[null,"Ann peak kW",50.261000000000003,17.908000000000001,53.466999999999999,19.065999999999999,66.674999999999997,104.065,37.274999999999999,112.307,39.369999999999997,143.077,54.497,19.460999999999999,58.338000000000001,20.492999999999999,77.153000000000006,873.41300000000001]
[null,"EFLH Cooling",1602.972483635423,1579.7408979227159,1499.0554921727421,1469.1073114444562,1739.1076115485564,1681.4298755585451,1662.9376257545273,1551.0698353619987,1544.2976885953774,1770.0259300935859,1614.9145824540801,1603.3091824674991,1504.7310500874216,1493.1440003903774,1660.7520122354281,"1469-1770",1630.2768564241658]
[]
["SCooper Tech Col 8-22 7days w setback - Baseline Design.SIM"]
[null,851,30.283000000000001,89354,50.206000000000003]
[null,711,17.891999999999999,31368,17.591000000000001]
[null,1815,54.534999999999997,88961,53.485999999999997]
[null,721,19.312999999999999,31011,18.986000000000001]
[null,306,13.132,128005,65.911000000000001]
[null,1762,42.082999999999998,192904,103.35899999999999]
[null,1328,26.231000000000002,68204,36.869999999999997]
[null,3848,55.210999999999999,192244,111.309]
[null,1438,26.555,67014,39.015999999999998]
[null,1047,33.003999999999998,277954,136.79499999999999]
[null,1995,63.734999999999999,97157,54.136000000000003]
[null,1175,24.01,34374,19.257999999999999]
[null,3673,66.573999999999998,96961,58.12]
[null,1328,24.186,33766,20.311]
[null,4239,84.126999999999995,140899,75.41]
[]
[null,851,711,1815,721,306,1762,1328,3848,1438,1047,1995,1175,3673,1328,4239]
[null,30.283000000000001,17.891999999999999,54.534999999999997,19.312999999999999,13.132,42.082999999999998,26.231000000000002,55.210999999999999,26.555,33.003999999999998,63.734999999999999,24.01,66.573999999999998,24.186,84.126999999999995]
[null,89354,31368,88961,31011,128005,192904,68204,192244,67014,277954,97157,34374,96961,33766,140899]
[null,50.206000000000003,17.591000000000001,53.485999999999997,18.986000000000001,65.911000000000001,103.35899999999999,36.869999999999997,111.309,39.015999999999998,136.79499999999999,54.136000000000003,19.257999999999999,58.12,20.311,75.41]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann kWh",851,711,1815,721,306,1762,1328,3848,1438,1047,1995,1175,3673,1328,4239,26237]
[null,"Ann peak kW",30.283000000000001,17.891999999999999,54.534999999999997,19.312999999999999,13.132,42.082999999999998,26.231000000000002,55.210999999999999,26.555,33.003999999999998,63.734999999999999,24.01,66.573999999999998,24.186,84.126999999999995,580.87099999999998]
[null,"EFLH Heating",28.101575141168311,39.738430583501007,33.281378930961772,37.332366799565065,23.301858056655497,41.869638571394624,50.627120582516866,69.696256180833529,54.151760497081533,31.723427463337778,31.301482701812191,48.937942523948351,55.171688647219639,54.907797899611346,50.388103700357796,"23-70",45.16837645535756]
["Cooling","Ann kWh",89354,31368,88961,31011,128005,192904,68204,192244,67014,277954,97157,34374,96961,33766,140899,1570176]
[null,"Ann peak kW",50.206000000000003,17.591000000000001,53.485999999999997,18.986000000000001,65.911000000000001,103.35899999999999,36.869999999999997,111.309,39.015999999999998,136.79499999999999,54.136000000000003,19.257999999999999,58.12,20.311,75.41,860.76400000000001]
[null,"EFLH Cooling",1779.7474405449548,1783.1845830254106,1663.2576749055829,1633.3614242073106,1942.0885739861328,1866.3493261351214,1849.8508272308111,1727.1199992812801,1717.6030346524503,2031.9017507949854,1794.6837594207182,1784.9205524976635,1668.2897453544392,1662.4489193048103,1868.4391990452195,"1633-2032",1824.1655087805716]
[]
["SCooper Tech Col 5-23 7days w setback - Baseline Design.SIM"]
[null,1640,31.408999999999999,105403,49.569000000000003]
[null,1151,14.689,36836,17.238]
[null,2878,56.677,104929,53.128999999999998]
[null,1157,15.378,36491,18.718]
[null,235,11.903,149849,63.756999999999998]
[null,3451,41.948999999999998,225852,101.35]
[null,2239,21.425999999999998,79338,36.009]
[null,5995,54.158999999999999,225039,109.163]
[null,2296,21.646000000000001,78326,38.24]
[null,566,28.783000000000001,323289,130.38399999999999]
[null,3278,43.762999999999998,113846,53.183999999999997]
[null,1755,20.728000000000002,40026,18.847000000000001]
[null,5147,60.106999999999999,113621,57.091000000000001]
[null,1896,19.276,39518,19.942]
[null,5464,40.514000000000003,164220,72.16]
[]
[null,1640,1151,2878,1157,235,3451,2239,5995,2296,566,3278,1755,5147,1896,5464]
[null,31.408999999999999,14.689,56.677,15.378,11.903,41.948999999999998,21.425999999999998,54.158999999999999,21.646000000000001,28.783000000000001,43.762999999999998,20.728000000000002,60.106999999999999,19.276,40.514000000000003]
[null,105403,36836,104929,36491,149849,225852,79338,225039,78326,323289,113846,40026,113621,39518,164220]
[null,49.569000000000003,17.238,53.128999999999998,18.718,63.756999999999998,101.35,36.009,109.163,38.24,130.38399999999999,53.183999999999997,18.847000000000001,57.091000000000001,19.942,72.16]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann kWh",1640,1151,2878,1157,235,3451,2239,5995,2296,566,3278,1755,5147,1896,5464,39148]
[null,"Ann peak kW",31.408999999999999,14.689,56.677,15.378,11.903,41.948999999999998,21.425999999999998,54.158999999999999,21.646000000000001,28.783000000000001,43.762999999999998,20.728000000000002,60.106999999999999,19.276,40.514000000000003,482.40699999999998]
[null,"EFLH Heating",52.21433347129804,78.357954932262231,50.778975598567321,75.237352061386389,19.742921952448963,82.266561777396362,104.49920657145525,110.69259033586293,106.07040561766608,19.664385227391168,74.903457258414647,84.668081821690464,85.630625384730564,98.360655737704917,134.8669595695315,"20-135",81.151392910965228]
["Cooling","Ann kWh",105403,36836,104929,36491,149849,225852,79338,225039,78326,323289,113846,40026,113621,39518,164220,1836583]
[null,"Ann peak kW",49.569000000000003,17.238,53.128999999999998,18.718,63.756999999999998,101.35,36.009,109.163,38.24,130.38399999999999,53.183999999999997,18.847000000000001,57.091000000000001,19.942,72.16,838.78099999999995]
[null,"EFLH Cooling",2126.3894772942767,2136.9068337394128,1974.9854128630316,1949.5138369483918,2350.3144752733033,2228.4361124815,2203.2825127051569,2061.4951952584665,2048.2740585774059,2479.5143575898887,2140.6061973525875,2123.7332201411364,1990.1735825261424,1981.6467756493832,2275.7760532150778,"1950-2480",2189.5858394503452]
[]
["SCooper Tech Col 24h 7days w setback - Baseline Design.SIM"]
[null,2286,18.289000000000001,132638,51.241999999999997]
[null,1475,10.384,45958,17.859000000000002]
[null,3489,27.847999999999999,131998,54.780999999999999]
[null,1475,10.840999999999999,45638,19.288]
[null,58,7.4829999999999997,186793,66.242999999999995]
[null,5060,33.024999999999999,281886,104.361]
[null,3063,16.937999999999999,98187,37.110999999999997]
[null,8006,40.433,280955,112.095]
[null,3052,17.783999999999999,97360,39.253]
[null,0,0,403828,133.977]
[null,4293,34.478999999999999,142094,54.677]
[null,2156,14.409000000000001,49509,19.460999999999999]
[null,6108,42.985999999999997,141776,58.548999999999999]
[null,2276,14.584,49102,20.448]
[null,6302,19.068000000000001,204963,73.975999999999999]
[]
[null,2286,1475,3489,1475,58,5060,3063,8006,3052,0,4293,2156,6108,2276,6302]
[null,18.289000000000001,10.384,27.847999999999999,10.840999999999999,7.4829999999999997,33.024999999999999,16.937999999999999,40.433,17.783999999999999,0,34.478999999999999,14.409000000000001,42.985999999999997,14.584,19.068000000000001]
[null,132638,45958,131998,45638,186793,281886,98187,280955,97360,403828,142094,49509,141776,49102,204963]
[null,51.241999999999997,17.859000000000002,54.780999999999999,19.288,66.242999999999995,104.361,37.110999999999997,112.095,39.253,133.977,54.677,19.460999999999999,58.548999999999999,20.448,73.975999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann kWh",2286,1475,3489,1475,58,5060,3063,8006,3052,0,4293,2156,6108,2276,6302,49099]
[null,"Ann peak kW",18.289000000000001,10.384,27.847999999999999,10.840999999999999,7.4829999999999997,33.024999999999999,16.937999999999999,40.433,17.783999999999999,0,34.478999999999999,14.409000000000001,42.985999999999997,14.584,19.068000000000001,308.55099999999999]
[null,"EFLH Heating",124.99316529061183,142.04545454545453,125.28727377190462,136.0575592657504,7.7509020446345049,153.21725965177896,180.83599008147362,198.00657878465609,171.61493477282951,"",124.51057165231011,149.62870428204593,142.0927743916624,156.06143719144268,330.50136354101107,"8-331",159.1276644703793]
["Cooling","Ann kWh",132638,45958,131998,45638,186793,281886,98187,280955,97360,403828,142094,49509,141776,49102,204963,2292685]
[null,"Ann peak kW",51.241999999999997,17.859000000000002,54.780999999999999,19.288,66.242999999999995,104.361,37.110999999999997,112.095,39.253,133.977,54.677,19.460999999999999,58.548999999999999,20.448,73.975999999999999,863.32100000000003]
[null,"EFLH Cooling",2588.4625892822296,2573.3803684416816,2409.558058450923,2366.1343840729987,2819.8149238410097,2701.0664903555926,2645.7654064832532,2506.4008207324146,2480.3199755432706,3014.1591467192129,2598.78925325091,2544.0110991213196,2421.4931083366068,2401.3106416275432,2770.6688655780254,"2366-3014",2655.6576290858206]
[]
[]
["SCooper Office 8-17 wo setback - Baseline Design.SIM"]
[null,181,2.2989999999999999,6335,3.7429999999999999]
[null,1810,5.1139999999999999,13632,9.6140000000000008]
[null,582,2.1019999999999999,4485,3.0219999999999998]
[null,1833,5.165,12979,9.3670000000000009]
[null,1,1.304,11629,10.282999999999999]
[null,402,2.8879999999999999,6980,3.9620000000000002]
[null,2271,6.6890000000000001,15142,9.86]
[null,694,2.6259999999999999,5161,3.4180000000000001]
[null,2279,6.7060000000000004,14442,10.079000000000001]
[null,28,2.415,13659,12.592000000000001]
[]
[null,181,1810,582,1833,1,402,2271,694,2279,28]
[null,2.2989999999999999,5.1139999999999999,2.1019999999999999,5.165,1.304,2.8879999999999999,6.6890000000000001,2.6259999999999999,6.7060000000000004,2.415]
[null,6335,13632,4485,12979,11629,6980,15142,5161,14442,13659]
[null,3.7429999999999999,9.6140000000000008,3.0219999999999998,9.3670000000000009,10.282999999999999,3.9620000000000002,9.86,3.4180000000000001,10.079000000000001,12.592000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",181,1810,582,1833,1,402,2271,694,2279,28,10081]
[null,"Ann peak kW",2.2989999999999999,5.1139999999999999,2.1019999999999999,5.165,1.304,2.8879999999999999,6.6890000000000001,2.6259999999999999,6.7060000000000004,2.415,37.308]
[null,"EFLH Heating",78.729882557633758,353.93038717246776,276.87916270218841,354.88867376573086,0.76687116564417179,139.196675900277,339.51263268052026,264.2802741812643,339.84491500149119,11.594202898550725,"1-355",270.21014259676207]
["Cooling","Ann kWh",6335,13632,4485,12979,11629,6980,15142,5161,14442,13659,104444]
[null,"Ann peak kW",3.7429999999999999,9.6140000000000008,3.0219999999999998,9.3670000000000009,10.282999999999999,3.9620000000000002,9.86,3.4180000000000001,10.079000000000001,12.592000000000001,75.940000000000012]
[null,"EFLH Cooling",1692.4926529521774,1417.9321822342415,1484.116479152879,1385.6090530586098,1130.8956530195469,1761.7364967188289,1535.6997971602434,1509.9473376243416,1432.8802460561562,1084.7363405336721,"1085-1762",1375.34895970503]
[]
["SCooper Office 7-19 wo setback - Baseline Design.SIM"]
[null,183,2.2269999999999999,6676,3.7290000000000001]
[null,1572,4.9390000000000001,14665,9.5289999999999999]
[null,514,2.0390000000000001,4800,2.9750000000000001]
[null,1623,5.077,14109,10.029999999999999]
[null,2,1.2250000000000001,14754,10.67]
[null,382,2.8039999999999998,7340,3.956]
[null,2015,6.4980000000000002,16214,9.7720000000000002]
[null,634,2.5569999999999999,5514,3.3570000000000002]
[null,2047,6.6159999999999997,15623,10.884]
[null,36,4.2160000000000002,17084,12.614000000000001]
[]
[null,183,1572,514,1623,2,382,2015,634,2047,36]
[null,2.2269999999999999,4.9390000000000001,2.0390000000000001,5.077,1.2250000000000001,2.8039999999999998,6.4980000000000002,2.5569999999999999,6.6159999999999997,4.2160000000000002]
[null,6676,14665,4800,14109,14754,7340,16214,5514,15623,17084]
[null,3.7290000000000001,9.5289999999999999,2.9750000000000001,10.029999999999999,10.67,3.956,9.7720000000000002,3.3570000000000002,10.884,12.614000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",183,1572,514,1623,2,382,2015,634,2047,36,9008]
[null,"Ann peak kW",2.2269999999999999,4.9390000000000001,2.0390000000000001,5.077,1.2250000000000001,2.8039999999999998,6.4980000000000002,2.5569999999999999,6.6159999999999997,4.2160000000000002,38.198]
[null,"EFLH Heating",82.173327346205667,318.28305324964566,252.08435507601763,319.67697459129408,1.6326530612244896,136.2339514978602,310.0954139735303,247.94681267109894,309.40145102781139,8.5388994307400381,"2-320",235.82386512382848]
["Cooling","Ann kWh",6676,14665,4800,14109,14754,7340,16214,5514,15623,17084,116779]
[null,"Ann peak kW",3.7290000000000001,9.5289999999999999,2.9750000000000001,10.029999999999999,10.67,3.956,9.7720000000000002,3.3570000000000002,10.884,12.614000000000001,77.516000000000005]
[null,"EFLH Cooling",1790.2923035666397,1538.9862524923917,1613.4453781512605,1406.6799601196412,1382.755388940956,1855.4095045500505,1659.2304543593941,1642.5379803395888,1435.409775817714,1354.3681623592834,"1354-1855",1506.5147840445843]
[]
["SCooper Office 7-22 wo setback - Baseline Design.SIM"]
[null,174,2.165,7069,3.7309999999999999]
[null,1356,4.76,15752,9.5709999999999997]
[null,475,2.032,5160,2.9860000000000002]
[null,1417,4.8860000000000001,15196,9.984]
[null,1,1.3140000000000001,18106,10.856999999999999]
[null,342,2.722,7742,3.952]
[null,1797,6.258,17355,9.7759999999999998]
[null,581,2.4809999999999999,5910,3.355]
[null,1844,6.3929999999999998,16784,10.811999999999999]
[null,29,4.2279999999999998,20729,12.726000000000001]
[]
[null,174,1356,475,1417,1,342,1797,581,1844,29]
[null,2.165,4.76,2.032,4.8860000000000001,1.3140000000000001,2.722,6.258,2.4809999999999999,6.3929999999999998,4.2279999999999998]
[null,7069,15752,5160,15196,18106,7742,17355,5910,16784,20729]
[null,3.7309999999999999,9.5709999999999997,2.9860000000000002,9.984,10.856999999999999,3.952,9.7759999999999998,3.355,10.811999999999999,12.726000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",174,1356,475,1417,1,342,1797,581,1844,29,8016]
[null,"Ann peak kW",2.165,4.76,2.032,4.8860000000000001,1.3140000000000001,2.722,6.258,2.4809999999999999,6.3929999999999998,4.2279999999999998,37.239000000000004]
[null,"EFLH Heating",80.36951501154735,284.87394957983196,233.75984251968504,290.01227998362668,0.76103500761035003,125.64290962527554,287.15244487056566,234.17976622329707,288.44048177694356,6.8590350047303694,"1-290",215.25819705147828]
["Cooling","Ann kWh",7069,15752,5160,15196,18106,7742,17355,5910,16784,20729,129803]
[null,"Ann peak kW",3.7309999999999999,9.5709999999999997,2.9860000000000002,9.984,10.856999999999999,3.952,9.7759999999999998,3.355,10.811999999999999,12.726000000000001,77.75]
[null,"EFLH Cooling",1894.6663093004556,1645.8050360463901,1728.0643000669791,1522.0352564102564,1667.6798378926039,1959.008097165992,1775.2659574468084,1761.5499254843517,1552.349241583426,1628.8700298601289,"1522-1959",1669.4919614147909]
[]
["SCooper Office 6-19 7days wo setback - Baseline Design.SIM"]
[null,314,2.976,6835,3.734]
[null,1647,7.1680000000000001,15273,9.5370000000000008]
[null,663,3.9209999999999998,4966,2.9820000000000002]
[null,1732,7.2480000000000002,14663,10.050000000000001]
[null,78,2.83,17394,10.734999999999999]
[null,515,3.516,7528,3.9620000000000002]
[null,1969,8.98,16920,9.7970000000000006]
[null,771,4.3179999999999996,5693,3.363]
[null,2096,8.8620000000000001,16233,10.9]
[null,966,44.201000000000001,19796,12.694000000000001]
[]
[null,314,1647,663,1732,78,515,1969,771,2096,966]
[null,2.976,7.1680000000000001,3.9209999999999998,7.2480000000000002,2.83,3.516,8.98,4.3179999999999996,8.8620000000000001,44.201000000000001]
[null,6835,15273,4966,14663,17394,7528,16920,5693,16233,19796]
[null,3.734,9.5370000000000008,2.9820000000000002,10.050000000000001,10.734999999999999,3.9620000000000002,9.7970000000000006,3.363,10.9,12.694000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",314,1647,663,1732,78,515,1969,771,2096,966,10751]
[null,"Ann peak kW",2.976,7.1680000000000001,3.9209999999999998,7.2480000000000002,2.83,3.516,8.98,4.3179999999999996,8.8620000000000001,44.201000000000001,94.02]
[null,"EFLH Heating",105.51075268817205,229.77120535714286,169.08951798010713,238.96247240618101,27.561837455830389,146.47326507394766,219.26503340757236,178.55488652153775,236.51545926427443,21.854709169475804,"22-239",114.34801106147629]
["Cooling","Ann kWh",6835,15273,4966,14663,17394,7528,16920,5693,16233,19796,125301]
[null,"Ann peak kW",3.734,9.5370000000000008,2.9820000000000002,10.050000000000001,10.734999999999999,3.9620000000000002,9.7970000000000006,3.363,10.9,12.694000000000001,77.754000000000005]
[null,"EFLH Cooling",1830.4767005891806,1601.4469959106636,1665.3252850435947,1459.004975124378,1620.3074056823475,1900.0504795557799,1727.0593038685311,1692.8337793636633,1489.2660550458716,1559.4769182290845,"1459-1900",1611.505517401034]
[]
["SCooper Office 6-21 7days wo setback - Baseline Design.SIM"]
[null,349,2.8530000000000002,7041,3.6779999999999999]
[null,1653,6.7880000000000003,15876,9.61]
[null,699,3.7519999999999998,5204,3.01]
[null,1726,6.883,15248,10.048999999999999]
[null,66,2.645,19386,10.726000000000001]
[null,525,3.355,7686,3.8889999999999998]
[null,1981,8.4049999999999994,17401,9.6760000000000002]
[null,799,4.109,5897,3.3650000000000002]
[null,2086,8.3849999999999998,16710,10.837999999999999]
[null,919,16.498999999999999,22406,12.391]
[]
[null,349,1653,699,1726,66,525,1981,799,2086,919]
[null,2.8530000000000002,6.7880000000000003,3.7519999999999998,6.883,2.645,3.355,8.4049999999999994,4.109,8.3849999999999998,16.498999999999999]
[null,7041,15876,5204,15248,19386,7686,17401,5897,16710,22406]
[null,3.6779999999999999,9.61,3.01,10.048999999999999,10.726000000000001,3.8889999999999998,9.6760000000000002,3.3650000000000002,10.837999999999999,12.391]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",349,1653,699,1726,66,525,1981,799,2086,919,10803]
[null,"Ann peak kW",2.8530000000000002,6.7880000000000003,3.7519999999999998,6.883,2.645,3.355,8.4049999999999994,4.109,8.3849999999999998,16.498999999999999,63.673999999999992]
[null,"EFLH Heating",122.32737469330529,243.51797289334118,186.30063965884864,250.76274880139474,24.952741020793951,156.48286140089419,235.69303985722786,194.45120467266975,248.77757901013715,55.700345475483367,"25-251",169.66108615761539]
["Cooling","Ann kWh",7041,15876,5204,15248,19386,7686,17401,5897,16710,22406,132855]
[null,"Ann peak kW",3.6779999999999999,9.61,3.01,10.048999999999999,10.726000000000001,3.8889999999999998,9.6760000000000002,3.3650000000000002,10.837999999999999,12.391,77.232000000000014]
[null,"EFLH Cooling",1914.3556280587277,1652.0291363163371,1728.9036544850499,1517.3649119315355,1807.383926906582,1976.3435330419131,1798.3670938404298,1752.4517087667161,1541.7973795903304,1808.247921878783,"1517-1976",1720.2066500932253]
[]
["SCooper Office 5-23 7days wo setback - Baseline Design.SIM"]
[null,402,2.8519999999999999,7444,3.7360000000000002]
[null,1541,6.8419999999999996,16999,9.5909999999999993]
[null,736,3.778,5513,3.0049999999999999]
[null,1597,6.9240000000000004,16376,10.031000000000001]
[null,55,2.3210000000000002,23386,11.061]
[null,556,3.3130000000000002,8152,3.9569999999999999]
[null,1815,8.2650000000000006,18717,9.8079999999999998]
[null,799,4.0999999999999996,6297,3.371]
[null,1909,8.2210000000000001,18027,10.846]
[null,1043,44.796999999999997,26266,12.846]
[]
[null,402,1541,736,1597,55,556,1815,799,1909,1043]
[null,2.8519999999999999,6.8419999999999996,3.778,6.9240000000000004,2.3210000000000002,3.3130000000000002,8.2650000000000006,4.0999999999999996,8.2210000000000001,44.796999999999997]
[null,7444,16999,5513,16376,23386,8152,18717,6297,18027,26266]
[null,3.7360000000000002,9.5909999999999993,3.0049999999999999,10.031000000000001,11.061,3.9569999999999999,9.8079999999999998,3.371,10.846,12.846]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",402,1541,736,1597,55,556,1815,799,1909,1043,10453]
[null,"Ann peak kW",2.8519999999999999,6.8419999999999996,3.778,6.9240000000000004,2.3210000000000002,3.3130000000000002,8.2650000000000006,4.0999999999999996,8.2210000000000001,44.796999999999997,91.412999999999997]
[null,"EFLH Heating",140.95371669004209,225.22654194679919,194.81206987824245,230.64702484113229,23.696682464454973,167.82372472079686,219.60072595281306,194.87804878048783,232.21019340712809,23.282809116681921,"23-232",114.34916259175391]
["Cooling","Ann kWh",7444,16999,5513,16376,23386,8152,18717,6297,18027,26266,147177]
[null,"Ann peak kW",3.7360000000000002,9.5909999999999993,3.0049999999999999,10.031000000000001,11.061,3.9569999999999999,9.8079999999999998,3.371,10.846,12.846,78.25200000000001]
[null,"EFLH Cooling",1992.5053533190578,1772.3907830257535,1834.6089850249584,1632.5391287010268,2114.2753819726968,2060.1465756886532,1908.3401305057096,1867.991693859389,1662.0874054951134,2044.6831698583217,"1633-2114",1880.8081582579357]
[]
["SCooper Office 24 7days wo setback - Baseline Design.SIM"]
[null,526,2.7719999999999998,7944,3.758]
[null,1623,6.7169999999999996,18406,9.5990000000000002]
[null,847,3.7210000000000001,5960,3.0289999999999999]
[null,1674,6.78,17808,10.099]
[null,10,1.2070000000000001,28702,11.427]
[null,641,3.238,8678,3.9769999999999999]
[null,1884,8.1300000000000008,20226,9.8550000000000004]
[null,879,4.0419999999999998,6777,3.3959999999999999]
[null,1918,8.0969999999999995,19508,10.904]
[null,1085,45.264000000000003,31956,13.198]
[]
[null,526,1623,847,1674,10,641,1884,879,1918,1085]
[null,2.7719999999999998,6.7169999999999996,3.7210000000000001,6.78,1.2070000000000001,3.238,8.1300000000000008,4.0419999999999998,8.0969999999999995,45.264000000000003]
[null,7944,18406,5960,17808,28702,8678,20226,6777,19508,31956]
[null,3.758,9.5990000000000002,3.0289999999999999,10.099,11.427,3.9769999999999999,9.8550000000000004,3.3959999999999999,10.904,13.198]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",526,1623,847,1674,10,641,1884,879,1918,1085,11087]
[null,"Ann peak kW",2.7719999999999998,6.7169999999999996,3.7210000000000001,6.78,1.2070000000000001,3.238,8.1300000000000008,4.0419999999999998,8.0969999999999995,45.264000000000003,89.968000000000004]
[null,"EFLH Heating",189.75468975468976,241.62572577043323,227.6269819940876,246.90265486725662,8.2850041425020713,197.96170475602224,231.73431734317342,217.46660069272639,236.87785599604794,23.970484270060091,"8-247",123.23270496176418]
["Cooling","Ann kWh",7944,18406,5960,17808,28702,8678,20226,6777,19508,31956,165965]
[null,"Ann peak kW",3.758,9.5990000000000002,3.0289999999999999,10.099,11.427,3.9769999999999999,9.8550000000000004,3.3959999999999999,10.904,13.198,79.24199999999999]
[null,"EFLH Cooling",2113.8903672166048,1917.4914053547245,1967.6460878177618,1763.3429052381423,2511.7703684256585,2182.0467689212974,2052.3592085235919,1995.583038869258,1789.0682318415261,2421.2759509016519,"1763-2512",2094.4070063855029]
[]
[]
["SCooper Rest 9-18 wo setback - Baseline Design.SIM"]
[null,1296,3.0920000000000001,9202,5.7539999999999996]
[null,1469,2.839,8415,5.7320000000000002]
[null,1781,2.927,7377,5.907]
[null,1657,2.9449999999999998,8113,6.806,null,null,null,null,null,null,null,null,null,null,null,"Restaurant Defaults do not estimate require ventilation, refrigeration, or cooking loads correctly!"]
[null,1,0.43,3903,2.7850000000000001]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"From DOE Com Bldg Stocks Models.pdf"]
[]
[]
[]
[]
[null,1296,1469,1781,1657,1]
[null,3.0920000000000001,2.839,2.927,2.9449999999999998,0.43]
[null,9202,8415,7377,8113,3903]
[null,5.7539999999999996,5.7320000000000002,5.907,6.806,2.7850000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",1296,1469,1781,1657,1,null,null,null,null,null,6204]
[null,"Ann peak kW",3.0920000000000001,2.839,2.927,2.9449999999999998,0.43,null,null,null,null,null,12.233000000000001]
[null,"EFLH Heating",419.14618369987062,517.43571680169077,608.47283908438669,562.64855687606121,2.3255813953488373,"","","","","","2-608",507.15278345459001]
["Cooling","Ann kWh",9202,8415,7377,8113,3903,null,null,null,null,null,37010]
[null,"Ann peak kW",5.7539999999999996,5.7320000000000002,5.907,6.806,2.7850000000000001,null,null,null,null,null,26.984000000000002]
[null,"EFLH Cooling",1599.2353145637819,1468.0739706908582,1248.8572879634332,1192.0364384366735,1401.436265709156,"","","","","","1192-1599",1371.5535131930033]
[]
["SCooper Rest 8-20 wo setback - Baseline Design.SIM"]
[null,1231,3.0960000000000001,9893,5.7590000000000003]
[null,1402,2.8460000000000001,9149,5.8760000000000003]
[null,1651,2.9039999999999999,8119,5.5289999999999999]
[null,1573,2.9529999999999998,8826,6.7939999999999996]
[null,1,0.59599999999999997,4493,2.6709999999999998]
[]
[]
[]
[]
[]
[]
[null,1231,1402,1651,1573,1]
[null,3.0960000000000001,2.8460000000000001,2.9039999999999999,2.9529999999999998,0.59599999999999997]
[null,9893,9149,8119,8826,4493]
[null,5.7590000000000003,5.8760000000000003,5.5289999999999999,6.7939999999999996,2.6709999999999998]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",1231,1402,1651,1573,1,null,null,null,null,null,5858]
[null,"Ann peak kW",3.0960000000000001,2.8460000000000001,2.9039999999999999,2.9529999999999998,0.59599999999999997,null,null,null,null,null,12.395]
[null,"EFLH Heating",397.609819121447,492.6212227687983,568.52617079889808,532.67863189976299,1.6778523489932886,"","","","","","2-569",472.60992335619204]
["Cooling","Ann kWh",9893,9149,8119,8826,4493,null,null,null,null,null,40480]
[null,"Ann peak kW",5.7590000000000003,5.8760000000000003,5.5289999999999999,6.7939999999999996,2.6709999999999998,null,null,null,null,null,26.629000000000001]
[null,"EFLH Cooling",1717.8329571106094,1557.0115724982982,1468.4391390848255,1299.0874300853695,1682.1415200299514,"","","","","","1299-1718",1520.1472079312027]
[]
["SCooper Rest 7-22 wo setback - Baseline Design.SIM"]
[null,1104,3.052,10485,5.9039999999999999]
[null,1261,3.5790000000000002,9758,5.9779999999999998]
[null,1478,4.952,8707,5.4930000000000003]
[null,1351,3.3530000000000002,9431,6.3150000000000004]
[null,2,0.98299999999999998,5032,2.5649999999999999]
[]
[]
[]
[]
[]
[]
[null,1104,1261,1478,1351,2]
[null,3.052,3.5790000000000002,4.952,3.3530000000000002,0.98299999999999998]
[null,10485,9758,8707,9431,5032]
[null,5.9039999999999999,5.9779999999999998,5.4930000000000003,6.3150000000000004,2.5649999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",1104,1261,1478,1351,2,null,null,null,null,null,5196]
[null,"Ann peak kW",3.052,3.5790000000000002,4.952,3.3530000000000002,0.98299999999999998,null,null,null,null,null,15.919]
[null,"EFLH Heating",361.7300131061599,352.33305392567752,298.46526655896605,402.92275574112733,2.0345879959308242,"","","","","","2-403",326.40241221182237]
["Cooling","Ann kWh",10485,9758,8707,9431,5032,null,null,null,null,null,43413]
[null,"Ann peak kW",5.9039999999999999,5.9779999999999998,5.4930000000000003,6.3150000000000004,2.5649999999999999,null,null,null,null,null,26.255000000000003]
[null,"EFLH Cooling",1775.9146341463415,1632.3185011709602,1585.1083196795921,1493.4283452098177,1961.7933723196882,"","","","","","1493-1962",1653.5136164540086]
[]
["SCooper Rest 9-22 7days wo setback - Baseline Design.SIM"]
[null,718,2.94,12245,5.827]
[null,802,2.7429999999999999,11424,5.68]
[null,1011,6.835,10498,5.4240000000000004]
[null,915,4.9219999999999997,11210,6.2640000000000002]
[null,0,0,6620,2.5139999999999998]
[]
[]
[]
[]
[]
[]
[null,718,802,1011,915,0]
[null,2.94,2.7429999999999999,6.835,4.9219999999999997,0]
[null,12245,11424,10498,11210,6620]
[null,5.827,5.68,5.4240000000000004,6.2640000000000002,2.5139999999999998]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",718,802,1011,915,0,null,null,null,null,null,3446]
[null,"Ann peak kW",2.94,2.7429999999999999,6.835,4.9219999999999997,0,null,null,null,null,null,17.440000000000001]
[null,"EFLH Heating",244.21768707482994,292.38060517681373,147.9151426481346,185.90004063388866,"","","","","","","148-292",197.59174311926603]
["Cooling","Ann kWh",12245,11424,10498,11210,6620,null,null,null,null,null,51997]
[null,"Ann peak kW",5.827,5.68,5.4240000000000004,6.2640000000000002,2.5139999999999998,null,null,null,null,null,25.709]
[null,"EFLH Cooling",2101.4244036382356,2011.267605633803,1935.4719764011797,1789.5913154533844,2633.2537788385048,"","","","","","1790-2633",2022.5212960441868]
[]
["SCooper Rest 8-22 7days wo setback - Baseline Design.SIM"]
[null,739,5.1609999999999996,12584,5.8860000000000001]
[null,829,5.31,11774,5.8840000000000003]
[null,998,7.8810000000000002,10840,5.4729999999999999]
[null,887,6.9080000000000004,11542,6.3049999999999997]
[null,0,0,6898,2.536]
[]
[]
[]
[]
[]
[]
[null,739,829,998,887,0]
[null,5.1609999999999996,5.31,7.8810000000000002,6.9080000000000004,0]
[null,12584,11774,10840,11542,6898]
[null,5.8860000000000001,5.8840000000000003,5.4729999999999999,6.3049999999999997,2.536]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",739,829,998,887,0,null,null,null,null,null,3453]
[null,"Ann peak kW",5.1609999999999996,5.31,7.8810000000000002,6.9080000000000004,0,null,null,null,null,null,25.26]
[null,"EFLH Heating",143.18930439837243,156.120527306968,126.63367592945058,128.40185292414591,"","","","","","","127-156",136.69833729216151]
["Cooling","Ann kWh",12584,11774,10840,11542,6898,null,null,null,null,null,53638]
[null,"Ann peak kW",5.8860000000000001,5.8840000000000003,5.4729999999999999,6.3049999999999997,2.536,null,null,null,null,null,26.084]
[null,"EFLH Cooling",2137.9544682296973,2001.0197144799456,1980.6321944089166,1830.6106264869152,2720.0315457413249,"","","","","","1831-2720",2056.3563870571998]
[]
["SCooper Rest 5-23 7days wo setback - Baseline Design.SIM"]
[null,538,5.4980000000000002,13635,5.9880000000000004]
[null,643,5.9189999999999996,12836,6.242]
[null,775,8.0609999999999999,11874,5.5579999999999998]
[null,627,7.1769999999999996,12618,6.1479999999999997]
[null,0,0,7850,2.6110000000000002]
[]
[]
[]
[]
[]
[]
[null,538,643,775,627,0]
[null,5.4980000000000002,5.9189999999999996,8.0609999999999999,7.1769999999999996,0]
[null,13635,12836,11874,12618,7850]
[null,5.9880000000000004,6.242,5.5579999999999998,6.1479999999999997,2.6110000000000002]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",538,643,775,627,0,null,null,null,null,null,2583]
[null,"Ann peak kW",5.4980000000000002,5.9189999999999996,8.0609999999999999,7.1769999999999996,0,null,null,null,null,null,26.655000000000001]
[null,"EFLH Heating",97.853765005456523,108.63321507011321,96.141917876194015,87.362407691235902,"","","","","","","87-109",96.904895891952719]
["Cooling","Ann kWh",13635,12836,11874,12618,7850,null,null,null,null,null,58813]
[null,"Ann peak kW",5.9880000000000004,6.242,5.5579999999999998,6.1479999999999997,2.6110000000000002,null,null,null,null,null,26.547000000000001]
[null,"EFLH Cooling",2277.0541082164327,2056.392181992951,2136.3799928031667,2052.3747560182173,3006.5109153581002,"","","","","","2052-3007",2215.4292387087053]
[]
["SCooper Rest 24 7days wo setback - Baseline Design.SIM"]
[null,52,2.2370000000000001,19169,6.6289999999999996]
[null,72,2.1269999999999998,18344,7.0289999999999999]
[null,117,5.15,17152,6.0860000000000003]
[null,68,2.4489999999999998,18109,6.968]
[null,0,0,10257,3.0369999999999999]
[]
[]
[]
[]
[]
[]
[null,52,72,117,68,0]
[null,2.2370000000000001,2.1269999999999998,5.15,2.4489999999999998,0]
[null,19169,18344,17152,18109,10257]
[null,6.6289999999999996,7.0289999999999999,6.0860000000000003,6.968,3.0369999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",52,72,117,68,0,null,null,null,null,null,309]
[null,"Ann peak kW",2.2370000000000001,2.1269999999999998,5.15,2.4489999999999998,0,null,null,null,null,null,11.962999999999999]
[null,"EFLH Heating",23.245417970496199,33.850493653032444,22.718446601941746,27.766435279706005,"","","","","","","23-34",25.829641394299092]
["Cooling","Ann kWh",19169,18344,17152,18109,10257,null,null,null,null,null,83031]
[null,"Ann peak kW",6.6289999999999996,7.0289999999999999,6.0860000000000003,6.968,3.0369999999999999,null,null,null,null,null,29.748999999999999]
[null,"EFLH Cooling",2891.6880374113744,2609.7595675060466,2818.2714426552743,2598.8805970149256,3377.3460651959172,"","","","","","2599-3377",2791.0518000605061]
[]
["SCooper Rest 10-23 7day Hol1 wo setback - Baseline Design.SIM"]
[null,1621,3.1989999999999998,10968,6.0339999999999998]
[null,2083,3.024,10230,5.5629999999999997]
[null,2339,3.0790000000000002,9474,5.4509999999999996]
[null,2201,3.0579999999999998,10047,6.1029999999999998]
[null,109,0.96299999999999997,5458,2.5289999999999999]
[]
[]
[]
[]
[]
[]
[null,1621,2083,2339,2201,109]
[null,3.1989999999999998,3.024,3.0790000000000002,3.0579999999999998,0.96299999999999997]
[null,10968,10230,9474,10047,5458]
[null,6.0339999999999998,5.5629999999999997,5.4509999999999996,6.1029999999999998,2.5289999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",1621,2083,2339,2201,109,null,null,null,null,null,8353]
[null,"Ann peak kW",3.1989999999999998,3.024,3.0790000000000002,3.0579999999999998,0.96299999999999997,null,null,null,null,null,13.322999999999999]
[null,"EFLH Heating",506.72085026570807,688.82275132275129,759.66222799610262,719.75147155003276,113.18795430944964,"","","","","","113-760",626.96089469338744]
["Cooling","Ann kWh",10968,10230,9474,10047,5458,null,null,null,null,null,46177]
[null,"Ann peak kW",6.0339999999999998,5.5629999999999997,5.4509999999999996,6.1029999999999998,2.5289999999999999,null,null,null,null,null,25.679999999999996]
[null,"EFLH Cooling",1817.6997016904211,1838.9358259931691,1738.0297193175566,1646.2395543175487,2158.165282720443,"","","","","","1646-2158",1798.1697819314645]
[]
["SCooper Rest 8-23 12-20 Hol2 wo setback - Baseline Design.SIM"]
[null,795,2.9489999999999998,12017,6.0519999999999996]
[null,949,2.8170000000000002,11158,5.8929999999999998]
[null,1186,2.8250000000000002,10329,5.5010000000000003]
[null,1082,2.8,11004,6.1230000000000002]
[null,0,0,6502,2.577]
[]
[]
[]
[]
[]
[]
[null,795,949,1186,1082,0]
[null,2.9489999999999998,2.8170000000000002,2.8250000000000002,2.8,0]
[null,12017,11158,10329,11004,6502]
[null,6.0519999999999996,5.8929999999999998,5.5010000000000003,6.1230000000000002,2.577]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",795,949,1186,1082,0,null,null,null,null,null,4012]
[null,"Ann peak kW",2.9489999999999998,2.8170000000000002,2.8250000000000002,2.8,0,null,null,null,null,null,11.391000000000002]
[null,"EFLH Heating",269.58290946083417,336.88320908768191,419.82300884955748,386.42857142857144,"","","","","","","270-420",352.20788341673244]
["Cooling","Ann kWh",12017,11158,10329,11004,6502,null,null,null,null,null,51010]
[null,"Ann peak kW",6.0519999999999996,5.8929999999999998,5.5010000000000003,6.1230000000000002,2.577,null,null,null,null,null,26.146000000000001]
[null,"EFLH Cooling",1985.6245869134173,1893.4328864754793,1877.6586075259042,1797.1582557569818,2523.0888630190143,"","","","","","1797-2523",1950.9676432341466]
[]
[]
["SCooper Htl 9-18 wo setback - Baseline Design.SIM"]
[null,2019,4.4390000000000001,7466,3.758]
[null,2651,5.6369999999999996,4564,2.8109999999999999]
[null,2871,5.6059999999999999,4607,2.9369999999999998]
[null,2741,4.7089999999999996,6633,4.3250000000000002]
[null,49,1.0309999999999999,974,0.49099999999999999]
[null,2450,5.024,10910,4.8959999999999999]
[null,2664,5.2430000000000003,6506,3.637]
[null,2772,5.2089999999999996,6818,4.0010000000000003]
[null,2894,5.0970000000000004,9496,5.8719999999999999]
[null,165,1.389,952,0.56399999999999995]
[]
[null,2019,2651,2871,2741,49,2450,2664,2772,2894,165]
[null,4.4390000000000001,5.6369999999999996,5.6059999999999999,4.7089999999999996,1.0309999999999999,5.024,5.2430000000000003,5.2089999999999996,5.0970000000000004,1.389]
[null,7466,4564,4607,6633,974,10910,6506,6818,9496,952]
[null,3.758,2.8109999999999999,2.9369999999999998,4.3250000000000002,0.49099999999999999,4.8959999999999999,3.637,4.0010000000000003,5.8719999999999999,0.56399999999999995]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",2019,2651,2871,2741,49,2450,2664,2772,2894,165,21276]
[null,"Ann peak kW",4.4390000000000001,5.6369999999999996,5.6059999999999999,4.7089999999999996,1.0309999999999999,5.024,5.2430000000000003,5.2089999999999996,5.0970000000000004,1.389,43.384]
[null,"EFLH Heating",454.83216940752419,470.28561291467093,512.1298608633607,582.07687407092806,47.526673132880703,487.65923566878979,508.10604615678045,532.15588404684206,567.78497155189325,118.79049676025917,"48-582",490.41121150654618]
["Cooling","Ann kWh",7466,4564,4607,6633,974,10910,6506,6818,9496,952,58926]
[null,"Ann peak kW",3.758,2.8109999999999999,2.9369999999999998,4.3250000000000002,0.49099999999999999,4.8959999999999999,3.637,4.0010000000000003,5.8719999999999999,0.56399999999999995,33.292000000000002]
[null,"EFLH Cooling",1986.6950505588079,1623.6214870152971,1568.6074225400068,1533.6416184971097,1983.7067209775967,2228.3496732026142,1788.8369535331317,1704.0739815046236,1617.1662125340599,1687.9432624113476,"1534-2228",1769.9747687132042]
[]
["SCooper Htl 8-21 wo setback - Baseline Design.SIM"]
[null,2165,4.8319999999999999,7549,3.758]
[null,2823,5.7080000000000002,4653,2.8130000000000002]
[null,3042,5.6790000000000003,4699,2.94]
[null,2898,5.1539999999999999,6750,4.3259999999999996]
[null,92,1.0569999999999999,975,0.53]
[null,2518,5.024,11040,4.8920000000000003]
[null,2819,5.4989999999999997,6603,3.6389999999999998]
[null,2921,5.4429999999999996,6922,4.0019999999999998]
[null,2980,5.0960000000000001,9644,5.8719999999999999]
[null,232,1.532,988,0.64900000000000002]
[]
[null,2165,2823,3042,2898,92,2518,2819,2921,2980,232]
[null,4.8319999999999999,5.7080000000000002,5.6790000000000003,5.1539999999999999,1.0569999999999999,5.024,5.4989999999999997,5.4429999999999996,5.0960000000000001,1.532]
[null,7549,4653,4699,6750,975,11040,6603,6922,9644,988]
[null,3.758,2.8130000000000002,2.94,4.3259999999999996,0.53,4.8920000000000003,3.6389999999999998,4.0019999999999998,5.8719999999999999,0.64900000000000002]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",2165,2823,3042,2898,92,2518,2819,2921,2980,232,22490]
[null,"Ann peak kW",4.8319999999999999,5.7080000000000002,5.6790000000000003,5.1539999999999999,1.0569999999999999,5.024,5.4989999999999997,5.4429999999999996,5.0960000000000001,1.532,45.024000000000001]
[null,"EFLH Heating",448.0546357615894,494.56902592852134,535.65768621236134,562.28172293364378,87.038789025543991,501.19426751592357,512.63866157483187,536.65258129707888,584.7723704866562,151.43603133159269,"87-585",499.51137171286422]
["Cooling","Ann kWh",7549,4653,4699,6750,975,11040,6603,6922,9644,988,59823]
[null,"Ann peak kW",3.758,2.8130000000000002,2.94,4.3259999999999996,0.53,4.8920000000000003,3.6389999999999998,4.0019999999999998,5.8719999999999999,0.64900000000000002,33.420999999999999]
[null,"EFLH Cooling",2008.7812666311868,1654.1059367223604,1598.2993197278911,1560.3328710124829,1839.6226415094338,2256.7457072771872,1814.5094806265458,1729.6351824087958,1642.3705722070845,1522.342064714946,"1522-2257",1789.982346428892]
[]
["SCooper Htl 9-22 7days wo setback - Baseline Design.SIM"]
[null,1940,5.0460000000000003,8147,3.7610000000000001]
[null,2696,5.6989999999999998,5197,2.9449999999999998]
[null,2902,5.6639999999999997,5266,3.0110000000000001]
[null,2688,6.0510000000000002,7314,4.3259999999999996]
[null,125,1.2390000000000001,1387,0.52900000000000003]
[null,2209,4.6959999999999997,11929,4.9279999999999999]
[null,2650,5.5940000000000003,7260,3.7109999999999999]
[null,2743,5.5229999999999997,7631,4.0789999999999997]
[null,2706,6.0389999999999997,10372,5.8719999999999999]
[null,219,1.6459999999999999,1332,0.64900000000000002]
[]
[null,1940,2696,2902,2688,125,2209,2650,2743,2706,219]
[null,5.0460000000000003,5.6989999999999998,5.6639999999999997,6.0510000000000002,1.2390000000000001,4.6959999999999997,5.5940000000000003,5.5229999999999997,6.0389999999999997,1.6459999999999999]
[null,8147,5197,5266,7314,1387,11929,7260,7631,10372,1332]
[null,3.7610000000000001,2.9449999999999998,3.0110000000000001,4.3259999999999996,0.52900000000000003,4.9279999999999999,3.7109999999999999,4.0789999999999997,5.8719999999999999,0.64900000000000002]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",1940,2696,2902,2688,125,2209,2650,2743,2706,219,20878]
[null,"Ann peak kW",5.0460000000000003,5.6989999999999998,5.6639999999999997,6.0510000000000002,1.2390000000000001,4.6959999999999997,5.5940000000000003,5.5229999999999997,6.0389999999999997,1.6459999999999999,47.197000000000003]
[null,"EFLH Heating",384.46294094332143,473.06545007896125,512.35875706214688,444.22409519087751,100.88781275221952,470.40034071550258,473.72184483375042,496.65037117508604,448.08743169398912,133.04981773997571,"101-512",442.35862448884461]
["Cooling","Ann kWh",8147,5197,5266,7314,1387,11929,7260,7631,10372,1332,65835]
[null,"Ann peak kW",3.7610000000000001,2.9449999999999998,3.0110000000000001,4.3259999999999996,0.52900000000000003,4.9279999999999999,3.7109999999999999,4.0789999999999997,5.8719999999999999,0.64900000000000002,33.811]
[null,"EFLH Cooling",2166.179207657538,1764.685908319185,1748.9206243772833,1690.7073509015258,2621.9281663516067,2420.6574675324678,1956.3459983831851,1870.8016670752636,1766.3487738419619,2052.3882896764253,"1691-2622",1947.1473780722249]
[]
["SCooper Htl 8-22 7days wo setback - Baseline Design.SIM"]
[null,2028,6.0209999999999999,8160,3.7610000000000001]
[null,2798,6.5819999999999999,5218,2.9470000000000001]
[null,3007,6.63,5289,3.0129999999999999]
[null,2782,6.6189999999999998,7329,4.3259999999999996]
[null,160,1.3140000000000001,1384,0.52900000000000003]
[null,2263,6.2030000000000003,11963,4.9279999999999999]
[null,2742,6.774,7285,3.714]
[null,2831,6.8140000000000001,7659,4.08]
[null,2768,6.7430000000000003,10402,5.8719999999999999]
[null,277,1.748,1335,0.64900000000000002]
[]
[null,2028,2798,3007,2782,160,2263,2742,2831,2768,277]
[null,6.0209999999999999,6.5819999999999999,6.63,6.6189999999999998,1.3140000000000001,6.2030000000000003,6.774,6.8140000000000001,6.7430000000000003,1.748]
[null,8160,5218,5289,7329,1384,11963,7285,7659,10402,1335]
[null,3.7610000000000001,2.9470000000000001,3.0129999999999999,4.3259999999999996,0.52900000000000003,4.9279999999999999,3.714,4.08,5.8719999999999999,0.64900000000000002]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",2028,2798,3007,2782,160,2263,2742,2831,2768,277,21656]
[null,"Ann peak kW",6.0209999999999999,6.5819999999999999,6.63,6.6189999999999998,1.3140000000000001,6.2030000000000003,6.774,6.8140000000000001,6.7430000000000003,1.748,55.448]
[null,"EFLH Heating",336.82112605879422,425.09875417806137,453.5444947209653,420.30518205166948,121.76560121765601,364.82347251329998,404.78299379982286,415.46815380099792,410.49977754708584,158.46681922196797,"122-454",390.56413215986151]
["Cooling","Ann kWh",8160,5218,5289,7329,1384,11963,7285,7659,10402,1335,66024]
[null,"Ann peak kW",3.7610000000000001,2.9470000000000001,3.0129999999999999,4.3259999999999996,0.52900000000000003,4.9279999999999999,3.714,4.08,5.8719999999999999,0.64900000000000002,33.819000000000003]
[null,"EFLH Cooling",2169.6357351768147,1770.6141839158465,1755.393295718553,1694.1747572815536,2616.2570888468808,2427.556818181818,1961.4970382337103,1877.2058823529412,1771.4577656675749,2057.010785824345,"1694-2616",1952.2753481770601]
[]
["SCooper Htl 5-23 7days wo setback - Baseline Design.SIM"]
[null,2364,6.6159999999999997,8282,3.7610000000000001]
[null,3223,7.0949999999999998,5287,2.9470000000000001]
[null,3418,7.0590000000000002,5364,3.012]
[null,3142,6.915,7442,4.3259999999999996]
[null,303,1.3109999999999999,1357,0.53]
[null,2451,6.78,12269,4.9279999999999999]
[null,3105,7.3339999999999996,7407,3.7109999999999999]
[null,3171,7.26,7800,4.0780000000000003]
[null,2999,6.9779999999999998,10642,5.8719999999999999]
[null,504,1.7989999999999999,1355,0.64900000000000002]
[]
[null,2364,3223,3418,3142,303,2451,3105,3171,2999,504]
[null,6.6159999999999997,7.0949999999999998,7.0590000000000002,6.915,1.3109999999999999,6.78,7.3339999999999996,7.26,6.9779999999999998,1.7989999999999999]
[null,8282,5287,5364,7442,1357,12269,7407,7800,10642,1355]
[null,3.7610000000000001,2.9470000000000001,3.012,4.3259999999999996,0.53,4.9279999999999999,3.7109999999999999,4.0780000000000003,5.8719999999999999,0.64900000000000002]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",2364,3223,3418,3142,303,2451,3105,3171,2999,504,24680]
[null,"Ann peak kW",6.6159999999999997,7.0949999999999998,7.0590000000000002,6.915,1.3109999999999999,6.78,7.3339999999999996,7.26,6.9779999999999998,1.7989999999999999,59.146999999999998]
[null,"EFLH Heating",357.31559854897222,454.26356589147287,484.20456155262787,454.37454808387565,231.12128146453091,361.50442477876106,423.37060267248432,436.77685950413223,429.77930639151623,280.15564202334633,"231-484",417.26545725057906]
["Cooling","Ann kWh",8282,5287,5364,7442,1357,12269,7407,7800,10642,1355,67205]
[null,"Ann peak kW",3.7610000000000001,2.9470000000000001,3.012,4.3259999999999996,0.53,4.9279999999999999,3.7109999999999999,4.0780000000000003,5.8719999999999999,0.64900000000000002,33.813999999999993]
[null,"EFLH Cooling",2202.073916511566,1794.0278249066848,1780.8764940239043,1720.2958853444293,2560.3773584905657,2489.6509740259739,1995.9579628132581,1912.7023050514956,1812.3297002724796,2087.8274268104774,"1720-2560",1987.4903885964397]
[]
["SCooper Htl 24 7days wo setback - Baseline Design.SIM"]
[null,2699,6.6130000000000004,8507,3.7610000000000001]
[null,3665,7.093,5386,2.9470000000000001]
[null,3844,7.056,5473,3.012]
[null,3476,6.9119999999999999,7613,4.3259999999999996]
[null,493,1.3129999999999999,1340,0.53]
[null,2564,6.7670000000000003,12744,4.9279999999999999]
[null,3468,7.3209999999999997,7570,3.7109999999999999]
[null,3498,7.2469999999999999,7993,4.0780000000000003]
[null,3182,6.9649999999999999,10966,5.8719999999999999]
[null,766,1.8129999999999999,1392,0.64900000000000002]
[]
[null,2699,3665,3844,3476,493,2564,3468,3498,3182,766]
[null,6.6130000000000004,7.093,7.056,6.9119999999999999,1.3129999999999999,6.7670000000000003,7.3209999999999997,7.2469999999999999,6.9649999999999999,1.8129999999999999]
[null,8507,5386,5473,7613,1340,12744,7570,7993,10966,1392]
[null,3.7610000000000001,2.9470000000000001,3.012,4.3259999999999996,0.53,4.9279999999999999,3.7109999999999999,4.0780000000000003,5.8719999999999999,0.64900000000000002]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",2699,3665,3844,3476,493,2564,3468,3498,3182,766,27655]
[null,"Ann peak kW",6.6130000000000004,7.093,7.056,6.9119999999999999,1.3129999999999999,6.7670000000000003,7.3209999999999997,7.2469999999999999,6.9649999999999999,1.8129999999999999,59.099999999999994]
[null,"EFLH Heating",408.13549070013607,516.70661215282678,544.78458049886626,502.89351851851853,375.47600913937549,378.89759125166245,473.70577789919412,482.68248930591972,456.85570710696339,422.50413678985109,"375-545",467.93570219966165]
["Cooling","Ann kWh",8507,5386,5473,7613,1340,12744,7570,7993,10966,1392,68984]
[null,"Ann peak kW",3.7610000000000001,2.9470000000000001,3.012,4.3259999999999996,0.53,4.9279999999999999,3.7109999999999999,4.0780000000000003,5.8719999999999999,0.64900000000000002,33.813999999999993]
[null,"EFLH Cooling",2261.8984312682796,1827.621309806583,1817.0650730411687,1759.8243180767454,2528.3018867924525,2586.0389610389611,2039.8814335758557,1960.0294261893084,1867.5068119891009,2144.8382126348229,"1760-2586",2040.1017330099962]
[]
[]
["SCooper Rtl 9-18 wo setback - Baseline Design.SIM"]
[null,2525,7.0259999999999998,16007,12.547000000000001]
[null,1309,2.8610000000000002,7501,5.0940000000000003]
[null,1341,4.3140000000000001,10607,8.6329999999999991]
[null,992,4.2629999999999999,12656,8.7129999999999992]
[null,1365,3.0190000000000001,5841,4.6740000000000004]
[null,2848,7.0289999999999999,20194,14.885]
[null,37,1.627,1615,1.6930000000000001]
[]
[]
[]
[]
[null,2525,1309,1341,992,1365,2848,37]
[null,7.0259999999999998,2.8610000000000002,4.3140000000000001,4.2629999999999999,3.0190000000000001,7.0289999999999999,1.627]
[null,16007,7501,10607,12656,5841,20194,1615]
[null,12.547000000000001,5.0940000000000003,8.6329999999999991,8.7129999999999992,4.6740000000000004,14.885,1.6930000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",2525,1309,1341,992,1365,2848,37,null,null,null,10417]
[null,"Ann peak kW",7.0259999999999998,2.8610000000000002,4.3140000000000001,4.2629999999999999,3.0190000000000001,7.0289999999999999,1.627,null,null,null,30.138999999999996]
[null,"EFLH Heating",359.37944776544265,457.53233135267385,310.84840055632822,232.69997654234109,452.13646902947994,405.17854602361643,22.741241548862938,"","","","23-458",345.63190550449588]
["Cooling","Ann kWh",16007,7501,10607,12656,5841,20194,1615,null,null,null,74421]
[null,"Ann peak kW",12.547000000000001,5.0940000000000003,8.6329999999999991,8.7129999999999992,4.6740000000000004,14.885,1.6930000000000001,null,null,null,56.238999999999997]
[null,"EFLH Cooling",1275.7631306288356,1472.516686297605,1228.657477122669,1452.5421783541835,1249.6790757381257,1356.6677863621096,953.92793857058473,"","","","954-1473",1323.2987784277816]
[]
["SCooper Rtl 8-20 wo setback - Baseline Design.SIM"]
[null,2208,6.8319999999999999,18977,13.090999999999999]
[null,1212,2.8149999999999999,8383,5.22]
[null,1175,4.2050000000000001,12728,9.0350000000000001]
[null,857,4.1539999999999999,14779,9.0289999999999999]
[null,1239,2.597,6684,4.8310000000000004]
[null,2657,7.0309999999999997,23192,16.132000000000001]
[null,126,1.81,2036,1.762]
[]
[]
[]
[]
[null,2208,1212,1175,857,1239,2657,126]
[null,6.8319999999999999,2.8149999999999999,4.2050000000000001,4.1539999999999999,2.597,7.0309999999999997,1.81]
[null,18977,8383,12728,14779,6684,23192,2036]
[null,13.090999999999999,5.22,9.0350000000000001,9.0289999999999999,4.8310000000000004,16.132000000000001,1.762]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",2208,1212,1175,857,1239,2657,126,null,null,null,9474]
[null,"Ann peak kW",6.8319999999999999,2.8149999999999999,4.2050000000000001,4.1539999999999999,2.597,7.0309999999999997,1.81,null,null,null,29.443999999999999]
[null,"EFLH Heating",323.18501170960189,430.55062166962699,279.4292508917955,206.30717380837748,477.08894878706201,377.89788081354004,69.613259668508292,"","","","70-477",321.7633473712811]
["Cooling","Ann kWh",18977,8383,12728,14779,6684,23192,2036,null,null,null,86779]
[null,"Ann peak kW",13.090999999999999,5.22,9.0350000000000001,9.0289999999999999,4.8310000000000004,16.132000000000001,1.762,null,null,null,59.100000000000009]
[null,"EFLH Cooling",1449.6218776258499,1605.9386973180078,1408.7437742114,1636.8368590098571,1383.5644794038501,1437.6394743367218,1155.5051078320091,"","","","1156-1637",1468.3417935702198]
[]
["SCooper Rtl 7-22 wo setback - Baseline Design.SIM"]
[null,1797,7.7649999999999997,21776,13.369]
[null,1078,2.99,9158,5.2759999999999998]
[null,916,4.609,14731,9.3140000000000001]
[null,710,4.4720000000000004,16738,9.2769999999999992]
[null,1072,3.3759999999999999,7462,4.8099999999999996]
[null,2214,7.1210000000000004,25968,16.675999999999998]
[null,131,1.873,2491,1.8069999999999999]
[]
[]
[]
[]
[null,1797,1078,916,710,1072,2214,131]
[null,7.7649999999999997,2.99,4.609,4.4720000000000004,3.3759999999999999,7.1210000000000004,1.873]
[null,21776,9158,14731,16738,7462,25968,2491]
[null,13.369,5.2759999999999998,9.3140000000000001,9.2769999999999992,4.8099999999999996,16.675999999999998,1.8069999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",1797,1078,916,710,1072,2214,131,null,null,null,7918]
[null,"Ann peak kW",7.7649999999999997,2.99,4.609,4.4720000000000004,3.3759999999999999,7.1210000000000004,1.873,null,null,null,32.205999999999996]
[null,"EFLH Heating",231.42305215711528,360.53511705685617,198.74159253634193,158.76565295169945,317.53554502369667,310.91138884988061,69.941270688734647,"","","","70-361",245.85480966279579]
["Cooling","Ann kWh",21776,9158,14731,16738,7462,25968,2491,null,null,null,98324]
[null,"Ann peak kW",13.369,5.2759999999999998,9.3140000000000001,9.2769999999999992,4.8099999999999996,16.675999999999998,1.8069999999999999,null,null,null,60.528999999999996]
[null,"EFLH Cooling",1628.8428453885856,1735.7846853677029,1581.5975950182522,1804.2470626280049,1551.3513513513515,1557.2079635404175,1378.5279468732706,"","","","1379-1804",1624.4114391448727]
[]
["SCooper Rtl 9-22 7days wo setback - Baseline Design.SIM"]
[null,1855,7.3070000000000004,21901,13.266999999999999]
[null,1023,2.956,9173,5.1219999999999999]
[null,936,4.2119999999999997,14860,9.2430000000000003]
[null,642,4.1710000000000003,16873,9.1120000000000001]
[null,1111,3.198,7553,4.79]
[null,2315,6.9119999999999999,26084,16.579000000000001]
[null,150,1.5820000000000001,2743,1.804]
[]
[]
[]
[]
[null,1855,1023,936,642,1111,2315,150]
[null,7.3070000000000004,2.956,4.2119999999999997,4.1710000000000003,3.198,6.9119999999999999,1.5820000000000001]
[null,21901,9173,14860,16873,7553,26084,2743]
[null,13.266999999999999,5.1219999999999999,9.2430000000000003,9.1120000000000001,4.79,16.579000000000001,1.804]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",1855,1023,936,642,1111,2315,150,null,null,null,8032]
[null,"Ann peak kW",7.3070000000000004,2.956,4.2119999999999997,4.1710000000000003,3.198,6.9119999999999999,1.5820000000000001,null,null,null,30.338000000000001]
[null,"EFLH Heating",253.8661557410702,346.07577807848446,222.22222222222223,153.919923279789,347.40462789243276,334.92476851851853,94.816687737041718,"","","","95-347",264.7504779484475]
["Cooling","Ann kWh",21901,9173,14860,16873,7553,26084,2743,null,null,null,99187]
[null,"Ann peak kW",13.266999999999999,5.1219999999999999,9.2430000000000003,9.1120000000000001,4.79,16.579000000000001,1.804,null,null,null,59.917000000000002]
[null,"EFLH Cooling",1650.7876686515415,1790.9019914096057,1607.7031266904685,1851.7339771729587,1576.8267223382045,1573.3156402678087,1520.509977827051,"","","","1521-1852",1655.4066458601064]
[]
["SCooper Rtl 8-22 7days wo setback - Baseline Design.SIM"]
[null,1354,16.367000000000001,24684,13.625]
[null,884,5.3819999999999997,9966,5.4829999999999997]
[null,622,10.603999999999999,16814,9.3330000000000002]
[null,436,10.426,18818,9.6080000000000005]
[null,909,5.9379999999999997,8320,4.798]
[null,1727,16.178000000000001,28760,16.597000000000001]
[null,141,1.839,3032,1.833]
[]
[]
[]
[]
[null,1354,884,622,436,909,1727,141]
[null,16.367000000000001,5.3819999999999997,10.603999999999999,10.426,5.9379999999999997,16.178000000000001,1.839]
[null,24684,9966,16814,18818,8320,28760,3032]
[null,13.625,5.4829999999999997,9.3330000000000002,9.6080000000000005,4.798,16.597000000000001,1.833]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",1354,884,622,436,909,1727,141,null,null,null,6073]
[null,"Ann peak kW",16.367000000000001,5.3819999999999997,10.603999999999999,10.426,5.9379999999999997,16.178000000000001,1.839,null,null,null,66.734000000000009]
[null,"EFLH Heating",82.727439359687168,164.2512077294686,58.657110524330449,41.818530596585461,153.08184573930617,106.74990728149338,76.672104404567705,"","","","42-164",91.003086882248923]
["Cooling","Ann kWh",24684,9966,16814,18818,8320,28760,3032,null,null,null,110394]
[null,"Ann peak kW",13.625,5.4829999999999997,9.3330000000000002,9.6080000000000005,4.798,16.597000000000001,1.833,null,null,null,61.277000000000008]
[null,"EFLH Cooling",1811.6697247706422,1817.6180922852454,1801.564341583628,1958.5761865112406,1734.0558566069196,1732.8432849310116,1654.1189307146753,"","","","1654-1959",1801.5568647290172]
[]
["SCooper Rtl 5-23 7days wo setback - Baseline Design.SIM"]
[null,824,9.7240000000000002,28890,13.45]
[null,643,3.4809999999999999,11152,5.3490000000000002]
[null,378,5.1710000000000003,19876,9.3759999999999994]
[null,319,5.1890000000000001,21771,9.48]
[null,644,4.1239999999999997,9565,4.8220000000000001]
[null,1052,8.6039999999999992,32904,16.797999999999998]
[null,133,1.9350000000000001,3842,1.823]
[]
[]
[]
[]
[null,824,643,378,319,644,1052,133]
[null,9.7240000000000002,3.4809999999999999,5.1710000000000003,5.1890000000000001,4.1239999999999997,8.6039999999999992,1.9350000000000001]
[null,28890,11152,19876,21771,9565,32904,3842]
[null,13.45,5.3490000000000002,9.3759999999999994,9.48,4.8220000000000001,16.797999999999998,1.823]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",824,643,378,319,644,1052,133,null,null,null,3993]
[null,"Ann peak kW",9.7240000000000002,3.4809999999999999,5.1710000000000003,5.1890000000000001,4.1239999999999997,8.6039999999999992,1.9350000000000001,null,null,null,38.228000000000002]
[null,"EFLH Heating",84.738790621143565,184.71703533467394,73.099980661380769,61.476199653112353,156.15906886517945,122.26871222687123,68.73385012919897,"","","","61-185",104.45223396463325]
["Cooling","Ann kWh",28890,11152,19876,21771,9565,32904,3842,null,null,null,128000]
[null,"Ann peak kW",13.45,5.3490000000000002,9.3759999999999994,9.48,4.8220000000000001,16.797999999999998,1.823,null,null,null,61.098000000000006]
[null,"EFLH Cooling",2147.9553903345727,2084.8756776967657,2119.8805460750855,2296.5189873417721,1983.6167565325591,1958.8046195975714,2107.5150850246846,"","","","1959-2297",2094.994926184163]
[]
["SCooper Rtl 24 7days wo setback - Baseline Design.SIM"]
[null,1855,7.3070000000000004,21901,13.266999999999999]
[null,1023,2.956,9173,5.1219999999999999]
[null,936,4.2119999999999997,14860,9.2430000000000003]
[null,642,4.1710000000000003,16873,9.1120000000000001]
[null,1111,3.198,7553,4.79]
[null,2315,6.9119999999999999,26084,16.579000000000001]
[null,150,1.5820000000000001,2743,1.804]
[]
[]
[]
[]
[null,1855,1023,936,642,1111,2315,150]
[null,7.3070000000000004,2.956,4.2119999999999997,4.1710000000000003,3.198,6.9119999999999999,1.5820000000000001]
[null,21901,9173,14860,16873,7553,26084,2743]
[null,13.266999999999999,5.1219999999999999,9.2430000000000003,9.1120000000000001,4.79,16.579000000000001,1.804]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",1855,1023,936,642,1111,2315,150,null,null,null,8032]
[null,"Ann peak kW",7.3070000000000004,2.956,4.2119999999999997,4.1710000000000003,3.198,6.9119999999999999,1.5820000000000001,null,null,null,30.338000000000001]
[null,"EFLH Heating",253.8661557410702,346.07577807848446,222.22222222222223,153.919923279789,347.40462789243276,334.92476851851853,94.816687737041718,"","","","95-347",264.7504779484475]
["Cooling","Ann kWh",21901,9173,14860,16873,7553,26084,2743,null,null,null,99187]
[null,"Ann peak kW",13.266999999999999,5.1219999999999999,9.2430000000000003,9.1120000000000001,4.79,16.579000000000001,1.804,null,null,null,59.917000000000002]
[null,"EFLH Cooling",1650.7876686515415,1790.9019914096057,1607.7031266904685,1851.7339771729587,1576.8267223382045,1573.3156402678087,1520.509977827051,"","","","1521-1852",1655.4066458601064]
[]
["SCooper Rtl 10-23 7day Hol1 wo setback - Baseline Design.SIM"]
[null,2534,7.0250000000000004,15986,12.548999999999999]
[null,1303,2.855,7503,5.125]
[null,1383,4.3239999999999998,10599,8.6329999999999991]
[null,1017,4.2750000000000004,12661,8.782]
[null,1378,2.6080000000000001,5828,4.6749999999999998]
[null,2892,7.0190000000000001,20136,14.882]
[null,101,1.6040000000000001,1555,1.6910000000000001]
[]
[]
[]
[]
[null,2534,1303,1383,1017,1378,2892,101]
[null,7.0250000000000004,2.855,4.3239999999999998,4.2750000000000004,2.6080000000000001,7.0190000000000001,1.6040000000000001]
[null,15986,7503,10599,12661,5828,20136,1555]
[null,12.548999999999999,5.125,8.6329999999999991,8.782,4.6749999999999998,14.882,1.6910000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",2534,1303,1383,1017,1378,2892,101,null,null,null,10608]
[null,"Ann peak kW",7.0250000000000004,2.855,4.3239999999999998,4.2750000000000004,2.6080000000000001,7.0190000000000001,1.6040000000000001,null,null,null,29.71]
[null,"EFLH Heating",360.71174377224196,456.39229422066552,319.84273820536544,237.89473684210523,528.37423312883436,412.02450491523007,62.967581047381543,"","","","63-528",357.05149781218444]
["Cooling","Ann kWh",15986,7503,10599,12661,5828,20136,1555,null,null,null,74268]
[null,"Ann peak kW",12.548999999999999,5.125,8.6329999999999991,8.782,4.6749999999999998,14.882,1.6910000000000001,null,null,null,56.336999999999996]
[null,"EFLH Cooling",1273.886365447446,1464,1227.7308004170047,1441.6989296287861,1246.6310160427809,1353.0439457062223,919.57421643997634,"","","","920-1464",1318.2810586293201]
[]
["SCooper Rtl 9-24 10-18 Hol2 wo setback - Baseline Design.SIM"]
[null,1354,16.367000000000001,24684,13.625]
[null,884,5.3819999999999997,9966,5.4829999999999997]
[null,622,10.603999999999999,16814,9.3330000000000002]
[null,436,10.426,18818,9.6080000000000005]
[null,909,5.9379999999999997,8320,4.798]
[null,1727,16.178000000000001,28760,16.597000000000001]
[null,141,1.839,3032,1.833]
[]
[]
[]
[]
[null,1354,884,622,436,909,1727,141]
[null,16.367000000000001,5.3819999999999997,10.603999999999999,10.426,5.9379999999999997,16.178000000000001,1.839]
[null,24684,9966,16814,18818,8320,28760,3032]
[null,13.625,5.4829999999999997,9.3330000000000002,9.6080000000000005,4.798,16.597000000000001,1.833]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",1354,884,622,436,909,1727,141,null,null,null,6073]
[null,"Ann peak kW",16.367000000000001,5.3819999999999997,10.603999999999999,10.426,5.9379999999999997,16.178000000000001,1.839,null,null,null,66.734000000000009]
[null,"EFLH Heating",82.727439359687168,164.2512077294686,58.657110524330449,41.818530596585461,153.08184573930617,106.74990728149338,76.672104404567705,"","","","42-164",91.003086882248923]
["Cooling","Ann kWh",24684,9966,16814,18818,8320,28760,3032,null,null,null,110394]
[null,"Ann peak kW",13.625,5.4829999999999997,9.3330000000000002,9.6080000000000005,4.798,16.597000000000001,1.833,null,null,null,61.277000000000008]
[null,"EFLH Cooling",1811.6697247706422,1817.6180922852454,1801.564341583628,1958.5761865112406,1734.0558566069196,1732.8432849310116,1654.1189307146753,"","","","1654-1959",1801.5568647290172]
[]
[]
[]
["SCooper Sch 7-16 wo setback - Baseline Design.SIM"]
[null,2604,19.015999999999998,46551,35.890999999999998]
[null,1908,10.587999999999999,18813,14.587999999999999]
[null,1657,15.106,27411,22.494]
[null,1573,14.56,28238,22.088000000000001]
[null,1918,11.305,18220,14.925000000000001]
[null,3604,23.856000000000002,46203,36.75]
[null,1290,133.14099999999999,123805,108.807]
[]
[]
[]
[]
[null,2604,1908,1657,1573,1918,3604,1290]
[null,19.015999999999998,10.587999999999999,15.106,14.56,11.305,23.856000000000002,133.14099999999999]
[null,46551,18813,27411,28238,18220,46203,123805]
[null,35.890999999999998,14.587999999999999,22.494,22.088000000000001,14.925000000000001,36.75,108.807]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",2604,1908,1657,1573,1918,3604,1290,null,null,null,14554]
[null,"Ann peak kW",19.015999999999998,10.587999999999999,15.106,14.56,11.305,23.856000000000002,133.14099999999999,null,null,null,227.572]
[null,"EFLH Heating",136.93731594446783,180.2040045334341,109.69151330597114,108.03571428571428,169.65944272445822,151.07310529845739,9.6889763483825426,"","","","10-180",63.953386181076759]
["Cooling","Ann kWh",46551,18813,27411,28238,18220,46203,123805,null,null,null,309241]
[null,"Ann peak kW",35.890999999999998,14.587999999999999,22.494,22.088000000000001,14.925000000000001,36.75,108.807,null,null,null,255.54300000000001]
[null,"EFLH Cooling",1297.0103925775265,1289.6216068001097,1218.5916244331822,1278.4317276349148,1220.7705192629815,1257.2244897959183,1137.8403962980324,"","","","1138-1297",1210.1329326179939]
[]
["SCooper Sch 6-20 wo setback - Baseline Design.SIM"]
[null,1854,17.986999999999998,57941,36.674999999999997]
[null,1469,9.9719999999999995,23282,14.752000000000001]
[null,1224,14.42,34426,22.789000000000001]
[null,1160,13.65,35226,22.388000000000002]
[null,1466,10.861000000000001,22708,15.095000000000001]
[null,2764,19.206,57936,38.887]
[null,772,74.195999999999998,162529,111.84399999999999]
[]
[]
[]
[]
[null,1854,1469,1224,1160,1466,2764,772]
[null,17.986999999999998,9.9719999999999995,14.42,13.65,10.861000000000001,19.206,74.195999999999998]
[null,57941,23282,34426,35226,22708,57936,162529]
[null,36.674999999999997,14.752000000000001,22.789000000000001,22.388000000000002,15.095000000000001,38.887,111.84399999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",1854,1469,1224,1160,1466,2764,772,null,null,null,10709]
[null,"Ann peak kW",17.986999999999998,9.9719999999999995,14.42,13.65,10.861000000000001,19.206,74.195999999999998,null,null,null,160.292]
[null,"EFLH Heating",103.07444265302719,147.31247492980344,84.882108183079055,84.981684981684978,134.97836295000459,143.91336040820576,10.404873578090463,"","","","10-147",66.809322985551361]
["Cooling","Ann kWh",57941,23282,34426,35226,22708,57936,162529,null,null,null,394048]
[null,"Ann peak kW",36.674999999999997,14.752000000000001,22.789000000000001,22.388000000000002,15.095000000000001,38.887,111.84399999999999,null,null,null,262.43]
[null,"EFLH Cooling",1579.8500340831631,1578.2266811279826,1510.6410987757251,1573.4321958191888,1504.3391851606491,1489.855221539332,1453.1758520796825,"","","","1453-1580",1501.5356476012651]
[]
["SCooper Sch 7-21 7days wo setback - Baseline Design.SIM"]
[null,3178,134.45099999999999,58996,36.552]
[null,2061,52.93,23776,14.712999999999999]
[null,2515,78.683999999999997,35186,22.722999999999999]
[null,2256,79.507999999999996,35984,22.321999999999999]
[null,2179,52.01,23207,15.053000000000001]
[null,4589,140.73400000000001,59090,38.780999999999999]
[null,3833,132.90700000000001,166889,111.31699999999999]
[]
[]
[]
[]
[null,3178,2061,2515,2256,2179,4589,3833]
[null,134.45099999999999,52.93,78.683999999999997,79.507999999999996,52.01,140.73400000000001,132.90700000000001]
[null,58996,23776,35186,35984,23207,59090,166889]
[null,36.552,14.712999999999999,22.722999999999999,22.321999999999999,15.053000000000001,38.780999999999999,111.31699999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",3178,2061,2515,2256,2179,4589,3833,null,null,null,20611]
[null,"Ann peak kW",134.45099999999999,52.93,78.683999999999997,79.507999999999996,52.01,140.73400000000001,132.90700000000001,null,null,null,671.22400000000005]
[null,"EFLH Heating",23.636863987623745,38.938220290950312,31.963296222866148,28.37450319464708,41.895789271293985,32.60761436468799,28.839714988676292,"","","","24-42",30.706589752452235]
["Cooling","Ann kWh",58996,23776,35186,35984,23207,59090,166889,null,null,null,403128]
[null,"Ann peak kW",36.552,14.712999999999999,22.722999999999999,22.321999999999999,15.053000000000001,38.780999999999999,111.31699999999999,null,null,null,261.46100000000001]
[null,"EFLH Cooling",1614.0293280805429,1615.9858628423844,1548.4751133213044,1612.0419317265478,1541.6860426493056,1523.6842783837446,1499.2229398923796,"","","","1499-1616",1541.8284180049795]
[]
["SCooper Sch 8-22 7days 12mths wo setback - Baseline Design.SIM"]
[null,2885,51.607999999999997,76569,41.051000000000002]
[null,2005,21.062999999999999,30797,16.404]
[null,2403,75.465999999999994,46211,25.571999999999999]
[null,2106,31.518999999999998,46964,24.939]
[null,2172,21.327999999999999,30290,16.927]
[null,4437,51.451000000000001,76518,42.889000000000003]
[null,3697,30.63,228971,127.48]
[]
[]
[]
[]
[null,2885,2005,2403,2106,2172,4437,3697]
[null,51.607999999999997,21.062999999999999,75.465999999999994,31.518999999999998,21.327999999999999,51.451000000000001,30.63]
[null,76569,30797,46211,46964,30290,76518,228971]
[null,41.051000000000002,16.404,25.571999999999999,24.939,16.927,42.889000000000003,127.48]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",2885,2005,2403,2106,2172,4437,3697,null,null,null,19705]
[null,"Ann peak kW",51.607999999999997,21.062999999999999,75.465999999999994,31.518999999999998,21.327999999999999,51.451000000000001,30.63,null,null,null,283.065]
[null,"EFLH Heating",55.902185707642232,95.190618620329488,31.84215408263324,66.816840635806983,101.83795948987247,86.237390915628467,120.69866144302971,"","","","32-121",69.612986416547443]
["Cooling","Ann kWh",76569,30797,46211,46964,30290,76518,228971,null,null,null,536320]
[null,"Ann peak kW",41.051000000000002,16.404,25.571999999999999,24.939,16.927,42.889000000000003,127.48,null,null,null,295.262]
[null,"EFLH Cooling",1865.2164380892061,1877.4079492806632,1807.0936962302519,1883.1548979510005,1789.4488095941397,1784.0938235911306,1796.1327267022277,"","","","1784-1883",1816.4206704553922]
[]
["SCooper Sch 5-23 7days 12 mths wo setback - Baseline Design.SIM"]
[null,3225,52.587000000000003,87817,41.767000000000003]
[null,2012,21.445,35187,16.654]
[null,2778,80.459999999999994,53111,26.015000000000001]
[null,2480,82.658000000000001,53840,25.352]
[null,2158,53.875,34704,17.198]
[null,4604,52.116999999999997,87849,43.61]
[null,4641,47.926000000000002,267154,130.56299999999999]
[]
[]
[]
[]
[null,3225,2012,2778,2480,2158,4604,4641]
[null,52.587000000000003,21.445,80.459999999999994,82.658000000000001,53.875,52.116999999999997,47.926000000000002]
[null,87817,35187,53111,53840,34704,87849,267154]
[null,41.767000000000003,16.654,26.015000000000001,25.352,17.198,43.61,130.56299999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",3225,2012,2778,2480,2158,4604,4641,null,null,null,21898]
[null,"Ann peak kW",52.587000000000003,21.445,80.459999999999994,82.658000000000001,53.875,52.116999999999997,47.926000000000002,null,null,null,391.06800000000004]
[null,"EFLH Heating",61.32694392150151,93.821403590580559,34.526472781506342,30.003145491059545,40.055684454756381,88.339697219717181,96.836790051329132,"","","","30-97",55.995376763120476]
["Cooling","Ann kWh",87817,35187,53111,53840,34704,87849,267154,null,null,null,619662]
[null,"Ann peak kW",41.767000000000003,16.654,26.015000000000001,25.352,17.198,43.61,130.56299999999999,null,null,null,301.15899999999999]
[null,"EFLH Cooling",2102.545071467905,2112.8257475681517,2041.5529502210263,2123.6983275481225,2017.9090591929294,2014.4232974088511,2046.1692822622031,"","","","2014-2124",2057.5908407186903]
[]
["SCooper Sch 24h 7days 12 mths wo setback - Baseline Design.SIM"]
[null,3521,50.03,104376,43.619]
[null,1983,20.346,41701,17.405000000000001]
[null,2843,30.513000000000002,63229,27.105]
[null,2648,30.414999999999999,63979,26.533000000000001]
[null,2118,20.43,41203,17.888999999999999]
[null,4830,49.786000000000001,104546,45.459000000000003]
[null,5448,31.914999999999999,325270,138.07]
[]
[]
[]
[]
[null,3521,1983,2843,2648,2118,4830,5448]
[null,50.03,20.346,30.513000000000002,30.414999999999999,20.43,49.786000000000001,31.914999999999999]
[null,104376,41701,63229,63979,41203,104546,325270]
[null,43.619,17.405000000000001,27.105,26.533000000000001,17.888999999999999,45.459000000000003,138.07]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann kWh",3521,1983,2843,2648,2118,4830,5448,null,null,null,23391]
[null,"Ann peak kW",50.03,20.346,30.513000000000002,30.414999999999999,20.43,49.786000000000001,31.914999999999999,null,null,null,233.435]
[null,"EFLH Heating",70.377773335998398,97.463874963137712,93.173401500999574,87.062304783823777,103.67107195301028,97.015225163700634,170.70343098856338,"","","","70-171",100.20348276822241]
["Cooling","Ann kWh",104376,41701,63229,63979,41203,104546,325270,null,null,null,744304]
[null,"Ann peak kW",43.619,17.405000000000001,27.105,26.533000000000001,17.888999999999999,45.459000000000003,138.07,null,null,null,316.08000000000004]
[null,"EFLH Cooling",2392.902175657397,2395.9207124389541,2332.7430363401586,2411.2991369238307,2303.2589859690315,2299.7866209111507,2355.8339972477729,"","","","2300-2411",2354.7962541128827]
[]
[]
["SCooper Tech Col 7-16 wo setback - Baseline Design.SIM"]
[null,235,14.654,71879,46.241]
[null,66,9.4009999999999998,26028,16.626999999999999]
[null,766,20.484000000000002,70758,48.616]
[null,64,12.683,25359,16.385999999999999]
[null,42,11.515000000000001,85985,58.85]
[null,337,39.472999999999999,155136,92.298000000000002]
[null,178,23.751000000000001,56885,33.676000000000002]
[null,794,52.716999999999999,153087,100.464]
[null,139,24.72,55591,33.633000000000003]
[null,245,49.470999999999997,184616,118.35599999999999]
[null,1711,25.001999999999999,78444,48.048000000000002]
[null,399,13.250999999999999,28558,17.443999999999999]
[null,2816,31.376000000000001,77801,51.713999999999999]
[null,364,12.321,27889,17.314]
[null,520,47.695999999999998,93365,64.113]
[]
[null,235,66,766,64,42,337,178,794,139,245,1711,399,2816,364,520]
[null,14.654,9.4009999999999998,20.484000000000002,12.683,11.515000000000001,39.472999999999999,23.751000000000001,52.716999999999999,24.72,49.470999999999997,25.001999999999999,13.250999999999999,31.376000000000001,12.321,47.695999999999998]
[null,71879,26028,70758,25359,85985,155136,56885,153087,55591,184616,78444,28558,77801,27889,93365]
[null,46.241,16.626999999999999,48.616,16.385999999999999,58.85,92.298000000000002,33.676000000000002,100.464,33.633000000000003,118.35599999999999,48.048000000000002,17.443999999999999,51.713999999999999,17.314,64.113]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann kWh",235,66,766,64,42,337,178,794,139,245,1711,399,2816,364,520,8676]
[null,"Ann peak kW",14.654,9.4009999999999998,20.484000000000002,12.683,11.515000000000001,39.472999999999999,23.751000000000001,52.716999999999999,24.72,49.470999999999997,25.001999999999999,13.250999999999999,31.376000000000001,12.321,47.695999999999998,388.51499999999999]
[null,"EFLH Heating",16.036577043810563,7.0205297308796935,37.395040031243894,5.0461247338957662,3.6474164133738598,8.5374813163428165,7.4944212875247356,15.061555096079063,5.6229773462783177,4.9523963534191751,68.434525237980964,30.110935023771791,89.750127485976535,29.543056570083596,10.902381751090239,"4-90",22.331184124165091]
["Cooling","Ann kWh",71879,26028,70758,25359,85985,155136,56885,153087,55591,184616,78444,28558,77801,27889,93365,1191381]
[null,"Ann peak kW",46.241,16.626999999999999,48.616,16.385999999999999,58.85,92.298000000000002,33.676000000000002,100.464,33.633000000000003,118.35599999999999,48.048000000000002,17.443999999999999,51.713999999999999,17.314,64.113,763.77999999999975]
[null,"EFLH Cooling",1554.4430267511516,1565.4056654838516,1455.4467664966267,1547.6016111314539,1461.0875106202209,1680.8164857310016,1689.1851763867442,1523.7995699952221,1652.8706924746527,1559.8364256987395,1632.6173826173826,1637.124512726439,1504.44753838419,1610.7774055677487,1456.2569213732004,"1455-1689",1559.8483856607929]
[]
["SCooper Tech Col 6-20 wo setback - Baseline Design.SIM"]
[null,123,13.624000000000001,91580,47.155000000000001]
[null,54,7.6369999999999996,32507,16.393999999999998]
[null,555,15.711,90484,50.173000000000002]
[null,49,7.6319999999999997,32152,17.846]
[null,36,12.029,116305,60.052999999999997]
[null,239,32.491,196330,96.353999999999999]
[null,143,17.385999999999999,70369,34.542000000000002]
[null,545,36.484000000000002,194585,103.03400000000001]
[null,120,16.559999999999999,69590,36.465000000000003]
[null,205,31.715,251556,122.946]
[null,1367,20.984000000000002,98899,50.896000000000001]
[null,317,9.6280000000000001,35337,18.187000000000001]
[null,2296,24.164999999999999,98432,54.097000000000001]
[null,256,10.08,34935,19.079999999999998]
[null,407,36.326999999999998,126930,68.679000000000002]
[]
[null,123,54,555,49,36,239,143,545,120,205,1367,317,2296,256,407]
[null,13.624000000000001,7.6369999999999996,15.711,7.6319999999999997,12.029,32.491,17.385999999999999,36.484000000000002,16.559999999999999,31.715,20.984000000000002,9.6280000000000001,24.164999999999999,10.08,36.326999999999998]
[null,91580,32507,90484,32152,116305,196330,70369,194585,69590,251556,98899,35337,98432,34935,126930]
[null,47.155000000000001,16.393999999999998,50.173000000000002,17.846,60.052999999999997,96.353999999999999,34.542000000000002,103.03400000000001,36.465000000000003,122.946,50.896000000000001,18.187000000000001,54.097000000000001,19.079999999999998,68.679000000000002]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann kWh",123,54,555,49,36,239,143,545,120,205,1367,317,2296,256,407,6712]
[null,"Ann peak kW",13.624000000000001,7.6369999999999996,15.711,7.6319999999999997,12.029,32.491,17.385999999999999,36.484000000000002,16.559999999999999,31.715,20.984000000000002,9.6280000000000001,24.164999999999999,10.08,36.326999999999998,292.45300000000003]
[null,"EFLH Heating",9.0281855549031125,7.0708393348173368,35.325568073324419,6.4203354297693922,2.9927674785933993,7.3558831676464251,8.2250086276314285,14.9380550378248,7.2463768115942031,6.4638183824688635,65.144872283644673,32.92480265891151,95.013449203393336,25.396825396825395,11.203787816224848,"3-95",22.950696351208567]
["Cooling","Ann kWh",91580,32507,90484,32152,116305,196330,70369,194585,69590,251556,98899,35337,98432,34935,126930,1539991]
[null,"Ann peak kW",47.155000000000001,16.393999999999998,50.173000000000002,17.846,60.052999999999997,96.353999999999999,34.542000000000002,103.03400000000001,36.465000000000003,122.946,50.896000000000001,18.187000000000001,54.097000000000001,19.079999999999998,68.679000000000002,795.90100000000007]
[null,"EFLH Cooling",1942.1058212278656,1982.8595827741858,1803.4400972634683,1801.6362210019051,1936.7059097796946,2037.590551507981,2037.2010885299055,1888.5513519808994,1908.4053201700258,2046.0690059050314,1943.1585979251806,1942.9812503436519,1819.5463704087103,1830.9748427672957,1848.1631939894289,"1802-2046",1934.9027077488279]
[]
["SCooper Tech Col 9-21 7days wo setback - Baseline Design.SIM"]
[null,792,17.696000000000002,84219,46.488]
[null,657,6.7119999999999997,30043,16.257000000000001]
[null,1935,46.290999999999997,83869,49.862000000000002]
[null,680,17.754999999999999,29711,17.736000000000001]
[null,405,13.547000000000001,109420,58.847000000000001]
[null,1335,35.195,180668,94.659000000000006]
[null,1179,14.901999999999999,64973,34.072000000000003]
[null,3609,61.61,179872,102.351]
[null,1381,28.515999999999998,64123,36.090000000000003]
[null,1759,33.058999999999997,234436,120.42100000000001]
[null,2377,34.109000000000002,91253,49.951999999999998]
[null,1090,14.583,32821,17.98]
[null,4369,49.213000000000001,91229,53.808999999999997]
[null,1259,18.739000000000001,32387,18.905999999999999]
[null,4174,42.265999999999998,119446,67.507000000000005]
[]
[null,792,657,1935,680,405,1335,1179,3609,1381,1759,2377,1090,4369,1259,4174]
[null,17.696000000000002,6.7119999999999997,46.290999999999997,17.754999999999999,13.547000000000001,35.195,14.901999999999999,61.61,28.515999999999998,33.058999999999997,34.109000000000002,14.583,49.213000000000001,18.739000000000001,42.265999999999998]
[null,84219,30043,83869,29711,109420,180668,64973,179872,64123,234436,91253,32821,91229,32387,119446]
[null,46.488,16.257000000000001,49.862000000000002,17.736000000000001,58.847000000000001,94.659000000000006,34.072000000000003,102.351,36.090000000000003,120.42100000000001,49.951999999999998,17.98,53.808999999999997,18.905999999999999,67.507000000000005]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann kWh",792,657,1935,680,405,1335,1179,3609,1381,1759,2377,1090,4369,1259,4174,27001]
[null,"Ann peak kW",17.696000000000002,6.7119999999999997,46.290999999999997,17.754999999999999,13.547000000000001,35.195,14.901999999999999,61.61,28.515999999999998,33.058999999999997,34.109000000000002,14.583,49.213000000000001,18.739000000000001,42.265999999999998,434.19299999999998]
[null,"EFLH Heating",44.755877034358043,97.884386174016697,41.800782009461884,38.29907068431428,29.895917915405622,37.931524364256283,79.116897060797214,58.578152897256942,48.428952167204379,53.207901025439369,69.688352047846607,74.744565590070636,88.77735557677849,67.186082501734347,98.755500875408131,"30-99",62.186631290693313]
["Cooling","Ann kWh",84219,30043,83869,29711,109420,180668,64973,179872,64123,234436,91253,32821,91229,32387,119446,1428470]
[null,"Ann peak kW",46.488,16.257000000000001,49.862000000000002,17.736000000000001,58.847000000000001,94.659000000000006,34.072000000000003,102.351,36.090000000000003,120.42100000000001,49.951999999999998,17.98,53.808999999999997,18.905999999999999,67.507000000000005,784.9369999999999]
[null,"EFLH Cooling",1811.6288074341767,1848.0039367657007,1682.0223817736953,1675.1804239963915,1859.3981001580369,1908.6193600185929,1906.9323784926037,1757.403445007865,1776.7525630368521,1946.8032984280148,1826.8137411915438,1825.4171301446052,1695.4226988050327,1713.0540569131495,1769.3868783977957,"1675-1947",1819.8530582709188]
[]
["SCooper Tech Col 8-22 7days wo setback - Baseline Design.SIM"]
[null,1095,53.956000000000003,92442,47.328000000000003]
[null,838,19.794,32742,16.504000000000001]
[null,2233,57.223999999999997,92054,50.826000000000001]
[null,869,20.398,32396,18.004999999999999]
[null,408,13.519,122371,60.256]
[null,2065,62.81,198046,96.561000000000007]
[null,1551,34.923999999999999,70529,34.496000000000002]
[null,4412,83.33,197148,104.166]
[null,1759,34.040999999999997,69691,36.649000000000001]
[null,1347,35.585000000000001,262639,122.745]
[null,2681,64.5,99828,50.871000000000002]
[null,1315,23.481000000000002,35620,18.146000000000001]
[null,4620,66.816000000000003,99691,54.680999999999997]
[null,1484,23.678000000000001,35181,19.175000000000001]
[null,4686,49.298999999999999,133729,68.475999999999999]
[]
[null,1095,838,2233,869,408,2065,1551,4412,1759,1347,2681,1315,4620,1484,4686]
[null,53.956000000000003,19.794,57.223999999999997,20.398,13.519,62.81,34.923999999999999,83.33,34.040999999999997,35.585000000000001,64.5,23.481000000000002,66.816000000000003,23.678000000000001,49.298999999999999]
[null,92442,32742,92054,32396,122371,198046,70529,197148,69691,262639,99828,35620,99691,35181,133729]
[null,47.328000000000003,16.504000000000001,50.826000000000001,18.004999999999999,60.256,96.561000000000007,34.496000000000002,104.166,36.649000000000001,122.745,50.871000000000002,18.146000000000001,54.680999999999997,19.175000000000001,68.475999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann kWh",1095,838,2233,869,408,2065,1551,4412,1759,1347,2681,1315,4620,1484,4686,31363]
[null,"Ann peak kW",53.956000000000003,19.794,57.223999999999997,20.398,13.519,62.81,34.923999999999999,83.33,34.040999999999997,35.585000000000001,64.5,23.481000000000002,66.816000000000003,23.678000000000001,49.298999999999999,643.3549999999999]
[null,"EFLH Heating",20.294313885388092,42.336061432757397,39.022088634139521,42.602215903519955,30.179747022708781,32.876930425091544,44.410720421486658,52.94611784471379,51.672982579830212,37.853027961219617,41.565891472868216,56.002725607938331,69.145114942528735,62.67421234901596,95.052637984543296,"20-95",48.749135391813233]
["Cooling","Ann kWh",92442,32742,92054,32396,122371,198046,70529,197148,69691,262639,99828,35620,99691,35181,133729,1574107]
[null,"Ann peak kW",47.328000000000003,16.504000000000001,50.826000000000001,18.004999999999999,60.256,96.561000000000007,34.496000000000002,104.166,36.649000000000001,122.745,50.871000000000002,18.146000000000001,54.680999999999997,19.175000000000001,68.475999999999999,798.88499999999999]
[null,"EFLH Cooling",1953.2200811359025,1983.882695104217,1811.1596427025538,1799.2779783393503,2030.8516994158258,2050.9936723936162,2044.5558905380333,1892.6329128506422,1901.5798521105623,2139.7124119108721,1962.3754201804563,1962.9670450788051,1823.1378358113423,1834.7327249022164,1952.9324142765349,"1799-2140",1970.3799670791166]
[]
["SCooper Tech Col 5-23 7days wo setback - Baseline Design.SIM"]
[null,1749,33.168999999999997,106859,48.488]
[null,1221,15.196,37408,16.867000000000001]
[null,3031,56.978999999999999,106336,52.012]
[null,1228,15.815,37068,18.350000000000001]
[null,243,11.988,146152,61.793999999999997]
[null,3686,43.085999999999999,228534,98.938999999999993]
[null,2349,21.934999999999999,80324,35.17]
[null,6268,55.720999999999997,227419,106.608]
[null,2448,22.039000000000001,79481,37.398000000000003]
[null,592,28.638000000000002,314607,125.55800000000001]
[null,3491,43.996000000000002,115013,52.000999999999998]
[null,1812,20.824999999999999,40543,18.465]
[null,5388,60.823999999999998,114773,55.841000000000001]
[null,1955,19.559999999999999,40112,19.530999999999999]
[null,5560,26.954000000000001,159959,69.453999999999994]
[]
[null,1749,1221,3031,1228,243,3686,2349,6268,2448,592,3491,1812,5388,1955,5560]
[null,33.168999999999997,15.196,56.978999999999999,15.815,11.988,43.085999999999999,21.934999999999999,55.720999999999997,22.039000000000001,28.638000000000002,43.996000000000002,20.824999999999999,60.823999999999998,19.559999999999999,26.954000000000001]
[null,106859,37408,106336,37068,146152,228534,80324,227419,79481,314607,115013,40543,114773,40112,159959]
[null,48.488,16.867000000000001,52.012,18.350000000000001,61.793999999999997,98.938999999999993,35.17,106.608,37.398000000000003,125.55800000000001,52.000999999999998,18.465,55.841000000000001,19.530999999999999,69.453999999999994]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann kWh",1749,1221,3031,1228,243,3686,2349,6268,2448,592,3491,1812,5388,1955,5560,41021]
[null,"Ann peak kW",33.168999999999997,15.196,56.978999999999999,15.815,11.988,43.085999999999999,21.934999999999999,55.720999999999997,22.039000000000001,28.638000000000002,43.996000000000002,20.824999999999999,60.823999999999998,19.559999999999999,26.954000000000001,476.72499999999997]
[null,"EFLH Heating",52.729958696373124,80.350092129507772,53.195036767932045,77.647802718937726,20.27027027027027,85.549830571415313,107.08912696603602,112.48900773496528,111.07582013702981,20.671834625322997,79.348122556596053,87.010804321728699,88.583453899776401,99.948875255623733,206.27736143058544,"20-206",86.047511668152509]
["Cooling","Ann kWh",106859,37408,106336,37068,146152,228534,80324,227419,79481,314607,115013,40543,114773,40112,159959,1834588]
[null,"Ann peak kW",48.488,16.867000000000001,52.012,18.350000000000001,61.793999999999997,98.938999999999993,35.17,106.608,37.398000000000003,125.55800000000001,52.000999999999998,18.465,55.841000000000001,19.530999999999999,69.453999999999994,816.476]
[null,"EFLH Cooling",2203.8236264642796,2217.8217821782177,2044.4512804737369,2020.0544959128065,2365.1487199404473,2309.8474817817041,2283.878305373898,2133.2263995197359,2125.2740788277447,2505.6706860574395,2211.7459279629238,2195.6674790143516,2055.3535932379432,2053.7606881368083,2303.0926944452444,"2020-2506",2246.958881828737]
[]
["SCooper Tech Col 24h 7days wo setback - Baseline Design.SIM"]
[null,2286,18.289000000000001,132638,51.241999999999997]
[null,1475,10.384,45958,17.859000000000002]
[null,3489,27.847999999999999,131998,54.780999999999999]
[null,1475,10.840999999999999,45638,19.288]
[null,58,7.4829999999999997,186793,66.242999999999995]
[null,5060,33.024999999999999,281886,104.361]
[null,3063,16.937999999999999,98187,37.110999999999997]
[null,8006,40.433,280955,112.095]
[null,3052,17.783999999999999,97360,39.253]
[null,0,0,403828,133.977]
[null,4293,34.478999999999999,142094,54.677]
[null,2156,14.409000000000001,49509,19.460999999999999]
[null,6108,42.985999999999997,141776,58.548999999999999]
[null,2276,14.584,49102,20.448]
[null,6302,19.068000000000001,204963,73.975999999999999]
[]
[null,2286,1475,3489,1475,58,5060,3063,8006,3052,0,4293,2156,6108,2276,6302]
[null,18.289000000000001,10.384,27.847999999999999,10.840999999999999,7.4829999999999997,33.024999999999999,16.937999999999999,40.433,17.783999999999999,0,34.478999999999999,14.409000000000001,42.985999999999997,14.584,19.068000000000001]
[null,132638,45958,131998,45638,186793,281886,98187,280955,97360,403828,142094,49509,141776,49102,204963]
[null,51.241999999999997,17.859000000000002,54.780999999999999,19.288,66.242999999999995,104.361,37.110999999999997,112.095,39.253,133.977,54.677,19.460999999999999,58.548999999999999,20.448,73.975999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann kWh",2286,1475,3489,1475,58,5060,3063,8006,3052,0,4293,2156,6108,2276,6302,49099]
[null,"Ann peak kW",18.289000000000001,10.384,27.847999999999999,10.840999999999999,7.4829999999999997,33.024999999999999,16.937999999999999,40.433,17.783999999999999,0,34.478999999999999,14.409000000000001,42.985999999999997,14.584,19.068000000000001,308.55099999999999]
[null,"EFLH Heating",124.99316529061183,142.04545454545453,125.28727377190462,136.0575592657504,7.7509020446345049,153.21725965177896,180.83599008147362,198.00657878465609,171.61493477282951,"",124.51057165231011,149.62870428204593,142.0927743916624,156.06143719144268,330.50136354101107,"8-331",159.1276644703793]
["Cooling","Ann kWh",132638,45958,131998,45638,186793,281886,98187,280955,97360,403828,142094,49509,141776,49102,204963,2292685]
[null,"Ann peak kW",51.241999999999997,17.859000000000002,54.780999999999999,19.288,66.242999999999995,104.361,37.110999999999997,112.095,39.253,133.977,54.677,19.460999999999999,58.548999999999999,20.448,73.975999999999999,863.32100000000003]
[null,"EFLH Cooling",2588.4625892822296,2573.3803684416816,2409.558058450923,2366.1343840729987,2819.8149238410097,2701.0664903555926,2645.7654064832532,2506.4008207324146,2480.3199755432706,3014.1591467192129,2598.78925325091,2544.0110991213196,2421.4931083366068,2401.3106416275432,2770.6688655780254,"2366-3014",2655.6576290858206]

{"sheet":"C&HLH","index":1,"n_rows":2713,"n_cols":31,"rows_kept":2713,"cut":false,"hidden":true,"merged":[[1383,0,1385,0],[1310,0,1312,0],[1313,0,1315,0],[1344,0,1344,1],[1345,0,1347,0],[1352,0,1352,19],[961,0,963,0],[987,0,987,1],[988,0,990,0],[991,0,993,0],[965,0,965,13],[996,0,996,13],[1348,0,1350,0],[1379,0,1379,1],[1380,0,1382,0],[1018,0,1018,1],[1019,0,1021,0],[1022,0,1024,0],[1204,0,1204,1],[1026,0,1026,13],[1079,0,1081,0],[1082,0,1084,0],[1146,0,1146,13],[1168,0,1168,1],[811,0,813,0],[837,0,837,1],[838,0,840,0],[841,0,843,0],[935,0,935,13],[928,0,930,0],[931,0,933,0],[748,0,750,0],[751,0,753,0],[777,0,777,1],[755,0,755,13],[785,0,785,13],[815,0,815,13],[778,0,780,0],[781,0,783,0],[807,0,807,1],[808,0,810,0],[897,0,897,1],[898,0,900,0],[901,0,903,0],[927,0,927,1],[867,0,867,1],[868,0,870,0],[871,0,873,0],[957,0,957,1],[845,0,845,13],[875,0,875,13],[905,0,905,13],[1112,0,1114,0],[1138,0,1138,1],[1139,0,1141,0],[1142,0,1144,0],[958,0,960,0],[1056,0,1056,13],[1086,0,1086,13],[1116,0,1116,13],[1169,0,1171,0],[1172,0,1174,0],[1177,0,1177,19],[1108,0,1108,1],[1109,0,1111,0],[1048,0,1048,1],[1049,0,1051,0],[1052,0,1054,0],[1078,0,1078,1],[1247,0,1247,19],[1282,0,1282,19],[1317,0,1317,19],[1212,0,1212,19],[1239,0,1239,1],[1240,0,1242,0],[1243,0,1245,0],[1205,0,1207,0],[1208,0,1210,0],[1274,0,1274,1],[1275,0,1277,0],[1278,0,1280,0],[1309,0,1309,1],[725,0,725,13],[687,0,689,0],[690,0,692,0],[716,0,716,1],[717,0,719,0],[656,0,656,1],[747,0,747,1],[604,0,604,13],[626,0,626,1],[627,0,629,0],[630,0,632,0],[660,0,662,0],[686,0,686,1],[720,0,722,0],[634,0,634,13],[664,0,664,13],[694,0,694,13],[657,0,659,0],[570,0,572,0],[574,0,574,13],[596,0,596,1],[597,0,599,0],[600,0,602,0],[509,0,511,0],[513,0,513,13],[535,0,535,1],[453,0,453,13],[475,0,475,1],[476,0,478,0],[479,0,481,0],[483,0,483,13],[536,0,538,0],[539,0,541,0],[544,0,544,13],[566,0,566,1],[567,0,569,0],[446,0,448,0],[449,0,451,0],[0,0,0,13],[386,0,388,0],[389,0,391,0],[393,0,393,13],[415,0,415,1],[505,0,505,1],[506,0,508,0],[416,0,418,0],[355,0,355,1],[356,0,358,0],[359,0,361,0],[363,0,363,13],[385,0,385,1],[419,0,421,0],[423,0,423,13],[445,0,445,1],[205,0,207,0],[144,0,144,1],[145,0,147,0],[148,0,150,0],[152,0,152,13],[174,0,174,1],[0,17,0,30],[22,17,22,18],[23,17,25,17],[26,17,28,17],[273,0,273,13],[295,0,295,1],[242,0,242,13],[264,0,264,1],[265,0,267,0],[268,0,270,0],[62,0,62,13],[84,0,84,1],[85,0,87,0],[30,0,30,13],[52,0,52,1],[53,0,55,0],[22,0,22,1],[23,0,25,0],[26,0,28,0],[60,0,60,14],[56,0,58,0],[88,0,90,0],[182,0,182,13],[204,0,204,1],[92,0,92,13],[175,0,177,0],[178,0,180,0],[114,0,114,1],[115,0,117,0],[118,0,120,0],[122,0,122,13],[1449,0,1449,13],[1471,0,1471,1],[1411,0,1411,1],[1412,0,1414,0],[1415,0,1417,0],[1441,0,1441,1],[208,0,210,0],[212,0,212,13],[234,0,234,1],[235,0,237,0],[238,0,240,0],[1389,0,1389,13],[1419,0,1419,13],[326,0,328,0],[329,0,331,0],[333,0,333,13],[296,0,298,0],[299,0,301,0],[303,0,303,13],[325,0,325,1],[1562,0,1564,0],[1565,0,1567,0],[1539,0,1539,13],[1591,0,1591,1],[1600,0,1600,13],[1622,0,1622,1],[1442,0,1444,0],[1445,0,1447,0],[1592,0,1594,0],[1595,0,1597,0],[1569,0,1569,13],[1531,0,1531,1],[1532,0,1534,0],[1535,0,1537,0],[1509,0,1509,13],[1561,0,1561,1],[1472,0,1474,0],[1475,0,1477,0],[1479,0,1479,13],[1501,0,1501,1],[1502,0,1504,0],[1505,0,1507,0],[1660,0,1660,13],[1682,0,1682,1],[1683,0,1685,0],[1686,0,1688,0],[1690,0,1690,13],[1712,0,1712,1],[1623,0,1625,0],[1626,0,1628,0],[1630,0,1630,13],[1652,0,1652,1],[1653,0,1655,0],[1656,0,1658,0],[1750,0,1750,13],[1772,0,1772,1],[1773,0,1775,0],[1776,0,1778,0],[1780,0,1780,13],[1802,0,1802,1],[1713,0,1715,0],[1716,0,1718,0],[1720,0,1720,13],[1742,0,1742,1],[1743,0,1745,0],[1746,0,1748,0],[1840,0,1840,13],[1862,0,1862,1],[1863,0,1865,0],[1866,0,1868,0],[1871,0,1871,13],[1893,0,1893,1],[1803,0,1805,0],[1806,0,1808,0],[1810,0,1810,13],[1832,0,1832,1],[1833,0,1835,0],[1836,0,1838,0],[1931,0,1931,13],[1953,0,1953,1],[1954,0,1956,0],[1957,0,1959,0],[1961,0,1961,13],[1983,0,1983,1],[1894,0,1896,0],[1897,0,1899,0],[1901,0,1901,13],[1923,0,1923,1],[1924,0,1926,0],[1927,0,1929,0],[2021,0,2021,13],[2043,0,2043,1],[2044,0,2046,0],[2047,0,2049,0],[2052,0,2052,13],[2074,0,2074,1],[1984,0,1986,0],[1987,0,1989,0],[1991,0,1991,13],[2013,0,2013,1],[2014,0,2016,0],[2017,0,2019,0],[2112,0,2112,13],[2134,0,2134,1],[2135,0,2137,0],[2138,0,2140,0],[2142,0,2142,13],[2164,0,2164,1],[2075,0,2077,0],[2078,0,2080,0],[2082,0,2082,13],[2104,0,2104,1],[2105,0,2107,0],[2108,0,2110,0],[2202,0,2202,13],[2224,0,2224,1],[2225,0,2227,0],[2228,0,2230,0],[2232,0,2232,13],[2254,0,2254,1],[2165,0,2167,0],[2168,0,2170,0],[2172,0,2172,13],[2194,0,2194,1],[2195,0,2197,0],[2198,0,2200,0],[2292,0,2292,13],[2314,0,2314,1],[2315,0,2317,0],[2318,0,2320,0],[2323,0,2323,13],[2345,0,2345,1],[2255,0,2257,0],[2258,0,2260,0],[2262,0,2262,13],[2284,0,2284,1],[2285,0,2287,0],[2288,0,2290,0],[2383,0,2383,13],[2405,0,2405,1],[2406,0,2408,0],[2409,0,2411,0],[2413,0,2413,13],[2435,0,2435,1],[2346,0,2348,0],[2349,0,2351,0],[2353,0,2353,13],[2375,0,2375,1],[2376,0,2378,0],[2379,0,2381,0],[2473,0,2473,13],[2495,0,2495,1],[2496,0,2498,0],[2499,0,2501,0],[2504,0,2504,19],[2531,0,2531,1],[2436,0,2438,0],[2439,0,2441,0],[2443,0,2443,13],[2465,0,2465,1],[2466,0,2468,0],[2469,0,2471,0],[2574,0,2574,19],[2601,0,2601,1],[2602,0,2604,0],[2605,0,2607,0],[2609,0,2609,19],[2636,0,2636,1],[2532,0,2534,0],[2535,0,2537,0],[2539,0,2539,19],[2566,0,2566,1],[2567,0,2569,0],[2570,0,2572,0],[2679,0,2679,19],[2706,0,2706,1],[2707,0,2709,0],[2710,0,2712,0],[2637,0,2639,0],[2640,0,2642,0],[2644,0,2644,19],[2671,0,2671,1],[2672,0,2674,0],[2675,0,2677,0]]}
["Scooper Office 8-17 wo setback intermittent",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"C&HLH Template"]
[null,-0.70099999999999996,-11.288,67.998000000000005,35.576999999999998]
[null,-10.156000000000001,-25.245999999999999,144.804,92.097999999999999]
[null,-3.2869999999999999,-10.808999999999999,47.63,28.635000000000002]
[null,-9.9139999999999997,-25.725999999999999,137.32400000000001,91.262]
[null,0,0,123.913,96.67]
[null,-1.841,-14.468,74.665000000000006,37.527999999999999]
[null,-13.013999999999999,-33.887,159.80799999999999,95.855000000000004]
[null,-3.98,-13.564,54.759,31.553999999999998]
[null,-12.523,-34.128999999999998,152.62100000000001,96.754999999999995]
[null,0,0,144.87899999999999,118.282]
[]
[null,-0.70099999999999996,-10.156000000000001,-3.2869999999999999,-9.9139999999999997,0,-1.841,-13.013999999999999,-3.98,-12.523,0]
[null,-11.288,-25.245999999999999,-10.808999999999999,-25.725999999999999,0,-14.468,-33.887,-13.564,-34.128999999999998,0]
[null,67.998000000000005,144.804,47.63,137.32400000000001,123.913,74.665000000000006,159.80799999999999,54.759,152.62100000000001,144.87899999999999]
[null,35.576999999999998,92.097999999999999,28.635000000000002,91.262,96.67,37.527999999999999,95.855000000000004,31.553999999999998,96.754999999999995,118.282]
[]
[null,"=-701","=-10156","=-3287","=-9914","=0","=-1841","=-13014","=-3980","=-12523","=0",null,null,null,null,null,null,null,"=0","=0","=0","=0","=0","=0","=0","=0","=0","=0"]
[null,-11.288,-25.245999999999999,-10.808999999999999,-25.725999999999999,0,-14.468,-33.887,-13.564,-34.128999999999998,0,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0]
[null,"=67998","=144804","=47630","=137324","=123913","=74665","=159808","=54759","=152621","=144879",null,null,null,null,null,null,null,"=0","=0","=0","=0","=0","=0","=0","=0","=0","=0"]
[null,35.576999999999998,92.097999999999999,28.635000000000002,91.262,96.67,37.527999999999999,95.855000000000004,31.553999999999998,96.754999999999995,118.282,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total",null,null,null,null,null,null,"SYS18","SYS19","SYS20","SYS21","SYS22","SYS23","SYS24","SYS25","SYS26","SYS27","Total"]
["Heating","Ann Heat Energy kBtu",-701,-10156,-3287,-9914,0,-1841,-13014,-3980,-12523,0,-55416,null,null,null,null,"Heating","Ann Heat Energy kBtu",null,null,null,null,null,null,null,null,null,null,0]
[null,"Ann peak Heating load kBtu/hr",-11.288,-25.245999999999999,-10.808999999999999,-25.725999999999999,0,-14.468,-33.887,-13.564,-34.128999999999998,0,-169.11699999999999,null,null,null,null,null,"Ann peak Heating load kBtu/hr",null,null,null,null,null,null,null,null,null,null,0]
[null,"HLH",62.101346562721474,402.28154955240439,304.09843648811176,385.36888750680248,"",127.24633674315731,384.04107769941277,293.4237687997641,366.93134870637874,"","62-402",327.67847111762865,null,null,null,null,"HLH","","","","","","","","","","","0-0",{"$error":"#DIV/0!"}]
["Cooling","Ann Cool Energy kBtu",67998,144804,47630,137324,123913,74665,159808,54759,152621,144879,1108401,null,null,null,null,"Cooling","Ann Cool Energy kBtu",null,null,null,null,null,null,null,null,null,null,0]
[null,"Ann peak Cooling load kBtu/hr",35.576999999999998,92.097999999999999,28.635000000000002,91.262,96.67,37.527999999999999,95.855000000000004,31.553999999999998,96.754999999999995,118.282,724.21600000000001,null,null,null,null,null,"Ann peak Cooling load kBtu/hr",null,null,null,null,null,null,null,null,null,null,0]
[null,"CLH",1911.2910026140485,1572.2816999283373,1663.3490483673825,1504.7226666082267,1281.8144201924072,1989.5811127691325,1667.1848103906941,1735.4059707168665,1577.3965169758669,1224.8609255846197,"1225-1990",1530.4839992488428,null,null,null,null,"CLH","","","","","","","","","","","0-0",{"$error":"#DIV/0!"}]
[]
["Scooper Office 8-17 wo setback continuous"]
[null,-0.621,-10.718999999999999,76.802000000000007,38.572000000000003]
[null,-8.9730000000000008,-24.145,159.614,96.667000000000002]
[null,-3.621,-10.776,51.686,29.832000000000001]
[null,-9.2789999999999999,-24.803000000000001,152.529,96.028999999999996]
[null,-0.61799999999999999,-32.731000000000002,134.17599999999999,116.43]
[null,-1.6759999999999999,-13.855,84.841999999999999,40.856999999999999]
[null,-11.929,-33.134,176.11500000000001,101.33499999999999]
[null,-4.0730000000000004,-13.513,59.924999999999997,32.908999999999999]
[null,-12.195,-33.475999999999999,170.27,102.17100000000001]
[null,-1.891,-36.485999999999997,155.48699999999999,134.434]
[]
[null,-0.621,-8.9730000000000008,-3.621,-9.2789999999999999,-0.61799999999999999,-1.6759999999999999,-11.929,-4.0730000000000004,-12.195,-1.891]
[null,-10.718999999999999,-24.145,-10.776,-24.803000000000001,-32.731000000000002,-13.855,-33.134,-13.513,-33.475999999999999,-36.485999999999997]
[null,76.802000000000007,159.614,51.686,152.529,134.17599999999999,84.841999999999999,176.11500000000001,59.924999999999997,170.27,155.48699999999999]
[null,38.572000000000003,96.667000000000002,29.832000000000001,96.028999999999996,116.43,40.856999999999999,101.33499999999999,32.908999999999999,102.17100000000001,134.434]
[]
[null,"=-621","=-8973","=-3621","=-9279","=-618","=-1676","=-11929","=-4073","=-12195","=-1891"]
[null,-10.718999999999999,-24.145,-10.776,-24.803000000000001,-32.731000000000002,-13.855,-33.134,-13.513,-33.475999999999999,-36.485999999999997]
[null,"=76802","=159614","=51686","=152529","=134176","=84842","=176115","=59925","=170270","=155487"]
[null,38.572000000000003,96.667000000000002,29.832000000000001,96.028999999999996,116.43,40.856999999999999,101.33499999999999,32.908999999999999,102.17100000000001,134.434]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-621,-8973,-3621,-9279,-618,-1676,-11929,-4073,-12195,-1891,-54876]
[null,"Ann peak Heating load kBtu/hr",-10.718999999999999,-24.145,-10.776,-24.803000000000001,-32.731000000000002,-13.855,-33.134,-13.513,-33.475999999999999,-36.485999999999997,-233.63800000000001]
[null,"HLH",57.934508816120911,371.62973700559121,336.02449888641428,374.10797080998265,18.881182976383243,120.96715987008299,360.02293716424214,301.413453711241,364.29083522523598,"19-374","19-374",234.87617596452631]
["Cooling","Ann Cool Energy kBtu",67998,144804,47630,137324,123913,74665,159808,54759,152621,144879,1108401]
[null,"Ann peak Cooling load kBtu/hr",35.576999999999998,92.097999999999999,28.635000000000002,91.262,96.67,37.527999999999999,95.855000000000004,31.553999999999998,96.754999999999995,118.282,724.21600000000001]
[null,"CLH",1911.2910026140485,1572.2816999283373,1663.3490483673825,1504.7226666082267,1281.8144201924072,1989.5811127691325,1667.1848103906941,1735.4059707168665,1577.3965169758669,"1282-1990","1282-1990",1530.4839992488428]
[]
["****Intermittent is default for remaining results"]
[]
["SCooper Office 8-17 w setback - Baseline Design.SIM"]
[null,-0.432,-23.838000000000001,51.923000000000002,39.369]
[null,-1.0309999999999999,-51.244,117.998,108.524]
[null,-1.014,-25.119,37.475000000000001,32.042999999999999]
[null,-1.7809999999999999,-52.366,107.617,98.923000000000002]
[null,-1.07,-84.747,157.08699999999999,135.86699999999999]
[null,-0.745,-30.335999999999999,56.837000000000003,41.622999999999998]
[null,-2.31,-67.599000000000004,133.517,119.688]
[null,-1.657,-29.701000000000001,43.508000000000003,35.348999999999997]
[null,-3.7909999999999999,-68.775000000000006,118.919,104.988]
[null,-2.835,-108.252,175.209,161.18]
[]
[null,-0.432,-1.0309999999999999,-1.014,-1.7809999999999999,-1.07,-0.745,-2.31,-1.657,-3.7909999999999999,-2.835]
[null,-23.838000000000001,-51.244,-25.119,-52.366,-84.747,-30.335999999999999,-67.599000000000004,-29.701000000000001,-68.775000000000006,-108.252]
[null,51.923000000000002,117.998,37.475000000000001,107.617,157.08699999999999,56.837000000000003,133.517,43.508000000000003,118.919,175.209]
[null,39.369,108.524,32.042999999999999,98.923000000000002,135.86699999999999,41.622999999999998,119.688,35.348999999999997,104.988,161.18]
[]
[null,"=-432","=-1031","=-1014","=-1781","=-1070","=-745","=-2310","=-1657","=-3791","=-2835"]
[null,-23.838000000000001,-51.244,-25.119,-52.366,-84.747,-30.335999999999999,-67.599000000000004,-29.701000000000001,-68.775000000000006,-108.252]
[null,"=51923","=117998","=37475","=107617","=157087","=56837","=133517","=43508","=118919","=175209"]
[null,39.369,108.524,32.042999999999999,98.923000000000002,135.86699999999999,41.622999999999998,119.688,35.348999999999997,104.988,161.18]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-432,-1031,-1014,-1781,-1070,-745,-2310,-1657,-3791,-2835,-16666]
[null,"Ann peak Heating load kBtu/hr",-23.838000000000001,-51.244,-25.119,-52.366,-84.747,-30.335999999999999,-67.599000000000004,-29.701000000000001,-68.775000000000006,-108.252,-541.97699999999998]
[null,"HLH",18.122325698464635,20.119428616033098,40.367849038576374,34.01061757628996,12.625815663091318,24.558280590717303,34.172103137620375,55.789367361368306,55.121773900399852,"13-56","13-56",30.750382396300953]
["Cooling","Ann Cool Energy kBtu",51923,117998,37475,107617,157087,56837,133517,43508,118919,175209,1000090]
[null,"Ann peak Cooling load kBtu/hr",39.369,108.524,32.042999999999999,98.923000000000002,135.86699999999999,41.622999999999998,119.688,35.348999999999997,104.988,161.18,877.55400000000009]
[null,"CLH",1318.8803373212427,1087.2986620471047,1169.5222045376527,1087.8865380144152,1156.1821487189679,1365.5190639790501,1115.5420760644342,1230.8127528360069,1132.6913552024994,"1087-1366","1087-1366",1139.6335724069402]
[]
["SCooper Office 7-22 w setback - Baseline Design.SIM"]
[null,-0.48299999999999998,-23.337,63.328000000000003,37.807000000000002]
[null,-1.3,-52.959000000000003,144.739,102.96899999999999]
[null,-1.0900000000000001,-24.809000000000001,47.576999999999998,30.361000000000001]
[null,-1.6539999999999999,-50.883000000000003,140.07,95.105999999999995]
[null,-0.71799999999999997,-76.328000000000003,231.93,124.253]
[null,-0.84,-30.459,70.155000000000001,39.472000000000001]
[null,-2.3220000000000001,-71.688999999999993,163.154,112.148]
[null,-1.472,-30.974,55.210999999999999,33.369999999999997]
[null,-3.077,-69.819000000000003,155.941,104.292]
[null,-2.0150000000000001,-119.19499999999999,255.30699999999999,156.476]
[]
[null,-0.48299999999999998,-1.3,-1.0900000000000001,-1.6539999999999999,-0.71799999999999997,-0.84,-2.3220000000000001,-1.472,-3.077,-2.0150000000000001]
[null,-23.337,-52.959000000000003,-24.809000000000001,-50.883000000000003,-76.328000000000003,-30.459,-71.688999999999993,-30.974,-69.819000000000003,-119.19499999999999]
[null,63.328000000000003,144.739,47.576999999999998,140.07,231.93,70.155000000000001,163.154,55.210999999999999,155.941,255.30699999999999]
[null,37.807000000000002,102.96899999999999,30.361000000000001,95.105999999999995,124.253,39.472000000000001,112.148,33.369999999999997,104.292,156.476]
[]
[null,"=-483","=-1300","=-1090","=-1654","=-718","=-840","=-2322","=-1472","=-3077","=-2015"]
[null,-23.337,-52.959000000000003,-24.809000000000001,-50.883000000000003,-76.328000000000003,-30.459,-71.688999999999993,-30.974,-69.819000000000003,-119.19499999999999]
[null,"=63328","=144739","=47577","=140070","=231930","=70155","=163154","=55211","=155941","=255307"]
[null,37.807000000000002,102.96899999999999,30.361000000000001,95.105999999999995,124.253,39.472000000000001,112.148,33.369999999999997,104.292,156.476]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-483,-1300,-1090,-1654,-718,-840,-2322,-1472,-3077,-2015,-14971]
[null,"Ann peak Heating load kBtu/hr",-23.337,-52.959000000000003,-24.809000000000001,-50.883000000000003,-76.328000000000003,-30.459,-71.688999999999993,-30.974,-69.819000000000003,-119.19499999999999,-550.452]
[null,"HLH",20.696747653940097,24.547291300817612,43.935668507396507,32.505945011103904,9.4067707787443666,27.578055747069833,32.389906401261008,47.523729579647444,44.071098125152176,"9-48","9-48",27.197648477978099]
["Cooling","Ann Cool Energy kBtu",63328,144739,47577,140070,231930,70155,163154,55211,155941,255307,1327412]
[null,"Ann peak Cooling load kBtu/hr",37.807000000000002,102.96899999999999,30.361000000000001,95.105999999999995,124.253,39.472000000000001,112.148,33.369999999999997,104.292,156.476,836.25400000000002]
[null,"CLH",1675.0337239135608,1405.6560712447435,1567.0432462698857,1472.7777427291655,1866.5947703475972,1777.3358329955411,1454.8097157327818,1654.5100389571473,1495.234533808921,"1406-1867","1406-1867",1587.3311218840208]
[]
["SCooper Office 7-19 w setback - Baseline Design.SIM"]
[null,-0.54800000000000004,-23.858000000000001,57.392000000000003,38.155999999999999]
[null,-1.38,-54.408999999999999,130.41399999999999,103.274]
[null,-1.115,-25.571000000000002,42.325000000000003,30.433]
[null,-1.8460000000000001,-52.347000000000001,124.47199999999999,97.058999999999997]
[null,-0.86199999999999999,-82.914000000000001,194.626,125.398]
[null,-0.94399999999999995,-31.196000000000002,63.264000000000003,40.057000000000002]
[null,-2.7040000000000002,-72.385999999999996,147.345,112.393]
[null,-1.65,-31.687999999999999,49.113,33.351999999999997]
[null,-3.569,-70.427999999999997,137.49,105.217]
[null,-2.3180000000000001,-122.361,215.26900000000001,159.785]
[]
[null,-0.54800000000000004,-1.38,-1.115,-1.8460000000000001,-0.86199999999999999,-0.94399999999999995,-2.7040000000000002,-1.65,-3.569,-2.3180000000000001]
[null,-23.858000000000001,-54.408999999999999,-25.571000000000002,-52.347000000000001,-82.914000000000001,-31.196000000000002,-72.385999999999996,-31.687999999999999,-70.427999999999997,-122.361]
[null,57.392000000000003,130.41399999999999,42.325000000000003,124.47199999999999,194.626,63.264000000000003,147.345,49.113,137.49,215.26900000000001]
[null,38.155999999999999,103.274,30.433,97.058999999999997,125.398,40.057000000000002,112.393,33.351999999999997,105.217,159.785]
[]
[null,"=-548","=-1380","=-1115","=-1846","=-862","=-944","=-2704","=-1650","=-3569","=-2318"]
[null,-23.858000000000001,-54.408999999999999,-25.571000000000002,-52.347000000000001,-82.914000000000001,-31.196000000000002,-72.385999999999996,-31.687999999999999,-70.427999999999997,-122.361]
[null,"=57392","=130414","=42325","=124472","=194626","=63264","=147345","=49113","=137490","=215269"]
[null,38.155999999999999,103.274,30.433,97.058999999999997,125.398,40.057000000000002,112.393,33.351999999999997,105.217,159.785]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-548,-1380,-1115,-1846,-862,-944,-2704,-1650,-3569,-2318,-16936]
[null,"Ann peak Heating load kBtu/hr",-23.858000000000001,-54.408999999999999,-25.571000000000002,-52.347000000000001,-82.914000000000001,-31.196000000000002,-72.385999999999996,-31.687999999999999,-70.427999999999997,-122.361,-567.15800000000002]
[null,"HLH",22.969234638276468,25.363450899667335,43.604082749990219,35.264676103692665,10.39631425332272,30.260289780741118,37.355289696902716,52.070184296894723,50.675867552677914,"10-52","10-52",29.861167434824157]
["Cooling","Ann Cool Energy kBtu",57392,130414,42325,124472,194626,63264,147345,49113,137490,215269,1161710]
[null,"Ann peak Cooling load kBtu/hr",38.155999999999999,103.274,30.433,97.058999999999997,125.398,40.057000000000002,112.393,33.351999999999997,105.217,159.785,845.12400000000002]
[null,"CLH",1504.1408952720412,1262.7960570908458,1390.7600302303422,1282.4364561761404,1552.0662211518525,1579.3494270664303,1310.9802211881522,1472.565363396498,1306.7280002281,"1263-1579","1263-1579",1374.6030168353993]
[]
["SCooper Office 6-21 7days w setback - Baseline Design.SIM"]
[null,-1.42,-20.343,72.504000000000005,36.488999999999997]
[null,-4.7560000000000002,-46.357999999999997,163.209,93.144000000000005]
[null,-3.1560000000000001,-20.47,52.572000000000003,28.576000000000001]
[null,-5.1529999999999996,-46.738,155.697,93.198999999999998]
[null,-0.97,-49.066000000000003,234.09100000000001,101.387]
[null,-2.145,-25.728000000000002,79.787999999999997,38.704000000000001]
[null,-6.2729999999999997,-60.753,182.114,96.793000000000006]
[null,-3.7029999999999998,-25.367000000000001,60.225999999999999,31.616]
[null,-7.3890000000000002,-60.805,171.21,100.768]
[null,-5.3019999999999996,-94.116,260.94900000000001,125.286]
[]
[null,-1.42,-4.7560000000000002,-3.1560000000000001,-5.1529999999999996,-0.97,-2.145,-6.2729999999999997,-3.7029999999999998,-7.3890000000000002,-5.3019999999999996]
[null,-20.343,-46.357999999999997,-20.47,-46.738,-49.066000000000003,-25.728000000000002,-60.753,-25.367000000000001,-60.805,-94.116]
[null,72.504000000000005,163.209,52.572000000000003,155.697,234.09100000000001,79.787999999999997,182.114,60.225999999999999,171.21,260.94900000000001]
[null,36.488999999999997,93.144000000000005,28.576000000000001,93.198999999999998,101.387,38.704000000000001,96.793000000000006,31.616,100.768,125.286]
[]
[null,"=-1420","=-4756","=-3156","=-5153","=-970","=-2145","=-6273","=-3703","=-7389","=-5302"]
[null,-20.343,-46.357999999999997,-20.47,-46.738,-49.066000000000003,-25.728000000000002,-60.753,-25.367000000000001,-60.805,-94.116]
[null,"=72504","=163209","=52572","=155697","=234091","=79788","=182114","=60226","=171210","=260949"]
[null,36.488999999999997,93.144000000000005,28.576000000000001,93.198999999999998,101.387,38.704000000000001,96.793000000000006,31.616,100.768,125.286]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1420,-4756,-3156,-5153,-970,-2145,-6273,-3703,-7389,-5302,-40267]
[null,"Ann peak Heating load kBtu/hr",-20.343,-46.357999999999997,-20.47,-46.738,-49.066000000000003,-25.728000000000002,-60.753,-25.367000000000001,-60.805,-94.116,-449.74400000000003]
[null,"HLH",69.802880597748612,102.59286423055353,154.17684416218859,110.25289913988618,19.769290343618799,83.372201492537314,103.25416028838082,145.97705680608664,121.51961187402352,"20-154","20-154",89.533156640221989]
["Cooling","Ann Cool Energy kBtu",72504,163209,52572,155697,234091,79788,182114,60226,171210,260949,1432360]
[null,"Ann peak Cooling load kBtu/hr",36.488999999999997,93.144000000000005,28.576000000000001,93.198999999999998,101.387,38.704000000000001,96.793000000000006,31.616,100.768,125.286,745.96199999999999]
[null,"CLH",1987.0097837704516,1752.2223653697499,1839.7256438969764,1670.5865942767628,2308.885754583921,2061.4923522116578,1881.4790325746696,1904.9215587044534,1699.0512861225786,"1671-2309","1671-2309",1920.1514286250506]
[]
["SCooper Office 6-19 7days w setback - Baseline Design.SIM"]
[null,-1.3660000000000001,-22.452000000000002,68.138999999999996,36.631999999999998]
[null,-4.38,-49.433,152.71299999999999,94.218999999999994]
[null,-2.96,-22.375,48.691000000000003,28.803000000000001]
[null,-4.9550000000000001,-49.671999999999997,144.17599999999999,94.888999999999996]
[null,-1.3540000000000001,-71.754999999999995,210.45099999999999,103.38500000000001]
[null,-2.218,-28.876999999999999,74.536000000000001,38.938000000000002]
[null,-6.117,-64.602999999999994,170.048,98.557000000000002]
[null,-3.6589999999999998,-28.469000000000001,55.52,32.140999999999998]
[null,-7.4850000000000003,-64.600999999999999,156.84299999999999,102.904]
[null,-6.032,-101.94199999999999,235.881,128.15700000000001]
[]
[null,-1.3660000000000001,-4.38,-2.96,-4.9550000000000001,-1.3540000000000001,-2.218,-6.117,-3.6589999999999998,-7.4850000000000003,-6.032]
[null,-22.452000000000002,-49.433,-22.375,-49.671999999999997,-71.754999999999995,-28.876999999999999,-64.602999999999994,-28.469000000000001,-64.600999999999999,-101.94199999999999]
[null,68.138999999999996,152.71299999999999,48.691000000000003,144.17599999999999,210.45099999999999,74.536000000000001,170.048,55.52,156.84299999999999,235.881]
[null,36.631999999999998,94.218999999999994,28.803000000000001,94.888999999999996,103.38500000000001,38.938000000000002,98.557000000000002,32.140999999999998,102.904,128.15700000000001]
[]
[null,"=-1366","=-4380","=-2960","=-4955","=-1354","=-2218","=-6117","=-3659","=-7485","=-6032"]
[null,-22.452000000000002,-49.433,-22.375,-49.671999999999997,-71.754999999999995,-28.876999999999999,-64.602999999999994,-28.469000000000001,-64.600999999999999,-101.94199999999999]
[null,"=68139","=152713","=48691","=144176","=210451","=74536","=170048","=55520","=156843","=235881"]
[null,36.631999999999998,94.218999999999994,28.803000000000001,94.888999999999996,103.38500000000001,38.938000000000002,98.557000000000002,32.140999999999998,102.904,128.15700000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1366,-4380,-2960,-4955,-1354,-2218,-6117,-3659,-7485,-6032,-40526]
[null,"Ann peak Heating load kBtu/hr",-22.452000000000002,-49.433,-22.375,-49.671999999999997,-71.754999999999995,-28.876999999999999,-64.602999999999994,-28.469000000000001,-64.600999999999999,-101.94199999999999,-504.17900000000003]
[null,"HLH",60.840905041867089,88.604778184613522,132.2905027932961,99.754388790465455,18.869765173158665,76.808532742320878,94.686005293871816,128.52576486704837,115.86507948793363,"19-132","19-132",80.380182435206535]
["Cooling","Ann Cool Energy kBtu",68139,152713,48691,144176,210451,74536,170048,55520,156843,235881,1316998]
[null,"Ann peak Cooling load kBtu/hr",36.631999999999998,94.218999999999994,28.803000000000001,94.888999999999996,103.38500000000001,38.938000000000002,98.557000000000002,32.140999999999998,102.904,128.15700000000001,758.625]
[null,"CLH",1860.0949989080586,1620.8301934853905,1690.4836301774121,1519.4174245697604,2035.6047782560331,1914.2226103035593,1725.3771928934525,1727.3886935689618,1524.1681567286014,"1519-2036","1519-2036",1736.0329543582138]
[]
["SCooper Office 5-23 7days w setback - Baseline Design.SIM"]
[null,-1.597,-16.852,78.290999999999997,36.159999999999997]
[null,-5.48,-41.31,177.60599999999999,92.174000000000007]
[null,-3.5760000000000001,-19.175000000000001,57.582999999999998,28.114999999999998]
[null,-5.6970000000000001,-41.796999999999997,170.31899999999999,92.411000000000001]
[null,-0.38700000000000001,-34.936,270.04599999999999,99.27]
[null,-2.2389999999999999,-20.721,86.126000000000005,38.226999999999997]
[null,-6.8869999999999996,-52.878999999999998,197.30799999999999,94.418000000000006]
[null,-3.919,-22.103000000000002,65.988,31.106000000000002]
[null,-7.4189999999999996,-52.350999999999999,188.148,100.023]
[null,-4.29,-82.102999999999994,298.267,121.934]
[]
[null,-1.597,-5.48,-3.5760000000000001,-5.6970000000000001,-0.38700000000000001,-2.2389999999999999,-6.8869999999999996,-3.919,-7.4189999999999996,-4.29]
[null,-16.852,-41.31,-19.175000000000001,-41.796999999999997,-34.936,-20.721,-52.878999999999998,-22.103000000000002,-52.350999999999999,-82.102999999999994]
[null,78.290999999999997,177.60599999999999,57.582999999999998,170.31899999999999,270.04599999999999,86.126000000000005,197.30799999999999,65.988,188.148,298.267]
[null,36.159999999999997,92.174000000000007,28.114999999999998,92.411000000000001,99.27,38.226999999999997,94.418000000000006,31.106000000000002,100.023,121.934]
[]
[null,"=-1597","=-5480","=-3576","=-5697","=-387","=-2239","=-6887","=-3919","=-7419","=-4290"]
[null,-16.852,-41.31,-19.175000000000001,-41.796999999999997,-34.936,-20.721,-52.878999999999998,-22.103000000000002,-52.350999999999999,-82.102999999999994]
[null,"=78291","=177606","=57583","=170319","=270046","=86126","=197308","=65988","=188148","=298267"]
[null,36.159999999999997,92.174000000000007,28.114999999999998,92.411000000000001,99.27,38.226999999999997,94.418000000000006,31.106000000000002,100.023,121.934]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1597,-5480,-3576,-5697,-387,-2239,-6887,-3919,-7419,-4290,-41491]
[null,"Ann peak Heating load kBtu/hr",-16.852,-41.31,-19.175000000000001,-41.796999999999997,-34.936,-20.721,-52.878999999999998,-22.103000000000002,-52.350999999999999,-82.102999999999994,-384.22700000000003]
[null,"HLH",94.766199857583672,132.65553134834181,186.49282920469361,136.30164844366823,11.077398671857111,108.05463056802277,130.24073828930199,177.30624802063068,141.71649061144964,"11-186","11-186",107.98564390321346]
["Cooling","Ann Cool Energy kBtu",78291,177606,57583,170319,270046,86126,197308,65988,188148,298267,1589682]
[null,"Ann peak Cooling load kBtu/hr",36.159999999999997,92.174000000000007,28.114999999999998,92.411000000000001,99.27,38.226999999999997,94.418000000000006,31.106000000000002,100.023,121.934,733.83799999999997]
[null,"CLH",2165.1272123893809,1926.8557293813872,2048.1237773430553,1843.0598088972092,2720.3183237634735,2253.0148847673113,2089.7286534347263,2121.3913714395935,1881.0473591074053,"1843-2720","1843-2720",2166.257402860032]
[]
["SCooper Office 24 7days w setback - Baseline Design.SIM"]
[null,-1.946,-13.704000000000001,85.840999999999994,35.658000000000001]
[null,-6.7770000000000001,-33.381999999999998,197.70500000000001,90.427999999999997]
[null,-4.4509999999999996,-17.233000000000001,64.241,27.843]
[null,-6.7690000000000001,-33.704000000000001,190.66300000000001,92.123999999999995]
[null,-1E-3,-0.16800000000000001,330.024,99.912000000000006]
[null,-2.3969999999999998,-16.084,94.08,37.656999999999996]
[null,-8.0419999999999998,-40.603000000000002,217.886,92.909000000000006]
[null,-4.4130000000000003,-18.917999999999999,73.382999999999996,30.893000000000001]
[null,-7.8810000000000002,-40.401000000000003,210.19800000000001,99.846000000000004]
[null,-2.8290000000000002,-74.293000000000006,360.38499999999999,122.20399999999999]
[]
[null,-1.946,-6.7770000000000001,-4.4509999999999996,-6.7690000000000001,-1E-3,-2.3969999999999998,-8.0419999999999998,-4.4130000000000003,-7.8810000000000002,-2.8290000000000002]
[null,-13.704000000000001,-33.381999999999998,-17.233000000000001,-33.704000000000001,-0.16800000000000001,-16.084,-40.603000000000002,-18.917999999999999,-40.401000000000003,-74.293000000000006]
[null,85.840999999999994,197.70500000000001,64.241,190.66300000000001,330.024,94.08,217.886,73.382999999999996,210.19800000000001,360.38499999999999]
[null,35.658000000000001,90.427999999999997,27.843,92.123999999999995,99.912000000000006,37.656999999999996,92.909000000000006,30.893000000000001,99.846000000000004,122.20399999999999]
[]
[null,"=-1946","=-6777","=-4451","=-6769","=-1","=-2397","=-8042","=-4413","=-7881","=-2829"]
[null,-13.704000000000001,-33.381999999999998,-17.233000000000001,-33.704000000000001,-0.16800000000000001,-16.084,-40.603000000000002,-18.917999999999999,-40.401000000000003,-74.293000000000006]
[null,"=85841","=197705","=64241","=190663","=330024","=94080","=217886","=73383","=210198","=360385"]
[null,35.658000000000001,90.427999999999997,27.843,92.123999999999995,99.912000000000006,37.656999999999996,92.909000000000006,30.893000000000001,99.846000000000004,122.20399999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1946,-6777,-4451,-6769,-1,-2397,-8042,-4413,-7881,-2829,-45506]
[null,"Ann peak Heating load kBtu/hr",-13.704000000000001,-33.381999999999998,-17.233000000000001,-33.704000000000001,-0.16800000000000001,-16.084,-40.603000000000002,-18.917999999999999,-40.401000000000003,-74.293000000000006,-288.49]
[null,"HLH",142.0023350846468,203.01360014379009,258.28352579353566,200.83669594113459,5.9523809523809517,149.03009201691123,198.06418244957268,233.2699016809388,195.06942897453033,38.078957640692927,"6-258",157.73856979444693]
["Cooling","Ann Cool Energy kBtu",85841,197705,64241,190663,330024,94080,217886,73383,210198,360385,1824406]
[null,"Ann peak Cooling load kBtu/hr",35.658000000000001,90.427999999999997,27.843,92.123999999999995,99.912000000000006,37.656999999999996,92.909000000000006,30.893000000000001,99.846000000000004,122.20399999999999,729.47399999999993]
[null,"CLH",2407.3419709462109,2186.325032069713,2307.258556908379,2069.6344058008772,3303.1467691568578,2498.3402820192796,2345.1549365508185,2375.3924837341792,2105.2220419445948,2949.0442211384243,"2070-3303",2500.9883834105126]
[]
[]
["SCooper Rest 9-18 w setback - Baseline Design.SIM"]
[null,-0.50600000000000001,-12.208,83.620999999999995,60.298000000000002]
[null,-1.1220000000000001,-11.808999999999999,77.358999999999995,63.587000000000003]
[null,-2.609,-16.795000000000002,66.569999999999993,62.072000000000003]
[null,-1.6419999999999999,-15.744999999999999,73.849999999999994,69.513000000000005]
[null,-0.18,-10.628,41.865000000000002,35.881999999999998]
[]
[]
[]
[]
[]
[]
[null,-0.50600000000000001,-1.1220000000000001,-2.609,-1.6419999999999999,-0.18]
[null,-12.208,-11.808999999999999,-16.795000000000002,-15.744999999999999,-10.628]
[null,83.620999999999995,77.358999999999995,66.569999999999993,73.849999999999994,41.865000000000002]
[null,60.298000000000002,63.587000000000003,62.072000000000003,69.513000000000005,35.881999999999998]
[]
[null,"=-506","=-1122","=-2609","=-1642","=-180","=0","=0","=0","=0","=0"]
[null,-12.208,-11.808999999999999,-16.795000000000002,-15.744999999999999,-10.628,0,0,0,0,0]
[null,"=83621","=77359","=66570","=73850","=41865","=0","=0","=0","=0","=0"]
[null,60.298000000000002,63.587000000000003,62.072000000000003,69.513000000000005,35.881999999999998,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-506,-1122,-2609,-1642,-180,0,0,0,0,0,-6059]
[null,"Ann peak Heating load kBtu/hr",-12.208,-11.808999999999999,-16.795000000000002,-15.744999999999999,-10.628,0,0,0,0,0,-67.185000000000002]
[null,"HLH",41.448230668414155,95.012278770429333,155.34385233700505,104.28707526198794,16.936394429808054,"","","","","","17-155",90.183820793331847]
["Cooling","Ann Cool Energy kBtu",83621,77359,66570,73850,41865,0,0,0,0,0,343265]
[null,"Ann peak Cooling load kBtu/hr",60.298000000000002,63.587000000000003,62.072000000000003,69.513000000000005,35.881999999999998,0,0,0,0,0,291.35199999999998]
[null,"CLH",1386.7955819430163,1216.585151052888,1072.4642350818403,1062.3912074000546,1166.740984337551,"","","","","","1062-1387",1178.1796589692194]
[]
["SCooper Rest 8-20 w setback - Baseline Design.SIM"]
[null,-0.17399999999999999,-10.867000000000001,49.701000000000001,32.406999999999996]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,-0.17399999999999999]
[null,-10.867000000000001]
[null,49.701000000000001]
[null,32.406999999999996]
[]
[null,"=-174","=0","=0","=0","=0","=0","=0","=0","=0","=0"]
[null,-10.867000000000001,0,0,0,0,0,0,0,0,0]
[null,"=49701","=0","=0","=0","=0","=0","=0","=0","=0","=0"]
[null,32.406999999999996,0,0,0,0,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-174,0,0,0,0,0,0,0,0,0,-174]
[null,"Ann peak Heating load kBtu/hr",-10.867000000000001,0,0,0,0,0,0,0,0,0,-10.867000000000001]
[null,"HLH",16.011778779792028,"","","","","","","","","","16-16",16.011778779792028]
["Cooling","Ann Cool Energy kBtu",49701,0,0,0,0,0,0,0,0,0,49701]
[null,"Ann peak Cooling load kBtu/hr",32.406999999999996,0,0,0,0,0,0,0,0,0,32.406999999999996]
[null,"CLH",1533.6501373160122,"","","","","","","","","","1534-1534",1533.6501373160122]
[]
["SCooper Rest 7-22 w setback - Baseline Design.SIM"]
[null,-0.96799999999999997,-17.754000000000001,103.98399999999999,59.276000000000003]
[null,-1.534,-20.085999999999999,97.382000000000005,61.713999999999999]
[null,-2.81,-26.838999999999999,86.174000000000007,57.429000000000002]
[null,-1.7629999999999999,-20.085999999999999,93.813999999999993,64.224000000000004]
[null,-0.16300000000000001,-10.715,56.917999999999999,31.658999999999999]
[]
[]
[]
[]
[]
[]
[null,-0.96799999999999997,-1.534,-2.81,-1.7629999999999999,-0.16300000000000001]
[null,-17.754000000000001,-20.085999999999999,-26.838999999999999,-20.085999999999999,-10.715]
[null,103.98399999999999,97.382000000000005,86.174000000000007,93.813999999999993,56.917999999999999]
[null,59.276000000000003,61.713999999999999,57.429000000000002,64.224000000000004,31.658999999999999]
[]
[null,"=-968","=-1534","=-2810","=-1763","=-163","=0","=0","=0","=0","=0"]
[null,-17.754000000000001,-20.085999999999999,-26.838999999999999,-20.085999999999999,-10.715,0,0,0,0,0]
[null,"=103984","=97382","=86174","=93814","=56918","=0","=0","=0","=0","=0"]
[null,59.276000000000003,61.713999999999999,57.429000000000002,64.224000000000004,31.658999999999999,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-968,-1534,-2810,-1763,-163,0,0,0,0,0,-7238]
[null,"Ann peak Heating load kBtu/hr",-17.754000000000001,-20.085999999999999,-26.838999999999999,-20.085999999999999,-10.715,0,0,0,0,0,-95.48]
[null,"HLH",54.522924411400247,76.371602110923035,104.69838667610567,87.772577914965652,15.212319178721419,"","","","","","15-105",75.806451612903217]
["Cooling","Ann Cool Energy kBtu",103984,97382,86174,93814,56918,0,0,0,0,0,438272]
[null,"Ann peak Cooling load kBtu/hr",59.276000000000003,61.713999999999999,57.429000000000002,64.224000000000004,31.658999999999999,0,0,0,0,0,274.30200000000002]
[null,"CLH",1754.2344287738713,1577.9563794276826,1500.5310905640008,1460.7311908320876,1797.8457942449224,"","","","","","1461-1798",1597.771798966103]
[]
["SCooper Rest 9-22 7days w setback - Baseline Design.SIM"]
[null,-0.28899999999999998,-11.84,128.34399999999999,59.313000000000002]
[null,-0.373,-10.574999999999999,119.283,64.164000000000001]
[null,-1.4710000000000001,-33.515999999999998,107.80500000000001,57.350999999999999]
[null,-1.0780000000000001,-27.111999999999998,116.652,63.716000000000001]
[null,-4.0000000000000001E-3,-4.3550000000000004,72.962999999999994,28.998000000000001]
[]
[]
[]
[]
[]
[]
[null,-0.28899999999999998,-0.373,-1.4710000000000001,-1.0780000000000001,-4.0000000000000001E-3]
[null,-11.84,-10.574999999999999,-33.515999999999998,-27.111999999999998,-4.3550000000000004]
[null,128.34399999999999,119.283,107.80500000000001,116.652,72.962999999999994]
[null,59.313000000000002,64.164000000000001,57.350999999999999,63.716000000000001,28.998000000000001]
[]
[null,"=-289","=-373","=-1471","=-1078","=-4","=0","=0","=0","=0","=0"]
[null,-11.84,-10.574999999999999,-33.515999999999998,-27.111999999999998,-4.3550000000000004,0,0,0,0,0]
[null,"=128344","=119283","=107805","=116652","=72963","=0","=0","=0","=0","=0"]
[null,59.313000000000002,64.164000000000001,57.350999999999999,63.716000000000001,28.998000000000001,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-289,-373,-1471,-1078,-4,0,0,0,0,0,-3215]
[null,"Ann peak Heating load kBtu/hr",-11.84,-10.574999999999999,-33.515999999999998,-27.111999999999998,-4.3550000000000004,0,0,0,0,0,-87.397999999999996]
[null,"HLH",24.408783783783782,35.27186761229315,43.889485618808926,39.760991442903517,0.91848450057405273,"","","","","","1-44",36.785738804091629]
["Cooling","Ann Cool Energy kBtu",128344,119283,107805,116652,72963,0,0,0,0,0,545047]
[null,"Ann peak Cooling load kBtu/hr",59.313000000000002,64.164000000000001,57.350999999999999,63.716000000000001,28.998000000000001,0,0,0,0,0,273.54200000000003]
[null,"CLH",2163.8426651830123,1859.0331026743968,1879.7405450646022,1830.8117270387343,2516.1390440720047,"","","","","","1831-2516",1992.5532459366384]
[]
["SCooper Rest 8-22 7days w setback - Baseline Design.SIM"]
[null,-0.67200000000000004,-17.123999999999999,132.93899999999999,59.052999999999997]
[null,-0.68799999999999994,-16.132000000000001,124.182,65.424000000000007]
[null,-1.8260000000000001,-35.658999999999999,112.574,57.444000000000003]
[null,-1.343,-34.259,121.19,63.542999999999999]
[null,0,0,76.061999999999998,28.582000000000001]
[]
[]
[]
[]
[]
[]
[null,-0.67200000000000004,-0.68799999999999994,-1.8260000000000001,-1.343,0]
[null,-17.123999999999999,-16.132000000000001,-35.658999999999999,-34.259,0]
[null,132.93899999999999,124.182,112.574,121.19,76.061999999999998]
[null,59.052999999999997,65.424000000000007,57.444000000000003,63.542999999999999,28.582000000000001]
[]
[null,"=-672","=-688","=-1826","=-1343","=0","=0","=0","=0","=0","=0"]
[null,-17.123999999999999,-16.132000000000001,-35.658999999999999,-34.259,0,0,0,0,0,0]
[null,"=132939","=124182","=112574","=121190","=76062","=0","=0","=0","=0","=0"]
[null,59.052999999999997,65.424000000000007,57.444000000000003,63.542999999999999,28.582000000000001,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-672,-688,-1826,-1343,0,0,0,0,0,0,-4529]
[null,"Ann peak Heating load kBtu/hr",-17.123999999999999,-16.132000000000001,-35.658999999999999,-34.259,0,0,0,0,0,0,-103.17399999999999]
[null,"HLH",39.243167484232657,42.648152739895856,51.207268852183184,39.20137774015587,"","","","","","","39-51",43.896718165429277]
["Cooling","Ann Cool Energy kBtu",132939,124182,112574,121190,76062,0,0,0,0,0,566947]
[null,"Ann peak Cooling load kBtu/hr",59.052999999999997,65.424000000000007,57.444000000000003,63.542999999999999,28.582000000000001,0,0,0,0,0,274.04599999999999]
[null,"CLH",2251.1811423636395,1898.1107850330152,1959.7172898823201,1907.2124388209559,2661.185361416276,"","","","","","1898-2661",2068.8023178590456]
[]
["SCooper Rest 5-23 7days w setback - Baseline Design.SIM"]
[null,-1.0960000000000001,-33.048999999999999,149.535,58.482999999999997]
[null,-1.409,-34.893000000000001,140.828,65.173000000000002]
[null,-2.2770000000000001,-36.677,128.63999999999999,56.354999999999997]
[null,-1.5469999999999999,-35.930999999999997,137.82300000000001,60.573]
[null,0,0,86.89,26.602]
[]
[]
[]
[]
[]
[]
[null,-1.0960000000000001,-1.409,-2.2770000000000001,-1.5469999999999999,0]
[null,-33.048999999999999,-34.893000000000001,-36.677,-35.930999999999997,0]
[null,149.535,140.828,128.63999999999999,137.82300000000001,86.89]
[null,58.482999999999997,65.173000000000002,56.354999999999997,60.573,26.602]
[]
[null,"=-1096","=-1409","=-2277","=-1547","=0","=0","=0","=0","=0","=0"]
[null,-33.048999999999999,-34.893000000000001,-36.677,-35.930999999999997,0,0,0,0,0,0]
[null,"=149535","=140828","=128640","=137823","=86890","=0","=0","=0","=0","=0"]
[null,58.482999999999997,65.173000000000002,56.354999999999997,60.573,26.602,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1096,-1409,-2277,-1547,0,0,0,0,0,0,-6329]
[null,"Ann peak Heating load kBtu/hr",-33.048999999999999,-34.893000000000001,-36.677,-35.930999999999997,0,0,0,0,0,0,-140.55000000000001]
[null,"HLH",33.162879360948892,40.380592095835837,62.082504021593913,43.054743814533417,"","","","","","","33-62",45.030238349341865]
["Cooling","Ann Cool Energy kBtu",149535,140828,128640,137823,86890,0,0,0,0,0,643716]
[null,"Ann peak Cooling load kBtu/hr",58.482999999999997,65.173000000000002,56.354999999999997,60.573,26.602,0,0,0,0,0,267.18599999999998]
[null,"CLH",2556.8968760152525,2160.8334739846255,2282.6723449560823,2275.3206874349958,3266.295767235546,"","","","","","2161-3266",2409.2429992589432]
[]
["SCooper Rest 24 7days w setback - Baseline Design.SIM"]
[null,-6.6000000000000003E-2,-9.4960000000000004,215.39500000000001,64.628]
[null,-6.5000000000000002E-2,-9.01,206.321,68.506]
[null,-0.25700000000000001,-26.591999999999999,191.53399999999999,58.758000000000003]
[null,-7.5999999999999998E-2,-11.17,202.94200000000001,65.17]
[null,0,0,113.982,28.693000000000001]
[]
[]
[]
[]
[]
[]
[null,-6.6000000000000003E-2,-6.5000000000000002E-2,-0.25700000000000001,-7.5999999999999998E-2,0]
[null,-9.4960000000000004,-9.01,-26.591999999999999,-11.17,0]
[null,215.39500000000001,206.321,191.53399999999999,202.94200000000001,113.982]
[null,64.628,68.506,58.758000000000003,65.17,28.693000000000001]
[]
[null,"=-66","=-65","=-257","=-76","=0","=0","=0","=0","=0","=0"]
[null,-9.4960000000000004,-9.01,-26.591999999999999,-11.17,0,0,0,0,0,0]
[null,"=215395","=206321","=191534","=202942","=113982","=0","=0","=0","=0","=0"]
[null,64.628,68.506,58.758000000000003,65.17,28.693000000000001,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-66,-65,-257,-76,0,0,0,0,0,0,-464]
[null,"Ann peak Heating load kBtu/hr",-9.4960000000000004,-9.01,-26.591999999999999,-11.17,0,0,0,0,0,0,-56.268000000000001]
[null,"HLH",6.9502948609941022,7.2142064372918977,9.664560770156438,6.8039391226499557,"","","","","","","7-10",8.2462500888604531]
["Cooling","Ann Cool Energy kBtu",215395,206321,191534,202942,113982,0,0,0,0,0,930174]
[null,"Ann peak Cooling load kBtu/hr",64.628,68.506,58.758000000000003,65.17,28.693000000000001,0,0,0,0,0,285.755]
[null,"CLH",3332.8433496317384,3011.721601027647,3259.7093161782223,3114.040202547184,3972.4671522671033,"","","","","","3012-3972",3255.145141817291]
[]
["SCooper Rest 10-23 7day Hol1 w setback - Baseline Design.SIM"]
[null,-1.0820000000000001,-12.295999999999999,106.345,61.634]
[null,-3.06,-12.468,103.461,61.151000000000003]
[null,-5.0549999999999997,-13.172000000000001,96.537000000000006,58.33]
[null,-3.0939999999999999,-12.696,101.449,61.709000000000003]
[null,-1.9E-2,-10.943,61.384,29.462]
[]
[]
[]
[]
[]
[]
[null,-1.0820000000000001,-3.06,-5.0549999999999997,-3.0939999999999999,-1.9E-2]
[null,-12.295999999999999,-12.468,-13.172000000000001,-12.696,-10.943]
[null,106.345,103.461,96.537000000000006,101.449,61.384]
[null,61.634,61.151000000000003,58.33,61.709000000000003,29.462]
[]
[null,"=-1082","=-3060","=-5055","=-3094","=-19","=0","=0","=0","=0","=0"]
[null,-12.295999999999999,-12.468,-13.172000000000001,-12.696,-10.943,0,0,0,0,0]
[null,"=106345","=103461","=96537","=101449","=61384","=0","=0","=0","=0","=0"]
[null,61.634,61.151000000000003,58.33,61.709000000000003,29.462,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1082,-3060,-5055,-3094,-19,0,0,0,0,0,-12310]
[null,"Ann peak Heating load kBtu/hr",-12.295999999999999,-12.468,-13.172000000000001,-12.696,-10.943,0,0,0,0,0,-61.574999999999996]
[null,"HLH",87.996096291476903,245.42829643888354,383.76860006073485,243.69880277252679,1.7362697614913645,"","","","","","2-384",199.91879821356071]
["Cooling","Ann Cool Energy kBtu",106345,103461,96537,101449,61384,0,0,0,0,0,469176]
[null,"Ann peak Cooling load kBtu/hr",61.634,61.151000000000003,58.33,61.709000000000003,29.462,0,0,0,0,0,272.286]
[null,"CLH",1725.427523769348,1691.8938365684942,1655.0145722612722,1643.9903417653827,2083.4973864639196,"","","","","","1644-2083",1723.099975760781]
[]
["SCooper Rest 8-23 12-20 Hol2 w setback - Baseline Design.SIM"]
[null,-0.74099999999999999,-15.782999999999999,70.174999999999997,53.768999999999998]
[null,-0.68200000000000005,-19.59,62.527999999999999,47.896999999999998]
[null,-1.8149999999999999,-27.236000000000001,53.963999999999999,39.896000000000001]
[null,-1.131,-18.422999999999998,60.101999999999997,48.649000000000001]
[null,-0.48699999999999999,-9.7370000000000001,23.352,24.754000000000001]
[]
[]
[]
[]
[]
[]
[null,-0.74099999999999999,-0.68200000000000005,-1.8149999999999999,-1.131,-0.48699999999999999]
[null,-15.782999999999999,-19.59,-27.236000000000001,-18.422999999999998,-9.7370000000000001]
[null,70.174999999999997,62.527999999999999,53.963999999999999,60.101999999999997,23.352]
[null,53.768999999999998,47.896999999999998,39.896000000000001,48.649000000000001,24.754000000000001]
[]
[null,"=-741","=-682","=-1815","=-1131","=-487","=0","=0","=0","=0","=0"]
[null,-15.782999999999999,-19.59,-27.236000000000001,-18.422999999999998,-9.7370000000000001,0,0,0,0,0]
[null,"=70175","=62528","=53964","=60102","=23352","=0","=0","=0","=0","=0"]
[null,53.768999999999998,47.896999999999998,39.896000000000001,48.649000000000001,24.754000000000001,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-741,-682,-1815,-1131,-487,0,0,0,0,0,-4856]
[null,"Ann peak Heating load kBtu/hr",-15.782999999999999,-19.59,-27.236000000000001,-18.422999999999998,-9.7370000000000001,0,0,0,0,0,-90.768999999999991]
[null,"HLH",46.949249192168793,34.813680449208782,66.639741518578347,61.390652988112691,50.01540515559207,"","","","","","35-67",53.498441097731607]
["Cooling","Ann Cool Energy kBtu",70175,62528,53964,60102,23352,0,0,0,0,0,270121]
[null,"Ann peak Cooling load kBtu/hr",53.768999999999998,47.896999999999998,39.896000000000001,48.649000000000001,24.754000000000001,0,0,0,0,0,214.965]
[null,"CLH",1305.1200505867694,1305.4679833810051,1352.6168036895929,1235.4210775144402,943.36268885836625,"","","","","","943-1353",1256.5813039331983]
[]
[]
["SCooper Htl 9-18 w setback - Baseline Design.SIM"]
[null,-1.383,-17.823,46.198,40.887999999999998]
[null,-5.1630000000000003,-21.321999999999999,29.856999999999999,36.822000000000003]
[null,-5.976,-21.231000000000002,29.478999999999999,38.994]
[null,-4.0709999999999997,-20.213000000000001,40.325000000000003,46.491999999999997]
[null,-1.034,-8.8789999999999996,7.2149999999999999,10.946]
[null,-2.1360000000000001,-19.614999999999998,67.203000000000003,57.063000000000002]
[null,-4.3940000000000001,-21.533999999999999,43.042999999999999,46.293999999999997]
[null,-4.6639999999999997,-21.585999999999999,43.984000000000002,50.390999999999998]
[null,-4.5350000000000001,-22.068000000000001,57.113999999999997,62.756999999999998]
[null,-1.508,-11.894,7.06,12.683999999999999]
[]
[null,-1.383,-5.1630000000000003,-5.976,-4.0709999999999997,-1.034,-2.1360000000000001,-4.3940000000000001,-4.6639999999999997,-4.5350000000000001,-1.508]
[null,-17.823,-21.321999999999999,-21.231000000000002,-20.213000000000001,-8.8789999999999996,-19.614999999999998,-21.533999999999999,-21.585999999999999,-22.068000000000001,-11.894]
[null,46.198,29.856999999999999,29.478999999999999,40.325000000000003,7.2149999999999999,67.203000000000003,43.042999999999999,43.984000000000002,57.113999999999997,7.06]
[null,40.887999999999998,36.822000000000003,38.994,46.491999999999997,10.946,57.063000000000002,46.293999999999997,50.390999999999998,62.756999999999998,12.683999999999999]
[]
[null,"=-1383","=-5163","=-5976","=-4071","=-1034","=-2136","=-4394","=-4664","=-4535","=-1508"]
[null,-17.823,-21.321999999999999,-21.231000000000002,-20.213000000000001,-8.8789999999999996,-19.614999999999998,-21.533999999999999,-21.585999999999999,-22.068000000000001,-11.894]
[null,"=46198","=29857","=29479","=40325","=7215","=67203","=43043","=43984","=57114","=7060"]
[null,40.887999999999998,36.822000000000003,38.994,46.491999999999997,10.946,57.063000000000002,46.293999999999997,50.390999999999998,62.756999999999998,12.683999999999999]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1383,-5163,-5976,-4071,-1034,-2136,-4394,-4664,-4535,-1508,-34864]
[null,"Ann peak Heating load kBtu/hr",-17.823,-21.321999999999999,-21.231000000000002,-20.213000000000001,-8.8789999999999996,-19.614999999999998,-21.533999999999999,-21.585999999999999,-22.068000000000001,-11.894,-186.16499999999999]
[null,"HLH",77.596364248443024,242.14426414032457,281.475201356507,201.40503636273684,116.4545556932087,108.8962528677033,204.04941023497724,216.06596868340591,205.50117817654521,126.78661510005044,"78-281",187.2747294067091]
["Cooling","Ann Cool Energy kBtu",46198,29857,29479,40325,7215,67203,43043,43984,57114,7060,371478]
[null,"Ann peak Cooling load kBtu/hr",40.887999999999998,36.822000000000003,38.994,46.491999999999997,10.946,57.063000000000002,46.293999999999997,50.390999999999998,62.756999999999998,12.683999999999999,403.33100000000002]
[null,"CLH",1129.8669536294267,810.84677638368362,755.98810073344623,867.35352318678486,659.14489311163902,1177.6983334209558,929.77491683587516,872.85427953404383,910.08174386920984,556.60674865972885,"557-1178",921.0251629554881]
[]
["SCooper Htl 8-21 w setback - Baseline Design.SIM"]
[null,-2.633,-17.808,49.737000000000002,39.790999999999997]
[null,-6.8330000000000002,-20.896999999999998,33.292999999999999,33.305999999999997]
[null,-7.633,-20.995999999999999,32.837000000000003,35.497]
[null,-5.5209999999999999,-20.68,44.761000000000003,45.097999999999999]
[null,-1.169,-8.73,8.1310000000000002,10.098000000000001]
[null,-3.1030000000000002,-21.745000000000001,72.260000000000005,57.314999999999998]
[null,-5.83,-23.053999999999998,47.6,41.613]
[null,-6.0620000000000003,-23.597000000000001,48.575000000000003,45.713000000000001]
[null,-5.391,-23.759,63.643000000000001,62.204999999999998]
[null,-1.651,-11.718,8.2460000000000004,11.912000000000001]
[]
[null,-2.633,-6.8330000000000002,-7.633,-5.5209999999999999,-1.169,-3.1030000000000002,-5.83,-6.0620000000000003,-5.391,-1.651]
[null,-17.808,-20.896999999999998,-20.995999999999999,-20.68,-8.73,-21.745000000000001,-23.053999999999998,-23.597000000000001,-23.759,-11.718]
[null,49.737000000000002,33.292999999999999,32.837000000000003,44.761000000000003,8.1310000000000002,72.260000000000005,47.6,48.575000000000003,63.643000000000001,8.2460000000000004]
[null,39.790999999999997,33.305999999999997,35.497,45.097999999999999,10.098000000000001,57.314999999999998,41.613,45.713000000000001,62.204999999999998,11.912000000000001]
[]
[null,"=-2633","=-6833","=-7633","=-5521","=-1169","=-3103","=-5830","=-6062","=-5391","=-1651"]
[null,-17.808,-20.896999999999998,-20.995999999999999,-20.68,-8.73,-21.745000000000001,-23.053999999999998,-23.597000000000001,-23.759,-11.718]
[null,"=49737","=33293","=32837","=44761","=8131","=72260","=47600","=48575","=63643","=8246"]
[null,39.790999999999997,33.305999999999997,35.497,45.097999999999999,10.098000000000001,57.314999999999998,41.613,45.713000000000001,62.204999999999998,11.912000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-2633,-6833,-7633,-5521,-1169,-3103,-5830,-6062,-5391,-1651,-45826]
[null,"Ann peak Heating load kBtu/hr",-17.808,-20.896999999999998,-20.995999999999999,-20.68,-8.73,-21.745000000000001,-23.053999999999998,-23.597000000000001,-23.759,-11.718,-192.98400000000001]
[null,"HLH",147.85489667565139,326.98473465090683,363.54543722613835,266.97292069632493,133.90607101947307,142.69947114279145,252.88453196842198,256.89706318599821,226.90348920409107,140.89435057176993,"134-364",237.46010031919744]
["Cooling","Ann Cool Energy kBtu",49737,33293,32837,44761,8131,72260,47600,48575,63643,8246,409083]
[null,"Ann peak Cooling load kBtu/hr",39.790999999999997,33.305999999999997,35.497,45.097999999999999,10.098000000000001,57.314999999999998,41.613,45.713000000000001,62.204999999999998,11.912000000000001,382.548]
[null,"CLH",1249.9560202055743,999.60967993754889,925.06408992309207,992.52738480642154,805.20895226777577,1260.7519846462533,1143.8733088217625,1062.6080108503052,1023.1171127722852,692.24311618535921,"692-1261",1069.3638445371562]
[]
["SCooper Htl 9-22 7days w setback - Baseline Design.SIM"]
[null,-3.0990000000000002,-18.472999999999999,60.460999999999999,38.607999999999997]
[null,-7.6829999999999998,-20.954999999999998,40.993000000000002,32.668999999999997]
[null,-8.4710000000000001,-20.849,40.356999999999999,34.826000000000001]
[null,-6.3380000000000001,-23.957999999999998,54.341000000000001,44.847000000000001]
[null,-1.292,-6.1950000000000003,9.6199999999999992,8.3559999999999999]
[null,-2.6619999999999999,-19.146000000000001,85.268000000000001,58.398000000000003]
[null,-5.8710000000000004,-21.073,57.052,42.783000000000001]
[null,-6.0339999999999998,-21.132999999999999,58.095999999999997,46.929000000000002]
[null,-5.7380000000000004,-26.015999999999998,75.566000000000003,62.177]
[null,-2.278,-10.448,10.763,9.0329999999999995]
[]
[null,-3.0990000000000002,-7.6829999999999998,-8.4710000000000001,-6.3380000000000001,-1.292,-2.6619999999999999,-5.8710000000000004,-6.0339999999999998,-5.7380000000000004,-2.278]
[null,-18.472999999999999,-20.954999999999998,-20.849,-23.957999999999998,-6.1950000000000003,-19.146000000000001,-21.073,-21.132999999999999,-26.015999999999998,-10.448]
[null,60.460999999999999,40.993000000000002,40.356999999999999,54.341000000000001,9.6199999999999992,85.268000000000001,57.052,58.095999999999997,75.566000000000003,10.763]
[null,38.607999999999997,32.668999999999997,34.826000000000001,44.847000000000001,8.3559999999999999,58.398000000000003,42.783000000000001,46.929000000000002,62.177,9.0329999999999995]
[]
[null,"=-3099","=-7683","=-8471","=-6338","=-1292","=-2662","=-5871","=-6034","=-5738","=-2278"]
[null,-18.472999999999999,-20.954999999999998,-20.849,-23.957999999999998,-6.1950000000000003,-19.146000000000001,-21.073,-21.132999999999999,-26.015999999999998,-10.448]
[null,"=60461","=40993","=40357","=54341","=9620","=85268","=57052","=58096","=75566","=10763"]
[null,38.607999999999997,32.668999999999997,34.826000000000001,44.847000000000001,8.3559999999999999,58.398000000000003,42.783000000000001,46.929000000000002,62.177,9.0329999999999995]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-3099,-7683,-8471,-6338,-1292,-2662,-5871,-6034,-5738,-2278,-49466]
[null,"Ann peak Heating load kBtu/hr",-18.472999999999999,-20.954999999999998,-20.849,-23.957999999999998,-6.1950000000000003,-19.146000000000001,-21.073,-21.132999999999999,-26.015999999999998,-10.448,-188.24600000000001]
[null,"HLH",167.75835002435988,366.64280601288476,406.30246054966665,264.5462893396778,208.55528652138821,139.03687454298549,278.60295164428413,285.52500828088773,220.55658056580566,218.03215926493107,"139-406",262.77317977540025]
["Cooling","Ann Cool Energy kBtu",60461,40993,40357,54341,9620,85268,57052,58096,75566,10763,492517]
[null,"Ann peak Cooling load kBtu/hr",38.607999999999997,32.668999999999997,34.826000000000001,44.847000000000001,8.3559999999999999,58.398000000000003,42.783000000000001,46.929000000000002,62.177,9.0329999999999995,378.62599999999998]
[null,"CLH",1566.0225859925406,1254.7981266644219,1158.8181243898237,1211.6975494458939,1151.268549545237,1460.1184972088085,1333.5203234929761,1237.9552089326428,1215.3368608971164,1191.5199822871693,"1151-1566",1300.8007902257109]
[]
["SCooper Htl 8-22 7days w setback - Baseline Design.SIM"]
[null,-3.9390000000000001,-20.611000000000001,61.66,38.420999999999999]
[null,-8.4890000000000008,-21.75,42.174999999999997,32.125999999999998]
[null,-9.282,-23.847999999999999,41.488,33.073999999999998]
[null,-7.1779999999999999,-25.823,55.209000000000003,44.619]
[null,-1.3280000000000001,-5.9950000000000001,9.6760000000000002,7.17]
[null,-3.8450000000000002,-25.890999999999998,86.826999999999998,58.749000000000002]
[null,-6.9459999999999997,-26.238,58.639000000000003,40.360999999999997]
[null,-7.0869999999999997,-26.574000000000002,59.738999999999997,43.695]
[null,-6.601,-28.324999999999999,76.566999999999993,62.070999999999998]
[null,-2.3540000000000001,-10.206,10.81,8.6050000000000004]
[]
[null,-3.9390000000000001,-8.4890000000000008,-9.282,-7.1779999999999999,-1.3280000000000001,-3.8450000000000002,-6.9459999999999997,-7.0869999999999997,-6.601,-2.3540000000000001]
[null,-20.611000000000001,-21.75,-23.847999999999999,-25.823,-5.9950000000000001,-25.890999999999998,-26.238,-26.574000000000002,-28.324999999999999,-10.206]
[null,61.66,42.174999999999997,41.488,55.209000000000003,9.6760000000000002,86.826999999999998,58.639000000000003,59.738999999999997,76.566999999999993,10.81]
[null,38.420999999999999,32.125999999999998,33.073999999999998,44.619,7.17,58.749000000000002,40.360999999999997,43.695,62.070999999999998,8.6050000000000004]
[]
[null,"=-3939","=-8489","=-9282","=-7178","=-1328","=-3845","=-6946","=-7087","=-6601","=-2354"]
[null,-20.611000000000001,-21.75,-23.847999999999999,-25.823,-5.9950000000000001,-25.890999999999998,-26.238,-26.574000000000002,-28.324999999999999,-10.206]
[null,"=61660","=42175","=41488","=55209","=9676","=86827","=58639","=59739","=76567","=10810"]
[null,38.420999999999999,32.125999999999998,33.073999999999998,44.619,7.17,58.749000000000002,40.360999999999997,43.695,62.070999999999998,8.6050000000000004]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-3939,-8489,-9282,-7178,-1328,-3845,-6946,-7087,-6601,-2354,-57049]
[null,"Ann peak Heating load kBtu/hr",-20.611000000000001,-21.75,-23.847999999999999,-25.823,-5.9950000000000001,-25.890999999999998,-26.238,-26.574000000000002,-28.324999999999999,-10.206,-215.261]
[null,"HLH",191.11154238028237,390.29885057471262,389.21502851392154,277.96925221701582,221.51793160967472,148.5072032752694,264.73054348654625,266.68924512681565,233.04501323918799,230.64863805604548,"149-390",265.02246110535583]
["Cooling","Ann Cool Energy kBtu",61660,42175,41488,55209,9676,86827,58639,59739,76567,10810,502790]
[null,"Ann peak Cooling load kBtu/hr",38.420999999999999,32.125999999999998,33.073999999999998,44.619,7.17,58.749000000000002,40.360999999999997,43.695,62.070999999999998,8.6050000000000004,368.89099999999996]
[null,"CLH",1604.851513495224,1312.7996015688229,1254.3992259781098,1237.3428360115645,1349.5118549511856,1477.9315392602427,1452.8629122172395,1367.1815997253691,1233.5390117768363,1256.2463683904707,"1234-1605",1362.9771395886592]
[]
["SCooper Htl 5-23 7days w setback - Baseline Design.SIM"]
[null,-7.2640000000000002,-26.256,64.334000000000003,37.921999999999997]
[null,-12.358000000000001,-27.901,44.326999999999998,31.292999999999999]
[null,-13.025,-27.792999999999999,43.573,32.048000000000002]
[null,-10.555999999999999,-27.350999999999999,57.682000000000002,44.124000000000002]
[null,-1.349,-5.2939999999999996,10.422000000000001,5.71]
[null,-7.1,-29.388000000000002,90.414000000000001,59.552]
[null,-11.002000000000001,-31.3,61.457999999999998,39.182000000000002]
[null,-10.999000000000001,-31.068999999999999,62.649000000000001,42.466999999999999]
[null,-9.4540000000000006,-30.138999999999999,79.617999999999995,61.88]
[null,-2.4649999999999999,-8.3450000000000006,11.45,7.1070000000000002]
[]
[null,-7.2640000000000002,-12.358000000000001,-13.025,-10.555999999999999,-1.349,-7.1,-11.002000000000001,-10.999000000000001,-9.4540000000000006,-2.4649999999999999]
[null,-26.256,-27.901,-27.792999999999999,-27.350999999999999,-5.2939999999999996,-29.388000000000002,-31.3,-31.068999999999999,-30.138999999999999,-8.3450000000000006]
[null,64.334000000000003,44.326999999999998,43.573,57.682000000000002,10.422000000000001,90.414000000000001,61.457999999999998,62.649000000000001,79.617999999999995,11.45]
[null,37.921999999999997,31.292999999999999,32.048000000000002,44.124000000000002,5.71,59.552,39.182000000000002,42.466999999999999,61.88,7.1070000000000002]
[]
[null,"=-7264","=-12358","=-13025","=-10556","=-1349","=-7100","=-11002","=-10999","=-9454","=-2465"]
[null,-26.256,-27.901,-27.792999999999999,-27.350999999999999,-5.2939999999999996,-29.388000000000002,-31.3,-31.068999999999999,-30.138999999999999,-8.3450000000000006]
[null,"=64334","=44327","=43573","=57682","=10422","=90414","=61458","=62649","=79618","=11450"]
[null,37.921999999999997,31.292999999999999,32.048000000000002,44.124000000000002,5.71,59.552,39.182000000000002,42.466999999999999,61.88,7.1070000000000002]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-7264,-12358,-13025,-10556,-1349,-7100,-11002,-10999,-9454,-2465,-85572]
[null,"Ann peak Heating load kBtu/hr",-26.256,-27.901,-27.792999999999999,-27.350999999999999,-5.2939999999999996,-29.388000000000002,-31.3,-31.068999999999999,-30.138999999999999,-8.3450000000000006,-244.83599999999998]
[null,"HLH",276.66057282145033,442.92319271710693,468.64318353542262,385.94566926254981,254.81677370608239,241.59520892881446,351.50159744408944,354.01847500724193,313.67994956700619,295.38645895745952,"242-469",349.50742537862084]
["Cooling","Ann Cool Energy kBtu",64334,44327,43573,57682,10422,90414,61458,62649,79618,11450,525927]
[null,"Ann peak Cooling load kBtu/hr",37.921999999999997,31.292999999999999,32.048000000000002,44.124000000000002,5.71,59.552,39.182000000000002,42.466999999999999,61.88,7.1070000000000002,361.28500000000003]
[null,"CLH",1696.4822530457257,1416.5148755312689,1359.6168247628557,1307.270419726226,1825.2189141856393,1518.2361633530361,1568.5263641468021,1475.2395978053548,1286.6515837104073,1611.0876600534684,"1287-1825",1455.7122493322445]
[]
["SCooper Htl 24 7days w setback - Baseline Design.SIM"]
[null,-10.093999999999999,-22.568999999999999,66.811000000000007,37.610999999999997]
[null,-16.138999999999999,-24.207000000000001,46.026000000000003,30.856999999999999]
[null,-16.678000000000001,-24.082000000000001,45.281999999999996,31.678999999999998]
[null,-13.646000000000001,-23.59,59.993000000000002,43.825000000000003]
[null,-1.659,-4.4820000000000002,10.875999999999999,5.3719999999999999]
[null,-8.9659999999999993,-23.094000000000001,93.628,59.838000000000001]
[null,-14.271000000000001,-24.986000000000001,63.43,38.835000000000001]
[null,-14.069000000000001,-24.734999999999999,64.706000000000003,42.125]
[null,-11.512,-23.77,82.522999999999996,61.792000000000002]
[null,-2.944,-6.1870000000000003,11.975,7.03]
[]
[null,-10.093999999999999,-16.138999999999999,-16.678000000000001,-13.646000000000001,-1.659,-8.9659999999999993,-14.271000000000001,-14.069000000000001,-11.512,-2.944]
[null,-22.568999999999999,-24.207000000000001,-24.082000000000001,-23.59,-4.4820000000000002,-23.094000000000001,-24.986000000000001,-24.734999999999999,-23.77,-6.1870000000000003]
[null,66.811000000000007,46.026000000000003,45.281999999999996,59.993000000000002,10.875999999999999,93.628,63.43,64.706000000000003,82.522999999999996,11.975]
[null,37.610999999999997,30.856999999999999,31.678999999999998,43.825000000000003,5.3719999999999999,59.838000000000001,38.835000000000001,42.125,61.792000000000002,7.03]
[]
[null,"=-10094","=-16139","=-16678","=-13646","=-1659","=-8966","=-14271","=-14069","=-11512","=-2944"]
[null,-22.568999999999999,-24.207000000000001,-24.082000000000001,-23.59,-4.4820000000000002,-23.094000000000001,-24.986000000000001,-24.734999999999999,-23.77,-6.1870000000000003]
[null,"=66811","=46026","=45282","=59993","=10876","=93628","=63430","=64706","=82523","=11975"]
[null,37.610999999999997,30.856999999999999,31.678999999999998,43.825000000000003,5.3719999999999999,59.838000000000001,38.835000000000001,42.125,61.792000000000002,7.03]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-10094,-16139,-16678,-13646,-1659,-8966,-14271,-14069,-11512,-2944,-109978]
[null,"Ann peak Heating load kBtu/hr",-22.568999999999999,-24.207000000000001,-24.082000000000001,-23.59,-4.4820000000000002,-23.094000000000001,-24.986000000000001,-24.734999999999999,-23.77,-6.1870000000000003,-201.70200000000003]
[null,"HLH",447.25065355133148,666.70797703143717,692.55045262021429,578.46545146248411,370.14725568942436,388.23936953321208,571.15984951572875,568.78916515059632,484.30795119899034,475.8364312267658,"370-693",545.24992315395968]
["Cooling","Ann Cool Energy kBtu",66811,46026,45282,59993,10876,93628,63430,64706,82523,11975,545250]
[null,"Ann peak Cooling load kBtu/hr",37.610999999999997,30.856999999999999,31.678999999999998,43.825000000000003,5.3719999999999999,59.838000000000001,38.835000000000001,42.125,61.792000000000002,7.03,358.96399999999994]
[null,"CLH",1776.3686155645955,1491.5902388436984,1429.4011805928219,1368.9218482601254,2024.571854058079,1564.6913332664863,1633.3204583494271,1536.0474777448071,1335.4965044018643,1703.4139402560454,"1335-2025",1518.9545469740701]
[]
[]
["SCooper Rtl 9-18 w setback - Baseline Design.SIM"]
[null,-3.12,-92.635999999999996,153.62200000000001,139.988]
[null,-1.3420000000000001,-34.845999999999997,64.685000000000002,59.655999999999999]
[null,-3.1469999999999998,-81.995000000000005,105.08499999999999,106.18899999999999]
[null,-2.2480000000000002,-74.364999999999995,116.646,113.562]
[null,-2.2000000000000002,-41.140999999999998,55.027000000000001,50.814999999999998]
[null,-4.6130000000000004,-104.343,178.17699999999999,155.46299999999999]
[null,-2.6419999999999999,-44.366999999999997,23.341999999999999,32.552]
[]
[]
[]
[]
[null,-3.12,-1.3420000000000001,-3.1469999999999998,-2.2480000000000002,-2.2000000000000002,-4.6130000000000004,-2.6419999999999999]
[null,-92.635999999999996,-34.845999999999997,-81.995000000000005,-74.364999999999995,-41.140999999999998,-104.343,-44.366999999999997]
[null,153.62200000000001,64.685000000000002,105.08499999999999,116.646,55.027000000000001,178.17699999999999,23.341999999999999]
[null,139.988,59.655999999999999,106.18899999999999,113.562,50.814999999999998,155.46299999999999,32.552]
[]
[null,"=-3120","=-1342","=-3147","=-2248","=-2200","=-4613","=-2642","=0","=0","=0"]
[null,-92.635999999999996,-34.845999999999997,-81.995000000000005,-74.364999999999995,-41.140999999999998,-104.343,-44.366999999999997,0,0,0]
[null,"=153622","=64685","=105085","=116646","=55027","=178177","=23342","=0","=0","=0"]
[null,139.988,59.655999999999999,106.18899999999999,113.562,50.814999999999998,155.46299999999999,32.552,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-3120,-1342,-3147,-2248,-2200,-4613,-2642,0,0,0,-19312]
[null,"Ann peak Heating load kBtu/hr",-92.635999999999996,-34.845999999999997,-81.995000000000005,-74.364999999999995,-41.140999999999998,-104.343,-44.366999999999997,0,0,0,-473.69300000000004]
[null,"HLH",33.680210717215772,38.512311312632733,38.38038904811269,30.22927452430579,53.474636007875361,44.209961377380367,59.548763720783469,"","","","30-60",40.769021285938358]
["Cooling","Ann Cool Energy kBtu",153622,64685,105085,116646,55027,178177,23342,0,0,0,696584]
[null,"Ann peak Cooling load kBtu/hr",139.988,59.655999999999999,106.18899999999999,113.562,50.814999999999998,155.46299999999999,32.552,0,0,0,658.22500000000002]
[null,"CLH",1097.3940623482013,1084.2999865897814,989.60344291781644,1027.1569715221642,1082.8889107546984,1146.1055042035725,717.06807569427383,"","","","717-1146",1058.2764252345323]
[]
["SCooper Rtl 8-20 w setback - Baseline Design.SIM"]
[null,-2.5049999999999999,-69.834999999999994,185.46600000000001,137.10300000000001]
[null,-1.3380000000000001,-32.442,76.129000000000005,58.747]
[null,-2.379,-56.911999999999999,127.285,93.289000000000001]
[null,-1.6559999999999999,-55.648000000000003,140.20500000000001,106.932]
[null,-1.931,-32.332999999999998,65.010999999999996,49.113]
[null,-3.593,-72.126999999999995,215.04300000000001,166.41]
[null,-2.1880000000000002,-38.546999999999997,27.988,30.120999999999999]
[]
[]
[]
[]
[null,-2.5049999999999999,-1.3380000000000001,-2.379,-1.6559999999999999,-1.931,-3.593,-2.1880000000000002]
[null,-69.834999999999994,-32.442,-56.911999999999999,-55.648000000000003,-32.332999999999998,-72.126999999999995,-38.546999999999997]
[null,185.46600000000001,76.129000000000005,127.285,140.20500000000001,65.010999999999996,215.04300000000001,27.988]
[null,137.10300000000001,58.747,93.289000000000001,106.932,49.113,166.41,30.120999999999999]
[]
[null,"=-2505","=-1338","=-2379","=-1656","=-1931","=-3593","=-2188","=0","=0","=0"]
[null,-69.834999999999994,-32.442,-56.911999999999999,-55.648000000000003,-32.332999999999998,-72.126999999999995,-38.546999999999997,0,0,0]
[null,"=185466","=76129","=127285","=140205","=65011","=215043","=27988","=0","=0","=0"]
[null,137.10300000000001,58.747,93.289000000000001,106.932,49.113,166.41,30.120999999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-2505,-1338,-2379,-1656,-1931,-3593,-2188,0,0,0,-15590]
[null,"Ann peak Heating load kBtu/hr",-69.834999999999994,-32.442,-56.911999999999999,-55.648000000000003,-32.332999999999998,-72.126999999999995,-38.546999999999997,0,0,0,-357.84399999999994]
[null,"HLH",35.870265626118709,41.242833364157576,41.801377565364071,29.75848188614146,59.722265177991531,49.814909811859643,56.761875113497815,"","","","30-60",43.56647030549626]
["Cooling","Ann Cool Energy kBtu",185466,76129,127285,140205,65011,215043,27988,0,0,0,837127]
[null,"Ann peak Cooling load kBtu/hr",137.10300000000001,58.747,93.289000000000001,106.932,49.113,166.41,30.120999999999999,0,0,0,641.71500000000003]
[null,"CLH",1352.7493927922801,1295.8789384989873,1364.4159547213499,1311.160363595556,1323.702482031234,1292.2480620155038,929.18561800737029,"","","","929-1364",1304.515244306273]
[]
["SCooper Rtl 7-22 w setback - Baseline Design.SIM"]
[null,-2.4580000000000002,-69.503,219.01300000000001,134.411]
[null,-1.5289999999999999,-33.561,87.394000000000005,58.8]
[null,-1.9510000000000001,-57.557000000000002,151.07599999999999,92.695999999999998]
[null,-1.6120000000000001,-56.011000000000003,164.80199999999999,106.05]
[null,-1.889,-33.222000000000001,75.361000000000004,48.185000000000002]
[null,-3.1,-72.366,251.464,165.46600000000001]
[null,-1.8129999999999999,-38.725000000000001,33.011000000000003,30.181999999999999]
[]
[]
[]
[]
[null,-2.4580000000000002,-1.5289999999999999,-1.9510000000000001,-1.6120000000000001,-1.889,-3.1,-1.8129999999999999]
[null,-69.503,-33.561,-57.557000000000002,-56.011000000000003,-33.222000000000001,-72.366,-38.725000000000001]
[null,219.01300000000001,87.394000000000005,151.07599999999999,164.80199999999999,75.361000000000004,251.464,33.011000000000003]
[null,134.411,58.8,92.695999999999998,106.05,48.185000000000002,165.46600000000001,30.181999999999999]
[]
[null,"=-2458","=-1529","=-1951","=-1612","=-1889","=-3100","=-1813","=0","=0","=0"]
[null,-69.503,-33.561,-57.557000000000002,-56.011000000000003,-33.222000000000001,-72.366,-38.725000000000001,0,0,0]
[null,"=219013","=87394","=151076","=164802","=75361","=251464","=33011","=0","=0","=0"]
[null,134.411,58.8,92.695999999999998,106.05,48.185000000000002,165.46600000000001,30.181999999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-2458,-1529,-1951,-1612,-1889,-3100,-1813,0,0,0,-14352]
[null,"Ann peak Heating load kBtu/hr",-69.503,-33.561,-57.557000000000002,-56.011000000000003,-33.222000000000001,-72.366,-38.725000000000001,0,0,0,-360.94499999999999]
[null,"HLH",35.365379911658486,45.55883316945264,33.89683270497072,28.780061059434754,56.859912106435495,42.837796755382364,46.817301484828917,"","","","29-57",39.762290653700703]
["Cooling","Ann Cool Energy kBtu",219013,87394,151076,164802,75361,251464,33011,0,0,0,982121]
[null,"Ann peak Cooling load kBtu/hr",134.411,58.8,92.695999999999998,106.05,48.185000000000002,165.46600000000001,30.181999999999999,0,0,0,635.79000000000008]
[null,"CLH",1629.4276510107059,1486.2925170068029,1629.8006386467594,1554.002828854314,1563.9929438621978,1519.7321504115648,1093.7313630640779,"","","","1094-1630",1544.7254596643545]
[]
["SCooper Rtl 9-22 7days w setback - Baseline Design.SIM"]
[null,-2.7930000000000001,-98.07,229.82,129.80000000000001]
[null,-1.3580000000000001,-39.712000000000003,90.200999999999993,53.804000000000002]
[null,-2.5409999999999999,-76.103999999999999,157.80699999999999,88.572999999999993]
[null,-1.8420000000000001,-74.164000000000001,171.024,99.628]
[null,-2.1160000000000001,-39.04,78.608999999999995,47.438000000000002]
[null,-3.9740000000000002,-99.516999999999996,261.404,165.31800000000001]
[null,-2.5720000000000001,-42.087000000000003,35.476999999999997,36.520000000000003]
[]
[]
[]
[]
[null,-2.7930000000000001,-1.3580000000000001,-2.5409999999999999,-1.8420000000000001,-2.1160000000000001,-3.9740000000000002,-2.5720000000000001]
[null,-98.07,-39.712000000000003,-76.103999999999999,-74.164000000000001,-39.04,-99.516999999999996,-42.087000000000003]
[null,229.82,90.200999999999993,157.80699999999999,171.024,78.608999999999995,261.404,35.476999999999997]
[null,129.80000000000001,53.804000000000002,88.572999999999993,99.628,47.438000000000002,165.31800000000001,36.520000000000003]
[]
[null,"=-2793","=-1358","=-2541","=-1842","=-2116","=-3974","=-2572","=0","=0","=0"]
[null,-98.07,-39.712000000000003,-76.103999999999999,-74.164000000000001,-39.04,-99.516999999999996,-42.087000000000003,0,0,0]
[null,"=229820","=90201","=157807","=171024","=78609","=261404","=35477","=0","=0","=0"]
[null,129.80000000000001,53.804000000000002,88.572999999999993,99.628,47.438000000000002,165.31800000000001,36.520000000000003,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-2793,-1358,-2541,-1842,-2116,-3974,-2572,0,0,0,-17196]
[null,"Ann peak Heating load kBtu/hr",-98.07,-39.712000000000003,-76.103999999999999,-74.164000000000001,-39.04,-99.516999999999996,-42.087000000000003,0,0,0,-468.69399999999996]
[null,"HLH",28.479657387580303,34.196212731668005,33.388520971302427,24.836848066447331,54.200819672131146,39.932875790066021,61.111507116211655,"","","","25-61",36.689183134411792]
["Cooling","Ann Cool Energy kBtu",229820,90201,157807,171024,78609,261404,35477,0,0,0,1024342]
[null,"Ann peak Cooling load kBtu/hr",129.80000000000001,53.804000000000002,88.572999999999993,99.628,47.438000000000002,165.31800000000001,36.520000000000003,0,0,0,621.08100000000002]
[null,"CLH",1770.5701078582433,1676.4738681138949,1781.6603253813241,1716.6258481551372,1657.0892533412032,1581.2192259766025,971.4403066812705,"","","","971-1782",1649.2889011256179]
[]
["SCooper Rtl 8-22 7days w setback - Baseline Design.SIM"]
[null,-1.923,-80.195999999999998,258.584,133.64599999999999]
[null,-1.0669999999999999,-29.273,100.325,57.826999999999998]
[null,-1.702,-58.645000000000003,178.595,97.191999999999993]
[null,-1.167,-52.91,193.22399999999999,103.108]
[null,-1.66,-28.766999999999999,87.644000000000005,47.360999999999997]
[null,-2.6629999999999998,-88.075000000000003,291.726,166.57499999999999]
[null,-1.857,-36.756999999999998,39.978999999999999,33.042999999999999]
[]
[]
[]
[]
[null,-1.923,-1.0669999999999999,-1.702,-1.167,-1.66,-2.6629999999999998,-1.857]
[null,-80.195999999999998,-29.273,-58.645000000000003,-52.91,-28.766999999999999,-88.075000000000003,-36.756999999999998]
[null,258.584,100.325,178.595,193.22399999999999,87.644000000000005,291.726,39.978999999999999]
[null,133.64599999999999,57.826999999999998,97.191999999999993,103.108,47.360999999999997,166.57499999999999,33.042999999999999]
[]
[null,"=-1923","=-1067","=-1702","=-1167","=-1660","=-2663","=-1857","=0","=0","=0"]
[null,-80.195999999999998,-29.273,-58.645000000000003,-52.91,-28.766999999999999,-88.075000000000003,-36.756999999999998,0,0,0]
[null,"=258584","=100325","=178595","=193224","=87644","=291726","=39979","=0","=0","=0"]
[null,133.64599999999999,57.826999999999998,97.191999999999993,103.108,47.360999999999997,166.57499999999999,33.042999999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1923,-1067,-1702,-1167,-1660,-2663,-1857,0,0,0,-12039]
[null,"Ann peak Heating load kBtu/hr",-80.195999999999998,-29.273,-58.645000000000003,-52.91,-28.766999999999999,-88.075000000000003,-36.756999999999998,0,0,0,-374.62299999999999]
[null,"HLH",23.978752057459225,36.449970963003452,29.022082018927442,22.056322056322056,57.705009211944244,30.235594663638942,50.520989199336185,"","","","22-58",32.136307701342417]
["Cooling","Ann Cool Energy kBtu",258584,100325,178595,193224,87644,291726,39979,0,0,0,1150077]
[null,"Ann peak Cooling load kBtu/hr",133.64599999999999,57.826999999999998,97.191999999999993,103.108,47.360999999999997,166.57499999999999,33.042999999999999,0,0,0,638.75199999999995]
[null,"CLH",1934.8427936488936,1734.9162156086259,1837.5483578895385,1873.9961981611514,1850.5521420578114,1751.319225574066,1209.908301304361,"","","","1210-1935",1800.5062997845801]
[]
["SCooper Rtl 5-23 7days w setback - Baseline Design.SIM"]
[null,-1.742,-55.045000000000002,311.29399999999998,144.9]
[null,-1.5840000000000001,-21.643999999999998,118.057,53.277999999999999]
[null,-1.093,-33.753,215.29,102.22199999999999]
[null,-1.0089999999999999,-33.414000000000001,231.09700000000001,101.655]
[null,-1.7470000000000001,-23.474,103.121,47.332000000000001]
[null,-2.0920000000000001,-47.343000000000004,347.99400000000003,164.57599999999999]
[null,-1.101,-33.194000000000003,47.493000000000002,34.999000000000002]
[]
[]
[]
[]
[null,-1.742,-1.5840000000000001,-1.093,-1.0089999999999999,-1.7470000000000001,-2.0920000000000001,-1.101]
[null,-55.045000000000002,-21.643999999999998,-33.753,-33.414000000000001,-23.474,-47.343000000000004,-33.194000000000003]
[null,311.29399999999998,118.057,215.29,231.09700000000001,103.121,347.99400000000003,47.493000000000002]
[null,144.9,53.277999999999999,102.22199999999999,101.655,47.332000000000001,164.57599999999999,34.999000000000002]
[]
[null,"=-1742","=-1584","=-1093","=-1009","=-1747","=-2092","=-1101","=0","=0","=0"]
[null,-55.045000000000002,-21.643999999999998,-33.753,-33.414000000000001,-23.474,-47.343000000000004,-33.194000000000003,0,0,0]
[null,"=311294","=118057","=215290","=231097","=103121","=347994","=47493","=0","=0","=0"]
[null,144.9,53.277999999999999,102.22199999999999,101.655,47.332000000000001,164.57599999999999,34.999000000000002,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1742,-1584,-1093,-1009,-1747,-2092,-1101,0,0,0,-10368]
[null,"Ann peak Heating load kBtu/hr",-55.045000000000002,-21.643999999999998,-33.753,-33.414000000000001,-23.474,-47.343000000000004,-33.194000000000003,0,0,0,-247.86700000000002]
[null,"HLH",31.646834408211461,73.18425429680282,32.382306757917817,30.196923445262463,74.422765613018655,44.18815875631033,33.168644935831772,"","","","30-74",41.828884038617481]
["Cooling","Ann Cool Energy kBtu",311294,118057,215290,231097,103121,347994,47493,0,0,0,1374346]
[null,"Ann peak Cooling load kBtu/hr",144.9,53.277999999999999,102.22199999999999,101.655,47.332000000000001,164.57599999999999,34.999000000000002,0,0,0,648.96199999999999]
[null,"CLH",2148.3367839889579,2215.8677127519804,2106.1024045704448,2273.3461216860951,2178.674047156258,2114.4881392183552,1356.9816280465154,"","","","1357-2273",2117.7603619318234]
[]
["SCooper Rtl 24 7days w setback - Baseline Design.SIM"]
[null,-0.218,-36.164999999999999,451.19299999999998,132.619]
[null,-0.45700000000000002,-14.884,163.32900000000001,58.476999999999997]
[null,-1.0999999999999999E-2,-5.1820000000000004,313.16800000000001,90.036000000000001]
[null,-6.0000000000000001E-3,-2.7480000000000002,334.46800000000002,106.69799999999999]
[null,-0.53400000000000003,-21.853999999999999,144.643,47.143000000000001]
[null,-0.2,-24.661999999999999,495.4,167.11699999999999]
[null,-5.0000000000000001E-3,-1.016,61.529000000000003,17.855]
[]
[]
[]
[]
[null,-0.218,-0.45700000000000002,-1.0999999999999999E-2,-6.0000000000000001E-3,-0.53400000000000003,-0.2,-5.0000000000000001E-3]
[null,-36.164999999999999,-14.884,-5.1820000000000004,-2.7480000000000002,-21.853999999999999,-24.661999999999999,-1.016]
[null,451.19299999999998,163.32900000000001,313.16800000000001,334.46800000000002,144.643,495.4,61.529000000000003]
[null,132.619,58.476999999999997,90.036000000000001,106.69799999999999,47.143000000000001,167.11699999999999,17.855]
[]
[null,"=-218","=-457","=-11","=-6","=-534","=-200","=-5","=0","=0","=0"]
[null,-36.164999999999999,-14.884,-5.1820000000000004,-2.7480000000000002,-21.853999999999999,-24.661999999999999,-1.016,0,0,0]
[null,"=451193","=163329","=313168","=334468","=144643","=495400","=61529","=0","=0","=0"]
[null,132.619,58.476999999999997,90.036000000000001,106.69799999999999,47.143000000000001,167.11699999999999,17.855,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-218,-457,-11,-6,-534,-200,-5,0,0,0,-1431]
[null,"Ann peak Heating load kBtu/hr",-36.164999999999999,-14.884,-5.1820000000000004,-2.7480000000000002,-21.853999999999999,-24.661999999999999,-1.016,0,0,0,-106.51100000000001]
[null,"HLH",6.0279275542651733,30.704111797903789,2.1227325357005018,2.1834061135371177,24.43488606204814,8.1096423647717142,4.9212598425196852,"","","","2-31",13.435232041760944]
["Cooling","Ann Cool Energy kBtu",451193,163329,313168,334468,144643,495400,61529,0,0,0,1963730]
[null,"Ann peak Cooling load kBtu/hr",132.619,58.476999999999997,90.036000000000001,106.69799999999999,47.143000000000001,167.11699999999999,17.855,0,0,0,619.94499999999994]
[null,"CLH",3402.1746506910777,2793.0468389281259,3478.2531431871694,3134.7166769761384,3068.1755509831787,2964.3902176319584,3446.0375245029404,"","","","2793-3478",3167.5874472735486]
[]
["SCooper Rtl 10-23 7day Hol1 w setback - Baseline Design.SIM"]
[null,-2.6890000000000001,-38.326000000000001,222.48699999999999,132.06200000000001]
[null,-2.0009999999999999,-11.917,87.331999999999994,56.472999999999999]
[null,-2.1230000000000002,-32.103999999999999,158.374,98.950999999999993]
[null,-1.4330000000000001,-20.585999999999999,168.65600000000001,100.807]
[null,-2.371,-19.68,79.718999999999994,47.085999999999999]
[null,-4.508,-49.24,256.471,166.101]
[null,-0.38300000000000001,-39.564,35.906999999999996,30.126999999999999]
[]
[]
[]
[]
[null,-2.6890000000000001,-2.0009999999999999,-2.1230000000000002,-1.4330000000000001,-2.371,-4.508,-0.38300000000000001]
[null,-38.326000000000001,-11.917,-32.103999999999999,-20.585999999999999,-19.68,-49.24,-39.564]
[null,222.48699999999999,87.331999999999994,158.374,168.65600000000001,79.718999999999994,256.471,35.906999999999996]
[null,132.06200000000001,56.472999999999999,98.950999999999993,100.807,47.085999999999999,166.101,30.126999999999999]
[]
[null,"=-2689","=-2001","=-2123","=-1433","=-2371","=-4508","=-383","=0","=0","=0"]
[null,-38.326000000000001,-11.917,-32.103999999999999,-20.585999999999999,-19.68,-49.24,-39.564,0,0,0]
[null,"=222487","=87332","=158374","=168656","=79719","=256471","=35907","=0","=0","=0"]
[null,132.06200000000001,56.472999999999999,98.950999999999993,100.807,47.085999999999999,166.101,30.126999999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-2689,-2001,-2123,-1433,-2371,-4508,-383,0,0,0,-15508]
[null,"Ann peak Heating load kBtu/hr",-38.326000000000001,-11.917,-32.103999999999999,-20.585999999999999,-19.68,-49.24,-39.564,0,0,0,-211.417]
[null,"HLH",70.161248238793505,167.91138709406729,66.128831298280588,69.610414845040324,120.47764227642277,91.551584077985368,9.6805176423010817,"","","","10-168",73.352663220081638]
["Cooling","Ann Cool Energy kBtu",222487,87332,158374,168656,79719,256471,35907,0,0,0,1008946]
[null,"Ann peak Cooling load kBtu/hr",132.06200000000001,56.472999999999999,98.950999999999993,100.807,47.085999999999999,166.101,30.126999999999999,0,0,0,631.60699999999997]
[null,"CLH",1684.7162696309308,1546.4381208719212,1600.5295550322887,1673.0584185622031,1693.0510130399696,1544.0665619111264,1191.8544826899461,"","","","1192-1693",1597.4268809560376]
[]
["SCooper Rtl 9-24 10-18 Hol2 w setback - Baseline Design.SIM"]
[null,-3.351,-105.37,234.703,127.621]
[null,-1.351,-35.695999999999998,92.132000000000005,53.557000000000002]
[null,-3.7850000000000001,-87.741,161.19399999999999,100.199]
[null,-2.7839999999999998,-78.135000000000005,174.18899999999999,101.289]
[null,-2.42,-44.953000000000003,81.180999999999997,48.21]
[null,-5.226,-119.57299999999999,267.06799999999998,164.23099999999999]
[null,-3.5870000000000002,-45.755000000000003,35.807000000000002,31.626999999999999]
[]
[]
[]
[]
[null,-3.351,-1.351,-3.7850000000000001,-2.7839999999999998,-2.42,-5.226,-3.5870000000000002]
[null,-105.37,-35.695999999999998,-87.741,-78.135000000000005,-44.953000000000003,-119.57299999999999,-45.755000000000003]
[null,234.703,92.132000000000005,161.19399999999999,174.18899999999999,81.180999999999997,267.06799999999998,35.807000000000002]
[null,127.621,53.557000000000002,100.199,101.289,48.21,164.23099999999999,31.626999999999999]
[]
[null,"=-3351","=-1351","=-3785","=-2784","=-2420","=-5226","=-3587","=0","=0","=0"]
[null,-105.37,-35.695999999999998,-87.741,-78.135000000000005,-44.953000000000003,-119.57299999999999,-45.755000000000003,0,0,0]
[null,"=234703","=92132","=161194","=174189","=81181","=267068","=35807","=0","=0","=0"]
[null,127.621,53.557000000000002,100.199,101.289,48.21,164.23099999999999,31.626999999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-3351,-1351,-3785,-2784,-2420,-5226,-3587,0,0,0,-22504]
[null,"Ann peak Heating load kBtu/hr",-105.37,-35.695999999999998,-87.741,-78.135000000000005,-44.953000000000003,-119.57299999999999,-45.755000000000003,0,0,0,-517.22299999999996]
[null,"HLH",31.802220745942865,37.847377857463023,43.138327577757266,35.630639278172389,53.834004404600357,43.705518804412371,78.395803737296461,"","","","32-78",43.509279363060038]
["Cooling","Ann Cool Energy kBtu",234703,92132,161194,174189,81181,267068,35807,0,0,0,1046274]
[null,"Ann peak Cooling load kBtu/hr",127.621,53.557000000000002,100.199,101.289,48.21,164.23099999999999,31.626999999999999,0,0,0,626.73399999999992]
[null,"CLH",1839.0625367298487,1720.2606568702504,1608.7386101657701,1719.7227734502264,1683.9037544077992,1626.172890623573,1132.1655547475259,"","","","1132-1839",1669.4067977802388]
[]
[]
["SCooper Sch 7-16 w setback - Baseline Design.SIM"]
[null,-1.4179999999999999,-230.233,455.43299999999999,425.74400000000003]
[null,-1.333,-108.14400000000001,184.554,178.553]
[null,-1.528,-162.91800000000001,273.15100000000001,268.32400000000001]
[null,-1.411,-159.64400000000001,281.274,268.88400000000001]
[null,-1.5209999999999999,-110.697,178.69900000000001,175.541]
[null,-2.573,-259.11799999999999,454.46100000000001,437.70699999999999]
[null,-1.72,-1389.701,1291.5550000000001,1421.3989999999999]
[]
[]
[]
[]
[null,-1.4179999999999999,-1.333,-1.528,-1.411,-1.5209999999999999,-2.573,-1.72]
[null,-230.233,-108.14400000000001,-162.91800000000001,-159.64400000000001,-110.697,-259.11799999999999,-1389.701]
[null,455.43299999999999,184.554,273.15100000000001,281.274,178.69900000000001,454.46100000000001,1291.5550000000001]
[null,425.74400000000003,178.553,268.32400000000001,268.88400000000001,175.541,437.70699999999999,1421.3989999999999]
[]
[null,"=-1418","=-1333","=-1528","=-1411","=-1521","=-2573","=-1720","=0","=0","=0"]
[null,-230.233,-108.14400000000001,-162.91800000000001,-159.64400000000001,-110.697,-259.11799999999999,-1389.701,0,0,0]
[null,"=455433","=184554","=273151","=281274","=178699","=454461","=1291555","=0","=0","=0"]
[null,425.74400000000003,178.553,268.32400000000001,268.88400000000001,175.541,437.70699999999999,1421.3989999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1418,-1333,-1528,-1411,-1521,-2573,-1720,0,0,0,-11504]
[null,"Ann peak Heating load kBtu/hr",-230.233,-108.14400000000001,-162.91800000000001,-159.64400000000001,-110.697,-259.11799999999999,-1389.701,0,0,0,-2420.4549999999999]
[null,"HLH",6.1589780787289401,12.326157715638407,9.3789513743110025,8.838415474430608,13.740209761782161,9.9298389150888795,1.2376763059104081,"","","","1-14",4.7528253985304421]
["Cooling","Ann Cool Energy kBtu",455433,184554,273151,281274,178699,454461,1291555,0,0,0,3119127]
[null,"Ann peak Cooling load kBtu/hr",425.74400000000003,178.553,268.32400000000001,268.88400000000001,175.541,437.70699999999999,1421.3989999999999,0,0,0,3176.152]
[null,"CLH",1069.7343943778419,1033.6090684558646,1017.9894455956231,1046.0793502030615,1017.9900991791092,1038.2767467735266,908.65056187601101,"","","","909-1070",982.04588445389265]
[]
["SCooper Sch 6-20 w setback - Baseline Design.SIM"]
[null,-1.2849999999999999,-223.38200000000001,610.28899999999999,427.41199999999998]
[null,-1.232,-106.117,245.31100000000001,177.102]
[null,-1.383,-159.84,366.875,271.47399999999999]
[null,-1.3049999999999999,-155.06399999999999,374.91800000000001,266.81299999999999]
[null,-1.353,-108.383,239.44,177.369]
[null,-2.1880000000000002,-254.02799999999999,613.71199999999999,465.61]
[null,-1.0349999999999999,-720.13099999999997,1800.23,1468.0419999999999]
[]
[]
[]
[]
[null,-1.2849999999999999,-1.232,-1.383,-1.3049999999999999,-1.353,-2.1880000000000002,-1.0349999999999999]
[null,-223.38200000000001,-106.117,-159.84,-155.06399999999999,-108.383,-254.02799999999999,-720.13099999999997]
[null,610.28899999999999,245.31100000000001,366.875,374.91800000000001,239.44,613.71199999999999,1800.23]
[null,427.41199999999998,177.102,271.47399999999999,266.81299999999999,177.369,465.61,1468.0419999999999]
[]
[null,"=-1285","=-1232","=-1383","=-1305","=-1353","=-2188","=-1035","=0","=0","=0"]
[null,-223.38200000000001,-106.117,-159.84,-155.06399999999999,-108.383,-254.02799999999999,-720.13099999999997,0,0,0]
[null,"=610289","=245311","=366875","=374918","=239440","=613712","=1800230","=0","=0","=0"]
[null,427.41199999999998,177.102,271.47399999999999,266.81299999999999,177.369,465.61,1468.0419999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1285,-1232,-1383,-1305,-1353,-2188,-1035,0,0,0,-9781]
[null,"Ann peak Heating load kBtu/hr",-223.38200000000001,-106.117,-159.84,-155.06399999999999,-108.383,-254.02799999999999,-720.13099999999997,0,0,0,-1726.9450000000002]
[null,"HLH",5.7524778182664669,11.609826889188348,8.6524024024024015,8.4158798947531341,12.483507561148889,8.613223739115373,1.4372385024391396,"","","","1-12",5.6637588342419702]
["Cooling","Ann Cool Energy kBtu",610289,245311,366875,374918,239440,613712,1800230,0,0,0,4250775]
[null,"Ann peak Cooling load kBtu/hr",427.41199999999998,177.102,271.47399999999999,266.81299999999999,177.369,465.61,1468.0419999999999,0,0,0,3253.8219999999997]
[null,"CLH",1427.8705324136899,1385.1396370453185,1351.418552052867,1405.1714121875621,1349.954050595087,1318.0816563218143,1226.279629601878,"","","","1226-1428",1306.394449358324]
[]
["SCooper Sch 7-21 7days w setback - Baseline Design.SIM"]
[null,-9.0980000000000008,-537.87099999999998,646.34400000000005,428.78500000000003]
[null,-6.25,-214.54,259.91300000000001,175.68899999999999]
[null,-8.7449999999999992,-311.33999999999997,387.28899999999999,270.60700000000003]
[null,-7.6550000000000002,-316.50700000000001,396.12900000000002,266.09899999999999]
[null,-7.0679999999999996,-209.17,253.637,176.87700000000001]
[null,-14.09,-568.298,648.10599999999999,463.35]
[null,-7.9269999999999996,-1465.768,1879.21,1460.9949999999999]
[]
[]
[]
[]
[null,-9.0980000000000008,-6.25,-8.7449999999999992,-7.6550000000000002,-7.0679999999999996,-14.09,-7.9269999999999996]
[null,-537.87099999999998,-214.54,-311.33999999999997,-316.50700000000001,-209.17,-568.298,-1465.768]
[null,646.34400000000005,259.91300000000001,387.28899999999999,396.12900000000002,253.637,648.10599999999999,1879.21]
[null,428.78500000000003,175.68899999999999,270.60700000000003,266.09899999999999,176.87700000000001,463.35,1460.9949999999999]
[]
[null,"=-9098","=-6250","=-8745","=-7655","=-7068","=-14090","=-7927","=0","=0","=0"]
[null,-537.87099999999998,-214.54,-311.33999999999997,-316.50700000000001,-209.17,-568.298,-1465.768,0,0,0]
[null,"=646344","=259913","=387289","=396129","=253637","=648106","=1879210","=0","=0","=0"]
[null,428.78500000000003,175.68899999999999,270.60700000000003,266.09899999999999,176.87700000000001,463.35,1460.9949999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-9098,-6250,-8745,-7655,-7068,-14090,-7927,0,0,0,-60833]
[null,"Ann peak Heating load kBtu/hr",-537.87099999999998,-214.54,-311.33999999999997,-316.50700000000001,-209.17,-568.298,-1465.768,0,0,0,-3623.4940000000001]
[null,"HLH",16.914836457068702,29.132096578726578,28.088263634611682,24.185878985298903,33.79069656260458,24.793330259828469,5.4080864093089769,"","","","5-34",16.788491991431474]
["Cooling","Ann Cool Energy kBtu",646344,259913,387289,396129,253637,648106,1879210,0,0,0,4470628]
[null,"Ann peak Cooling load kBtu/hr",428.78500000000003,175.68899999999999,270.60700000000003,266.09899999999999,176.87700000000001,463.35,1460.9949999999999,0,0,0,3242.402]
[null,"CLH",1507.3848198980841,1479.3925629948376,1431.1861851319441,1488.6527194765858,1433.9738914612979,1398.7396136829609,1286.2535463844847,"","","","1286-1507",1378.801271403114]
[]
["SCooper Sch 8-22 7days 12mths w setback - Baseline Design.SIM"]
[null,-7.9329999999999998,-538.36599999999999,866.02099999999996,443.709]
[null,-5.5490000000000004,-218.34,347.84800000000001,179.59100000000001]
[null,-7.98,-315.06700000000001,524.26099999999997,278.95800000000003]
[null,-6.8440000000000003,-321.31700000000001,532.55700000000002,271.21800000000002]
[null,-6.5750000000000002,-212.25399999999999,342.28300000000002,183.04599999999999]
[null,-12.989000000000001,-574.53300000000002,865.67700000000002,455.50400000000002]
[null,-6.5739999999999998,-172.166,2637.3760000000002,1432.721]
[]
[]
[]
[]
[null,-7.9329999999999998,-5.5490000000000004,-7.98,-6.8440000000000003,-6.5750000000000002,-12.989000000000001,-6.5739999999999998]
[null,-538.36599999999999,-218.34,-315.06700000000001,-321.31700000000001,-212.25399999999999,-574.53300000000002,-172.166]
[null,866.02099999999996,347.84800000000001,524.26099999999997,532.55700000000002,342.28300000000002,865.67700000000002,2637.3760000000002]
[null,443.709,179.59100000000001,278.95800000000003,271.21800000000002,183.04599999999999,455.50400000000002,1432.721]
[]
[null,"=-7933","=-5549","=-7980","=-6844","=-6575","=-12989","=-6574","=0","=0","=0"]
[null,-538.36599999999999,-218.34,-315.06700000000001,-321.31700000000001,-212.25399999999999,-574.53300000000002,-172.166,0,0,0]
[null,"=866021","=347848","=524261","=532557","=342283","=865677","=2637376","=0","=0","=0"]
[null,443.709,179.59100000000001,278.95800000000003,271.21800000000002,183.04599999999999,455.50400000000002,1432.721,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-7933,-5549,-7980,-6844,-6575,-12989,-6574,0,0,0,-54444]
[null,"Ann peak Heating load kBtu/hr",-538.36599999999999,-218.34,-315.06700000000001,-321.31700000000001,-212.25399999999999,-574.53300000000002,-172.166,0,0,0,-2352.0430000000001]
[null,"HLH",14.735328754044646,25.414491160575249,25.327946119396827,21.29983785482872,30.977036946300188,22.607926785754689,38.184078157127423,"","","","15-38",23.147535993176994]
["Cooling","Ann Cool Energy kBtu",866021,347848,524261,532557,342283,865677,2637376,0,0,0,6116023]
[null,"Ann peak Cooling load kBtu/hr",443.709,179.59100000000001,278.95800000000003,271.21800000000002,183.04599999999999,455.50400000000002,1432.721,0,0,0,3244.7470000000003]
[null,"CLH",1951.7769529128325,1936.8899332371889,1879.354598183239,1963.5754264097513,1869.9288703386035,1900.481664266395,1840.8161812383569,"","","","1841-1964",1884.8998088294709]
[]
["SCooper Sch 5-23 7days 12 mths w setback - Baseline Design.SIM"]
[null,-11.763999999999999,-538.72900000000004,1012.215,435.28199999999998]
[null,-7.3559999999999999,-219.48699999999999,405.27699999999999,172.376]
[null,-10.631,-314.71499999999997,612.48800000000006,274.00200000000001]
[null,-9.1869999999999994,-323.577,620.81500000000005,264.94799999999998]
[null,-8.125,-211.233,399.66300000000001,180.21199999999999]
[null,-16.254000000000001,-253.548,1013.354,448.31599999999997]
[null,-9.9,-271.23,3089.1179999999999,1426.752]
[]
[]
[]
[]
[null,-11.763999999999999,-7.3559999999999999,-10.631,-9.1869999999999994,-8.125,-16.254000000000001,-9.9]
[null,-538.72900000000004,-219.48699999999999,-314.71499999999997,-323.577,-211.233,-253.548,-271.23]
[null,1012.215,405.27699999999999,612.48800000000006,620.81500000000005,399.66300000000001,1013.354,3089.1179999999999]
[null,435.28199999999998,172.376,274.00200000000001,264.94799999999998,180.21199999999999,448.31599999999997,1426.752]
[]
[null,"=-11764","=-7356","=-10631","=-9187","=-8125","=-16254","=-9900","=0","=0","=0"]
[null,-538.72900000000004,-219.48699999999999,-314.71499999999997,-323.577,-211.233,-253.548,-271.23,0,0,0]
[null,"=1012215","=405277","=612488","=620815","=399663","=1013354","=3089118","=0","=0","=0"]
[null,435.28199999999998,172.376,274.00200000000001,264.94799999999998,180.21199999999999,448.31599999999997,1426.752,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-11764,-7356,-10631,-9187,-8125,-16254,-9900,0,0,0,-73217]
[null,"Ann peak Heating load kBtu/hr",-538.72900000000004,-219.48699999999999,-314.71499999999997,-323.577,-211.233,-253.548,-271.23,0,0,0,-2132.5190000000002]
[null,"HLH",21.836582029183504,33.514513388036647,33.779768997346807,28.392005612265397,38.464633840356385,64.106204742297322,36.500387125317992,"","","","22-64",34.333574519148478]
["Cooling","Ann Cool Energy kBtu",1012215,405277,612488,620815,399663,1013354,3089118,0,0,0,7152930]
[null,"Ann peak Cooling load kBtu/hr",435.28199999999998,172.376,274.00200000000001,264.94799999999998,180.21199999999999,448.31599999999997,1426.752,0,0,0,3201.8879999999999]
[null,"CLH",2325.4235185465973,2351.1219659349331,2235.3413478733733,2343.1579026827908,2217.7379974696469,2260.35653423032,2165.1401224599649,"","","","2165-2351",2233.9725811771054]
[]
["SCooper Sch 24h 7days 12 mths w setback - Baseline Design.SIM"]
[null,-12.287000000000001,-243.56800000000001,1218.585,440.98700000000002]
[null,-7.407,-98.566999999999993,486.53,175.809]
[null,-10.263999999999999,-146.857,737.03399999999999,276.822]
[null,-9.3919999999999995,-147.33699999999999,746.11800000000005,270.16300000000001]
[null,-8.0879999999999992,-98.022000000000006,480.31599999999997,181.86600000000001]
[null,-16.722999999999999,-246.36699999999999,1221.2329999999999,455.04399999999998]
[null,-11.222,-159.63300000000001,3781.5140000000001,1454.7639999999999]
[]
[]
[]
[]
[null,-12.287000000000001,-7.407,-10.263999999999999,-9.3919999999999995,-8.0879999999999992,-16.722999999999999,-11.222]
[null,-243.56800000000001,-98.566999999999993,-146.857,-147.33699999999999,-98.022000000000006,-246.36699999999999,-159.63300000000001]
[null,1218.585,486.53,737.03399999999999,746.11800000000005,480.31599999999997,1221.2329999999999,3781.5140000000001]
[null,440.98700000000002,175.809,276.822,270.16300000000001,181.86600000000001,455.04399999999998,1454.7639999999999]
[]
[null,"=-12287","=-7407","=-10264","=-9392","=-8088","=-16723","=-11222","=0","=0","=0"]
[null,-243.56800000000001,-98.566999999999993,-146.857,-147.33699999999999,-98.022000000000006,-246.36699999999999,-159.63300000000001,0,0,0]
[null,"=1218585","=486530","=737034","=746118","=480316","=1221233","=3781514","=0","=0","=0"]
[null,440.98700000000002,175.809,276.822,270.16300000000001,181.86600000000001,455.04399999999998,1454.7639999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-12287,-7407,-10264,-9392,-8088,-16723,-11222,0,0,0,-75383]
[null,"Ann peak Heating load kBtu/hr",-243.56800000000001,-98.566999999999993,-146.857,-147.33699999999999,-98.022000000000006,-246.36699999999999,-159.63300000000001,0,0,0,-1140.3509999999999]
[null,"HLH",50.445871378834653,75.146854423894411,69.891118571127009,63.745019920318732,82.512089122849972,67.878409040171775,70.298747752657661,"","","","50-83",66.105085188683134]
["Cooling","Ann Cool Energy kBtu",1218585,486530,737034,746118,480316,1221233,3781514,0,0,0,8671330]
[null,"Ann peak Cooling load kBtu/hr",440.98700000000002,175.809,276.822,270.16300000000001,181.86600000000001,455.04399999999998,1454.7639999999999,0,0,0,3255.4549999999999]
[null,"CLH",2763.3127507160075,2767.3782343338512,2662.4834731343608,2761.7327317212203,2641.0434055843311,2683.769042114609,2599.4003151026559,"","","","2599-2767",2663.6307367172944]
[]
[]
["SCooper Tech Col 7-16 w setback - Baseline Design.SIM"]
[null,-8.3000000000000004E-2,-26.516999999999999,668.1,508.87]
[null,-0.128,-41.213999999999999,242.49199999999999,190.07599999999999]
[null,-0.25700000000000001,-116.919,665.62099999999998,544.64099999999996]
[null,-0.14699999999999999,-60.052999999999997,235.22,184.26300000000001]
[null,-5.8000000000000003E-2,-58.232999999999997,1044.057,741.61599999999999]
[null,-0.497,-129.91200000000001,1466.4680000000001,1044.048]
[null,-0.37,-101.238,531.08100000000002,394.08]
[null,-0.82299999999999995,-289.13200000000001,1455.481,1122.8869999999999]
[null,-0.35499999999999998,-106.727,512.67399999999998,375.39]
[null,-0.38900000000000001,-196.74100000000001,2352.3960000000002,1710.644]
[null,-1.159,-260.04700000000003,727.93,534.50900000000001]
[null,-0.63600000000000001,-119.374,267.10399999999998,198.19300000000001]
[null,-1.629,-336.04399999999998,728.16399999999999,571.16800000000001]
[null,-0.65800000000000003,-117.363,258.42,192.66399999999999]
[null,-2.3319999999999999,-490.66699999999997,1147.8599999999999,857.399]
[]
[null,-8.3000000000000004E-2,-0.128,-0.25700000000000001,-0.14699999999999999,-5.8000000000000003E-2,-0.497,-0.37,-0.82299999999999995,-0.35499999999999998,-0.38900000000000001,-1.159,-0.63600000000000001,-1.629,-0.65800000000000003,-2.3319999999999999]
[null,-26.516999999999999,-41.213999999999999,-116.919,-60.052999999999997,-58.232999999999997,-129.91200000000001,-101.238,-289.13200000000001,-106.727,-196.74100000000001,-260.04700000000003,-119.374,-336.04399999999998,-117.363,-490.66699999999997]
[null,668.1,242.49199999999999,665.62099999999998,235.22,1044.057,1466.4680000000001,531.08100000000002,1455.481,512.67399999999998,2352.3960000000002,727.93,267.10399999999998,728.16399999999999,258.42,1147.8599999999999]
[null,508.87,190.07599999999999,544.64099999999996,184.26300000000001,741.61599999999999,1044.048,394.08,1122.8869999999999,375.39,1710.644,534.50900000000001,198.19300000000001,571.16800000000001,192.66399999999999,857.399]
[]
[null,"=-83","=-128","=-257","=-147","=-58","=-497","=-370","=-823","=-355","=-389","=-1159","=-636","=-1629","=-658","=-2332"]
[null,-26.516999999999999,-41.213999999999999,-116.919,-60.052999999999997,-58.232999999999997,-129.91200000000001,-101.238,-289.13200000000001,-106.727,-196.74100000000001,-260.04700000000003,-119.374,-336.04399999999998,-117.363,-490.66699999999997]
[null,"=668100","=242492","=665621","=235220","=1044057","=1466468","=531081","=1455481","=512674","=2352396","=727930","=267104","=728164","=258420","=1147860"]
[null,508.87,190.07599999999999,544.64099999999996,184.26300000000001,741.61599999999999,1044.048,394.08,1122.8869999999999,375.39,1710.644,534.50900000000001,198.19300000000001,571.16800000000001,192.66399999999999,857.399]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann Heat Energy kBtu",-83,-128,-257,-147,-58,-497,-370,-823,-355,-389,-1159,-636,-1629,-658,-2332,-3107]
[null,"Ann peak Heating load kBtu/hr",-26.516999999999999,-41.213999999999999,-116.919,-60.052999999999997,-58.232999999999997,-129.91200000000001,-101.238,-289.13200000000001,-106.727,-196.74100000000001,-260.04700000000003,-119.374,-336.04399999999998,-117.363,-490.66699999999997,-1126.6860000000001]
[null,"HLH",3.1300675038654449,3.1057407677002962,2.1981029601690061,2.447837743326728,0.99599883227723118,3.82566660508652,3.6547541437009818,2.8464507560560572,3.3262435934674448,1.9772187800204328,4.4568866397228186,5.3277933218288744,4.8475794836390476,5.606536983546774,4.7527141625583136,"1-4",2.7576449871570246]
["Cooling","Ann Cool Energy kBtu",668100,242492,665621,235220,1044057,1466468,531081,1455481,512674,2352396,727930,267104,728164,258420,1147860,9173590]
[null,"Ann peak Cooling load kBtu/hr",508.87,190.07599999999999,544.64099999999996,184.26300000000001,741.61599999999999,1044.048,394.08,1122.8869999999999,375.39,1710.644,534.50900000000001,198.19300000000001,571.16800000000001,192.66399999999999,857.399,6816.5150000000003]
[null,"CLH",1312.9089944386583,1275.7633788589828,1222.1279705347192,1276.5449384846659,1407.813477594874,1404.5982560188804,1347.6476857490866,1296.1954319535271,1365.7103279256241,1375.1522818307023,1361.8666851259754,1347.6964373111057,1274.8683399630231,1341.2988415064569,1338.769930918977,"1222-1408",1345.7888671850644]
[]
["SCooper Tech Col 6-20 w setback - Baseline Design.SIM"]
[null,-0.113,-26.277999999999999,917.23299999999995,491.69499999999999]
[null,-0.13200000000000001,-35.613999999999997,321.00400000000002,179.92599999999999]
[null,-0.251,-89.986999999999995,909.09799999999996,522.24699999999996]
[null,-0.125,-35.378999999999998,317.69900000000001,179.10900000000001]
[null,-6.0999999999999999E-2,-57.978000000000002,1400.529,683.92600000000004]
[null,-0.52200000000000002,-120.616,1999.9459999999999,1001.764]
[null,-0.42199999999999999,-91.603999999999999,701.21,373.92599999999999]
[null,-0.86099999999999999,-248.59800000000001,1984.8050000000001,1067.6769999999999]
[null,-0.35399999999999998,-81.257000000000005,692.16600000000005,359.86799999999999]
[null,-0.497,-191.517,3086.9479999999999,1617.7539999999999]
[null,-1.1950000000000001,-213.738,996.03899999999999,517.14499999999998]
[null,-0.65800000000000003,-107.884,351.60700000000003,188.447]
[null,-1.5940000000000001,-307.15199999999999,991.30600000000004,548.03700000000003]
[null,-0.60299999999999998,-102.23,346.84899999999999,187.899]
[null,-2.5030000000000001,-460.74200000000002,1531.896,828.82500000000005]
[]
[null,-0.113,-0.13200000000000001,-0.251,-0.125,-6.0999999999999999E-2,-0.52200000000000002,-0.42199999999999999,-0.86099999999999999,-0.35399999999999998,-0.497,-1.1950000000000001,-0.65800000000000003,-1.5940000000000001,-0.60299999999999998,-2.5030000000000001]
[null,-26.277999999999999,-35.613999999999997,-89.986999999999995,-35.378999999999998,-57.978000000000002,-120.616,-91.603999999999999,-248.59800000000001,-81.257000000000005,-191.517,-213.738,-107.884,-307.15199999999999,-102.23,-460.74200000000002]
[null,917.23299999999995,321.00400000000002,909.09799999999996,317.69900000000001,1400.529,1999.9459999999999,701.21,1984.8050000000001,692.16600000000005,3086.9479999999999,996.03899999999999,351.60700000000003,991.30600000000004,346.84899999999999,1531.896]
[null,491.69499999999999,179.92599999999999,522.24699999999996,179.10900000000001,683.92600000000004,1001.764,373.92599999999999,1067.6769999999999,359.86799999999999,1617.7539999999999,517.14499999999998,188.447,548.03700000000003,187.899,828.82500000000005]
[]
[null,"=-113","=-132","=-251","=-125","=-61","=-522","=-422","=-861","=-354","=-497","=-1195","=-658","=-1594","=-603","=-2503"]
[null,-26.277999999999999,-35.613999999999997,-89.986999999999995,-35.378999999999998,-57.978000000000002,-120.616,-91.603999999999999,-248.59800000000001,-81.257000000000005,-191.517,-213.738,-107.884,-307.15199999999999,-102.23,-460.74200000000002]
[null,"=917233","=321004","=909098","=317699","=1400529","=1999946","=701210","=1984805","=692166","=3086948","=996039","=351607","=991306","=346849","=1531896"]
[null,491.69499999999999,179.92599999999999,522.24699999999996,179.10900000000001,683.92600000000004,1001.764,373.92599999999999,1067.6769999999999,359.86799999999999,1617.7539999999999,517.14499999999998,188.447,548.03700000000003,187.899,828.82500000000005]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann Heat Energy kBtu",-113,-132,-251,-125,-61,-522,-422,-861,-354,-497,-1195,-658,-1594,-603,-2503,-3338]
[null,"Ann peak Heating load kBtu/hr",-26.277999999999999,-35.613999999999997,-89.986999999999995,-35.378999999999998,-57.978000000000002,-120.616,-91.603999999999999,-248.59800000000001,-81.257000000000005,-191.517,-213.738,-107.884,-307.15199999999999,-102.23,-460.74200000000002,-978.82799999999997]
[null,"HLH",4.3001750513737731,3.7064075925197959,2.7892917865913969,3.5331693942734392,1.0521232191520922,4.3277840419181537,4.6067857298807917,3.4634228754857239,4.3565477435790143,2.5950698893570805,5.5909571531501188,6.099143524526343,5.1896129603583896,5.8984642472855322,5.4325414223144408,"1-5",3.4102007707176338]
["Cooling","Ann Cool Energy kBtu",917233,321004,909098,317699,1400529,1999946,701210,1984805,692166,3086948,996039,351607,991306,346849,1531896,12330638]
[null,"Ann peak Cooling load kBtu/hr",491.69499999999999,179.92599999999999,522.24699999999996,179.10900000000001,683.92600000000004,1001.764,373.92599999999999,1067.6769999999999,359.86799999999999,1617.7539999999999,517.14499999999998,188.447,548.03700000000003,187.899,828.82500000000005,6477.8919999999998]
[null,"CLH",1865.4511434934259,1784.0890143725755,1740.7433647297162,1773.774628857288,2047.7785608384531,1996.424307521532,1875.2640896861947,1858.9938717421094,1923.3885758111307,1908.1689799561616,1926.0342843883245,1865.8137301204051,1808.8304256829374,1845.9331875103114,1848.274364310922,"1741-2048",1903.4954580903789]
[]
["SCooper Tech Col 9-21 7days w setback - Baseline Design.SIM"]
[null,-0.99199999999999999,-41.747,870.84199999999998,470.09]
[null,-1.373,-24.23,304.93400000000003,180.33]
[null,-3.4740000000000002,-117.833,862.53399999999999,507.96199999999999]
[null,-1.524,-64.677000000000007,302.04899999999998,177.33500000000001]
[null,-0.441,-70.272999999999996,1265.8409999999999,636.97199999999998]
[null,-2.5009999999999999,-129.887,1897.421,962.98]
[null,-2.488,-57.253,669.08799999999997,373.62599999999998]
[null,-7.742,-186.21199999999999,1880.3009999999999,1040.1859999999999]
[null,-3.1579999999999999,-104.322,657.52,363.226]
[null,-1.901,-163.66399999999999,2770.357,1408.723]
[null,-4.7149999999999999,-245.42400000000001,952.23900000000003,507.03300000000002]
[null,-3.0659999999999998,-99.156999999999996,336.12200000000001,190.971]
[null,-10.364000000000001,-315.52300000000002,945.66300000000001,541.76800000000003]
[null,-3.8029999999999999,-116.23699999999999,330.28100000000001,189.32400000000001]
[null,-13.207000000000001,-354.46100000000001,1396.143,733.298]
[]
[null,-0.99199999999999999,-1.373,-3.4740000000000002,-1.524,-0.441,-2.5009999999999999,-2.488,-7.742,-3.1579999999999999,-1.901,-4.7149999999999999,-3.0659999999999998,-10.364000000000001,-3.8029999999999999,-13.207000000000001]
[null,-41.747,-24.23,-117.833,-64.677000000000007,-70.272999999999996,-129.887,-57.253,-186.21199999999999,-104.322,-163.66399999999999,-245.42400000000001,-99.156999999999996,-315.52300000000002,-116.23699999999999,-354.46100000000001]
[null,870.84199999999998,304.93400000000003,862.53399999999999,302.04899999999998,1265.8409999999999,1897.421,669.08799999999997,1880.3009999999999,657.52,2770.357,952.23900000000003,336.12200000000001,945.66300000000001,330.28100000000001,1396.143]
[null,470.09,180.33,507.96199999999999,177.33500000000001,636.97199999999998,962.98,373.62599999999998,1040.1859999999999,363.226,1408.723,507.03300000000002,190.971,541.76800000000003,189.32400000000001,733.298]
[]
[null,"=-992","=-1373","=-3474","=-1524","=-441","=-2501","=-2488","=-7742","=-3158","=-1901","=-4715","=-3066","=-10364","=-3803","=-13207"]
[null,-41.747,-24.23,-117.833,-64.677000000000007,-70.272999999999996,-129.887,-57.253,-186.21199999999999,-104.322,-163.66399999999999,-245.42400000000001,-99.156999999999996,-315.52300000000002,-116.23699999999999,-354.46100000000001]
[null,"=870842","=304934","=862534","=302049","=1265841","=1897421","=669088","=1880301","=657520","=2770357","=952239","=336122","=945663","=330281","=1396143"]
[null,470.09,180.33,507.96199999999999,177.33500000000001,636.97199999999998,962.98,373.62599999999998,1040.1859999999999,363.226,1408.723,507.03300000000002,190.971,541.76800000000003,189.32400000000001,733.298]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann Heat Energy kBtu",-992,-1373,-3474,-1524,-441,-2501,-2488,-7742,-3158,-1901,-4715,-3066,-10364,-3803,-13207,-25594]
[null,"Ann peak Heating load kBtu/hr",-41.747,-24.23,-117.833,-64.677000000000007,-70.272999999999996,-129.887,-57.253,-186.21199999999999,-104.322,-163.66399999999999,-245.42400000000001,-99.156999999999996,-315.52300000000002,-116.23699999999999,-354.46100000000001,-960.09799999999996]
[null,"HLH",23.762186504419478,56.665290961617828,29.482403061960571,23.563245048471632,6.2755254507421059,19.255198749682418,43.456238101060208,41.57626790969433,30.271658902244972,11.615260533776519,19.211650042375645,30.920661173694242,32.847050769674475,32.717637241153852,37.259388197855337,"6-57",26.657695360265308]
["Cooling","Ann Cool Energy kBtu",870842,304934,862534,302049,1265841,1897421,669088,1880301,657520,2770357,952239,336122,945663,330281,1396143,11480887]
[null,"Ann peak Cooling load kBtu/hr",470.09,180.33,507.96199999999999,177.33500000000001,636.97199999999998,962.98,373.62599999999998,1040.1859999999999,363.226,1408.723,507.03300000000002,190.971,541.76800000000003,189.32400000000001,733.298,6121.4299999999994]
[null,"CLH",1852.500584994363,1690.9776520822934,1698.0285926900044,1703.2678264302026,1987.2788756805637,1970.3638704853684,1790.7961437373203,1807.6584380101253,1810.2228364709574,1966.573272389249,1878.0611912834074,1760.068282618827,1745.5128394441901,1744.5278992626395,1903.923098112909,"1691-1987",1875.5236929933039]
[]
["SCooper Tech Col 8-22 7days w setback - Baseline Design.SIM"]
[null,-2.0070000000000001,-151.37799999999999,972.05799999999999,465.88099999999997]
[null,-1.986,-92.375,340.62099999999998,176.58199999999999]
[null,-4.9850000000000003,-269.77499999999998,963.72500000000002,502.58600000000001]
[null,-2.161,-97.662000000000006,336.76600000000002,176.74799999999999]
[null,-0.44500000000000001,-65.028999999999996,1405.9649999999999,620.274]
[null,-4.5410000000000004,-189.86199999999999,2106.1039999999998,951.55200000000002]
[null,-3.65,-133.30000000000001,741.77200000000005,359.67399999999998]
[null,-10.407,-269.10500000000002,2090.1579999999999,1026.3209999999999]
[null,-4.1689999999999996,-134.63800000000001,730.1,360.245]
[null,-1.7989999999999999,-154.20599999999999,3062.6489999999999,1298.2850000000001]
[null,-6.76,-317.66399999999999,1058.6579999999999,502.28699999999998]
[null,-3.9649999999999999,-115.441,373.161,183.173]
[null,-12.712,-320.62299999999999,1052.289,536.41399999999999]
[null,-4.6740000000000004,-117.176,367.24299999999999,187.77199999999999]
[null,-14.452999999999999,-420.74,1547.057,716.61199999999997]
[]
[null,-2.0070000000000001,-1.986,-4.9850000000000003,-2.161,-0.44500000000000001,-4.5410000000000004,-3.65,-10.407,-4.1689999999999996,-1.7989999999999999,-6.76,-3.9649999999999999,-12.712,-4.6740000000000004,-14.452999999999999]
[null,-151.37799999999999,-92.375,-269.77499999999998,-97.662000000000006,-65.028999999999996,-189.86199999999999,-133.30000000000001,-269.10500000000002,-134.63800000000001,-154.20599999999999,-317.66399999999999,-115.441,-320.62299999999999,-117.176,-420.74]
[null,972.05799999999999,340.62099999999998,963.72500000000002,336.76600000000002,1405.9649999999999,2106.1039999999998,741.77200000000005,2090.1579999999999,730.1,3062.6489999999999,1058.6579999999999,373.161,1052.289,367.24299999999999,1547.057]
[null,465.88099999999997,176.58199999999999,502.58600000000001,176.74799999999999,620.274,951.55200000000002,359.67399999999998,1026.3209999999999,360.245,1298.2850000000001,502.28699999999998,183.173,536.41399999999999,187.77199999999999,716.61199999999997]
[]
[null,"=-2007","=-1986","=-4985","=-2161","=-445","=-4541","=-3650","=-10407","=-4169","=-1799","=-6760","=-3965","=-12712","=-4674","=-14453"]
[null,-151.37799999999999,-92.375,-269.77499999999998,-97.662000000000006,-65.028999999999996,-189.86199999999999,-133.30000000000001,-269.10500000000002,-134.63800000000001,-154.20599999999999,-317.66399999999999,-115.441,-320.62299999999999,-117.176,-420.74]
[null,"=972058","=340621","=963725","=336766","=1405965","=2106104","=741772","=2090158","=730100","=3062649","=1058658","=373161","=1052289","=367243","=1547057"]
[null,465.88099999999997,176.58199999999999,502.58600000000001,176.74799999999999,620.274,951.55200000000002,359.67399999999998,1026.3209999999999,360.245,1298.2850000000001,502.28699999999998,183.173,536.41399999999999,187.77199999999999,716.61199999999997]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann Heat Energy kBtu",-2007,-1986,-4985,-2161,-445,-4541,-3650,-10407,-4169,-1799,-6760,-3965,-12712,-4674,-14453,-36150]
[null,"Ann peak Heating load kBtu/hr",-151.37799999999999,-92.375,-269.77499999999998,-97.662000000000006,-65.028999999999996,-189.86199999999999,-133.30000000000001,-269.10500000000002,-134.63800000000001,-154.20599999999999,-317.66399999999999,-115.441,-320.62299999999999,-117.176,-420.74,-1557.33]
[null,"HLH",13.258201323838339,21.499323410013531,18.478361597627654,22.127337142389056,6.8431007704255027,23.917371564610086,27.381845461365337,38.672637074747776,30.964512247656678,11.666212728428206,21.280346529666566,34.346549319565838,39.647810668604563,39.888714412507682,34.351380900318489,"7-39",23.212806534260562]
["Cooling","Ann Cool Energy kBtu",972058,340621,963725,336766,1405965,2106104,741772,2090158,730100,3062649,1058658,373161,1052289,367243,1547057,12749918]
[null,"Ann peak Cooling load kBtu/hr",465.88099999999997,176.58199999999999,502.58600000000001,176.74799999999999,620.274,951.55200000000002,359.67399999999998,1026.3209999999999,360.245,1298.2850000000001,502.28699999999998,183.173,536.41399999999999,187.77199999999999,716.61199999999997,5938.1480000000001]
[null,"CLH",2086.4941905765636,1928.9678449672108,1917.5325217972645,1905.3454635978908,2266.6837558885268,2213.3356873822977,2062.3453460633796,2036.5538657008872,2026.6762897472554,2358.9959061377122,2107.6754922982282,2037.2052649680902,1961.7105444675196,1955.7921308821337,2158.8488610293994,"1905-2359",2147.1202805992712]
[]
["SCooper Tech Col 5-23 7days w setback - Baseline Design.SIM"]
[null,-4.0650000000000004,-157.42099999999999,1157.404,460.471]
[null,-3.3260000000000001,-75.658000000000001,403.97899999999998,168.96]
[null,-7.98,-278.24400000000003,1147.4770000000001,494.05]
[null,-3.3780000000000001,-79.355999999999995,400.19799999999998,174.60400000000001]
[null,-0.26900000000000002,-50.304000000000002,1659.395,595.40899999999999]
[null,-8.3249999999999993,-188.108,2489.3209999999999,937.18]
[null,-6.173,-105.36199999999999,871.827,340.38799999999998]
[null,-15.49,-262.13499999999999,2470.681,1005.604]
[null,-6.1079999999999997,-106.212,861.89700000000005,353.73500000000001]
[null,-0.83599999999999997,-115.01,3595.3649999999998,1210.355]
[null,-10.385999999999999,-224.51,1252.692,494.44]
[null,-5.883,-106.17100000000001,439.13200000000001,176.917]
[null,-17.081,-301.72300000000001,1245.442,525.79999999999995]
[null,-6.234,-99.634,434.21199999999999,184.61699999999999]
[null,-14.958,-221.97300000000001,1820.7840000000001,688.52099999999996]
[]
[null,-4.0650000000000004,-3.3260000000000001,-7.98,-3.3780000000000001,-0.26900000000000002,-8.3249999999999993,-6.173,-15.49,-6.1079999999999997,-0.83599999999999997,-10.385999999999999,-5.883,-17.081,-6.234,-14.958]
[null,-157.42099999999999,-75.658000000000001,-278.24400000000003,-79.355999999999995,-50.304000000000002,-188.108,-105.36199999999999,-262.13499999999999,-106.212,-115.01,-224.51,-106.17100000000001,-301.72300000000001,-99.634,-221.97300000000001]
[null,1157.404,403.97899999999998,1147.4770000000001,400.19799999999998,1659.395,2489.3209999999999,871.827,2470.681,861.89700000000005,3595.3649999999998,1252.692,439.13200000000001,1245.442,434.21199999999999,1820.7840000000001]
[null,460.471,168.96,494.05,174.60400000000001,595.40899999999999,937.18,340.38799999999998,1005.604,353.73500000000001,1210.355,494.44,176.917,525.79999999999995,184.61699999999999,688.52099999999996]
[]
[null,"=-4065","=-3326","=-7980","=-3378","=-269","=-8325","=-6173","=-15490","=-6108","=-836","=-10386","=-5883","=-17081","=-6234","=-14958"]
[null,-157.42099999999999,-75.658000000000001,-278.24400000000003,-79.355999999999995,-50.304000000000002,-188.108,-105.36199999999999,-262.13499999999999,-106.212,-115.01,-224.51,-106.17100000000001,-301.72300000000001,-99.634,-221.97300000000001]
[null,"=1157404","=403979","=1147477","=400198","=1659395","=2489321","=871827","=2470681","=861897","=3595365","=1252692","=439132","=1245442","=434212","=1820784"]
[null,460.471,168.96,494.05,174.60400000000001,595.40899999999999,937.18,340.38799999999998,1005.604,353.73500000000001,1210.355,494.44,176.917,525.79999999999995,184.61699999999999,688.52099999999996]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann Heat Energy kBtu",-4065,-3326,-7980,-3378,-269,-8325,-6173,-15490,-6108,-836,-10386,-5883,-17081,-6234,-14958,-55950]
[null,"Ann peak Heating load kBtu/hr",-157.42099999999999,-75.658000000000001,-278.24400000000003,-79.355999999999995,-50.304000000000002,-188.108,-105.36199999999999,-262.13499999999999,-106.212,-115.01,-224.51,-106.17100000000001,-301.72300000000001,-99.634,-221.97300000000001,-1417.8100000000002]
[null,"HLH",25.822476035598811,43.960982315155036,28.679863716737824,42.56766974141842,5.3474872773536894,44.256490952006295,58.588485412197947,59.091689396684913,57.507626256920119,7.2689331362490215,46.260745623802947,55.410611183844928,56.611527792047667,62.569002549330548,67.386574042788979,"5-59",39.462269274444388]
["Cooling","Ann Cool Energy kBtu",1157404,403979,1147477,400198,1659395,2489321,871827,2470681,861897,3595365,1252692,439132,1245442,434212,1820784,15057544]
[null,"Ann peak Cooling load kBtu/hr",460.471,168.96,494.05,174.60400000000001,595.40899999999999,937.18,340.38799999999998,1005.604,353.73500000000001,1210.355,494.44,176.917,525.79999999999995,184.61699999999999,688.52099999999996,5740.7559999999994]
[null,"CLH",2513.5220241882766,2390.9741950757575,2322.592854974193,2292.0322558475177,2786.9834013258114,2656.1823769179882,2561.2741929797762,2456.9124625598147,2436.5612676155879,2970.5045214007459,2533.5571555699375,2482.1356907476388,2368.661087866109,2351.9610870071556,2644.4857891044721,"2292-2971",2622.920047464132]
[]
["SCooper Tech Col 24h 7days w setback - Baseline Design.SIM"]
[null,-4.67,-80.366,1469.723,477.19900000000001]
[null,-3.859,-51.281999999999996,508.77499999999998,172.92500000000001]
[null,-8.5500000000000007,-137.357,1456.72,508.964]
[null,-3.8479999999999999,-53.838000000000001,505.245,179.989]
[null,-4.0000000000000001E-3,-0.76800000000000002,2082.3069999999998,619.11099999999999]
[null,-9.7349999999999994,-134.53700000000001,3135.203,969.75300000000004]
[null,-7.3650000000000002,-78.658000000000001,1089.6420000000001,347.27699999999999]
[null,-17.922000000000001,-180.49199999999999,3113.3380000000002,1031.2059999999999]
[null,-6.93,-83.206000000000003,1081.5809999999999,363.35599999999999]
[null,0,0,4527.259,1252.9169999999999]
[null,-11.27,-171.27,1578.259,509.976]
[null,-6.4340000000000002,-73.442999999999998,548.72500000000002,182.03399999999999]
[null,-18.041,-220.57900000000001,1568.941,538.46600000000001]
[null,-6.5979999999999999,-74.290999999999997,544.80700000000002,189.40199999999999]
[null,-13.169,-77.272000000000006,2292.4870000000001,704.50699999999995]
[]
[null,-4.67,-3.859,-8.5500000000000007,-3.8479999999999999,-4.0000000000000001E-3,-9.7349999999999994,-7.3650000000000002,-17.922000000000001,-6.93,0,-11.27,-6.4340000000000002,-18.041,-6.5979999999999999,-13.169]
[null,-80.366,-51.281999999999996,-137.357,-53.838000000000001,-0.76800000000000002,-134.53700000000001,-78.658000000000001,-180.49199999999999,-83.206000000000003,0,-171.27,-73.442999999999998,-220.57900000000001,-74.290999999999997,-77.272000000000006]
[null,1469.723,508.77499999999998,1456.72,505.245,2082.3069999999998,3135.203,1089.6420000000001,3113.3380000000002,1081.5809999999999,4527.259,1578.259,548.72500000000002,1568.941,544.80700000000002,2292.4870000000001]
[null,477.19900000000001,172.92500000000001,508.964,179.989,619.11099999999999,969.75300000000004,347.27699999999999,1031.2059999999999,363.35599999999999,1252.9169999999999,509.976,182.03399999999999,538.46600000000001,189.40199999999999,704.50699999999995]
[]
[null,"=-4670","=-3859","=-8550","=-3848","=-4","=-9735","=-7365","=-17922","=-6930","=0","=-11270","=-6434","=-18041","=-6598","=-13169"]
[null,-80.366,-51.281999999999996,-137.357,-53.838000000000001,-0.76800000000000002,-134.53700000000001,-78.658000000000001,-180.49199999999999,-83.206000000000003,0,-171.27,-73.442999999999998,-220.57900000000001,-74.290999999999997,-77.272000000000006]
[null,"=1469723","=508775","=1456720","=505245","=2082307","=3135203","=1089642","=3113338","=1081581","=4527259","=1578259","=548725","=1568941","=544807","=2292487"]
[null,477.19900000000001,172.92500000000001,508.964,179.989,619.11099999999999,969.75300000000004,347.27699999999999,1031.2059999999999,363.35599999999999,1252.9169999999999,509.976,182.03399999999999,538.46600000000001,189.40199999999999,704.50699999999995]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann Heat Energy kBtu",-4670,-3859,-8550,-3848,-4,-9735,-7365,-17922,-6930,0,-11270,-6434,-18041,-6598,-13169,-62883]
[null,"Ann peak Heating load kBtu/hr",-80.366,-51.281999999999996,-137.357,-53.838000000000001,-0.76800000000000002,-134.53700000000001,-78.658000000000001,-180.49199999999999,-83.206000000000003,0,-171.27,-73.442999999999998,-220.57900000000001,-74.290999999999997,-77.272000000000006,-800.50400000000002]
[null,"HLH",58.109150635841026,75.250575250575253,62.246554598600724,71.473680300159742,5.208333333333333,72.359276630220677,93.633196877622112,99.295259623695244,83.287262937768901,"",65.802534010626488,87.605353811799631,81.789290911646162,88.812911388997321,170.42395693135933,"5-99",78.554260815686121]
["Cooling","Ann Cool Energy kBtu",1469723,508775,1456720,505245,2082307,3135203,1089642,3113338,1081581,4527259,1578259,548725,1568941,544807,2292487,18969793]
[null,"Ann peak Cooling load kBtu/hr",477.19900000000001,172.92500000000001,508.964,179.989,619.11099999999999,969.75300000000004,347.27699999999999,1031.2059999999999,363.35599999999999,1252.9169999999999,509.976,182.03399999999999,538.46600000000001,189.40199999999999,704.50699999999995,5922.6970000000001]
[null,"CLH",3079.8953895544623,2942.1714616163076,2862.1277732806248,2807.0882109462245,3363.3823337010649,3232.9912874721708,3137.6739605559828,3019.1232401673383,2976.6427415537378,3613.3750280345789,3094.7711264843838,3014.4093960468927,2913.7234291487298,2876.4585379246259,3254.0301231925305,"2807-3613",3202.8977676892805]
[]
[]
[]
["SCooper Office 8-17 wo setback - Baseline Design.SIM"]
[null,-0.873,-11.278,68.094999999999999,35.576999999999998]
[null,-10.348000000000001,-25.251999999999999,145.221,92.19]
[null,-3.609,-10.814,47.789000000000001,28.638000000000002]
[null,-10.356,-25.698,137.756,91.263000000000005]
[null,0,-0.36599999999999999,125.642,96.698999999999998]
[null,-2.1360000000000001,-14.452999999999999,74.846999999999994,37.527999999999999]
[null,-13.473000000000001,-33.865000000000002,160.38200000000001,95.924999999999997]
[null,-4.242,-13.555999999999999,54.927999999999997,31.556999999999999]
[null,-13.206,-34.094000000000001,153.12899999999999,96.757000000000005]
[null,-5.8999999999999997E-2,-9.6310000000000002,146.93799999999999,118.333]
[]
[null,-0.873,-10.348000000000001,-3.609,-10.356,0,-2.1360000000000001,-13.473000000000001,-4.242,-13.206,-5.8999999999999997E-2]
[null,-11.278,-25.251999999999999,-10.814,-25.698,-0.36599999999999999,-14.452999999999999,-33.865000000000002,-13.555999999999999,-34.094000000000001,-9.6310000000000002]
[null,68.094999999999999,145.221,47.789000000000001,137.756,125.642,74.846999999999994,160.38200000000001,54.927999999999997,153.12899999999999,146.93799999999999]
[null,35.576999999999998,92.19,28.638000000000002,91.263000000000005,96.698999999999998,37.527999999999999,95.924999999999997,31.556999999999999,96.757000000000005,118.333]
[]
[null,"=-873","=-10348","=-3609","=-10356","=0","=-2136","=-13473","=-4242","=-13206","=-59"]
[null,-11.278,-25.251999999999999,-10.814,-25.698,-0.36599999999999999,-14.452999999999999,-33.865000000000002,-13.555999999999999,-34.094000000000001,-9.6310000000000002]
[null,"=68095","=145221","=47789","=137756","=125642","=74847","=160382","=54928","=153129","=146938"]
[null,35.576999999999998,92.19,28.638000000000002,91.263000000000005,96.698999999999998,37.527999999999999,95.924999999999997,31.556999999999999,96.757000000000005,118.333]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-873,-10348,-3609,-10356,0,-2136,-13473,-4242,-13206,-59,-58302]
[null,"Ann peak Heating load kBtu/hr",-11.278,-25.251999999999999,-10.814,-25.698,-0.36599999999999999,-14.452999999999999,-33.865000000000002,-13.555999999999999,-34.094000000000001,-9.6310000000000002,-179.00700000000001]
[null,"HLH",77.407341727256608,409.78932361793125,333.73404845570559,402.98855942096662,0,147.78938628658412,397.84438210541856,312.92416642077313,387.34088109344754,6.1260512927006543,"0-410",325.69676046188135]
["Cooling","Ann Cool Energy kBtu",68095,145221,47789,137756,125642,74847,160382,54928,153129,146938,1114727]
[null,"Ann peak Cooling load kBtu/hr",35.576999999999998,92.19,28.638000000000002,91.263000000000005,96.698999999999998,37.527999999999999,95.924999999999997,31.556999999999999,96.757000000000005,118.333,724.46699999999998]
[null,"CLH",1914.0174832054417,1575.2359258054018,1668.726866401285,1509.4397510491656,1299.3102307159329,1994.4308249840119,1671.9520458691686,1740.5963811515671,1582.6141777855864,1241.7330753044375,"1242-1994",1538.6856820255443]
[]
["SCooper Office 7-19 wo setback - Baseline Design.SIM"]
[null,-0.87,-10.962,72.302000000000007,36.069000000000003]
[null,-8.93,-24.381,157.636,91.638000000000005]
[null,-3.169,-11.388,51.783000000000001,28.193000000000001]
[null,-8.9009999999999998,-25.042000000000002,151.154,93.463999999999999]
[null,-1E-3,-0.33400000000000002,161.89699999999999,100.605]
[null,-2.0129999999999999,-14.06,79.248000000000005,38.005000000000003]
[null,-11.901,-32.962000000000003,173.32499999999999,95.427000000000007]
[null,-3.875,-13.811,59.28,31.407]
[null,-11.597,-33.463999999999999,167.16300000000001,101.52500000000001]
[null,-9.6000000000000002E-2,-20.55,186.97499999999999,123.354]
[]
[null,-0.87,-8.93,-3.169,-8.9009999999999998,-1E-3,-2.0129999999999999,-11.901,-3.875,-11.597,-9.6000000000000002E-2]
[null,-10.962,-24.381,-11.388,-25.042000000000002,-0.33400000000000002,-14.06,-32.962000000000003,-13.811,-33.463999999999999,-20.55]
[null,72.302000000000007,157.636,51.783000000000001,151.154,161.89699999999999,79.248000000000005,173.32499999999999,59.28,167.16300000000001,186.97499999999999]
[null,36.069000000000003,91.638000000000005,28.193000000000001,93.463999999999999,100.605,38.005000000000003,95.427000000000007,31.407,101.52500000000001,123.354]
[]
[null,"=-870","=-8930","=-3169","=-8901","=-1","=-2013","=-11901","=-3875","=-11597","=-96"]
[null,-10.962,-24.381,-11.388,-25.042000000000002,-0.33400000000000002,-14.06,-32.962000000000003,-13.811,-33.463999999999999,-20.55]
[null,"=72302","=157636","=51783","=151154","=161897","=79248","=173325","=59280","=167163","=186975"]
[null,36.069000000000003,91.638000000000005,28.193000000000001,93.463999999999999,100.605,38.005000000000003,95.427000000000007,31.407,101.52500000000001,123.354]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-870,-8930,-3169,-8901,-1,-2013,-11901,-3875,-11597,-96,-51353]
[null,"Ann peak Heating load kBtu/hr",-10.962,-24.381,-11.388,-25.042000000000002,-0.33400000000000002,-14.06,-32.962000000000003,-13.811,-33.463999999999999,-20.55,-186.95400000000001]
[null,"HLH",79.365079365079367,366.26881588121898,278.27537759044611,355.44285600191677,2.9940119760479038,143.17211948790896,361.05212062374852,280.57345594091669,346.55151804924697,4.6715328467153281,"3-366",274.68254222963935]
["Cooling","Ann Cool Energy kBtu",72302,157636,51783,151154,161897,79248,173325,59280,167163,186975,1260763]
[null,"Ann peak Cooling load kBtu/hr",36.069000000000003,91.638000000000005,28.193000000000001,93.463999999999999,100.605,38.005000000000003,95.427000000000007,31.407,101.52500000000001,123.354,739.68700000000001]
[null,"CLH",2004.5468407773988,1720.203409066108,1836.7325222572979,1617.243002653428,1609.234133492371,2085.1993158794894,1816.3098494136877,1887.4773139745917,1646.5205614380693,1515.7595213774989,"1516-2085",1704.4547220648733]
[]
["SCooper Office 7-22 wo setback - Baseline Design.SIM"]
[null,-0.81100000000000005,-10.603999999999999,76.897000000000006,36.311999999999998]
[null,-7.62,-23.344999999999999,170.32900000000001,92.197000000000003]
[null,-2.843,-11.516,55.98,28.486999999999998]
[null,-7.6849999999999996,-23.95,163.93,92.941999999999993]
[null,-1E-3,-1.4279999999999999,199.797,102.746]
[null,-1.7849999999999999,-13.593999999999999,83.960999999999999,38.207999999999998]
[null,-10.555999999999999,-31.6,186.66900000000001,95.284000000000006]
[null,-3.52,-13.948,63.942,31.367000000000001]
[null,-10.388999999999999,-32.210999999999999,180.79900000000001,100.658]
[null,-0.104,-29.376999999999999,228.52600000000001,124.489]
[]
[null,-0.81100000000000005,-7.62,-2.843,-7.6849999999999996,-1E-3,-1.7849999999999999,-10.555999999999999,-3.52,-10.388999999999999,-0.104]
[null,-10.603999999999999,-23.344999999999999,-11.516,-23.95,-1.4279999999999999,-13.593999999999999,-31.6,-13.948,-32.210999999999999,-29.376999999999999]
[null,76.897000000000006,170.32900000000001,55.98,163.93,199.797,83.960999999999999,186.66900000000001,63.942,180.79900000000001,228.52600000000001]
[null,36.311999999999998,92.197000000000003,28.486999999999998,92.941999999999993,102.746,38.207999999999998,95.284000000000006,31.367000000000001,100.658,124.489]
[]
[null,"=-811","=-7620","=-2843","=-7685","=-1","=-1785","=-10556","=-3520","=-10389","=-104"]
[null,-10.603999999999999,-23.344999999999999,-11.516,-23.95,-1.4279999999999999,-13.593999999999999,-31.6,-13.948,-32.210999999999999,-29.376999999999999]
[null,"=76897","=170329","=55980","=163930","=199797","=83961","=186669","=63942","=180799","=228526"]
[null,36.311999999999998,92.197000000000003,28.486999999999998,92.941999999999993,102.746,38.207999999999998,95.284000000000006,31.367000000000001,100.658,124.489]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-811,-7620,-2843,-7685,-1,-1785,-10556,-3520,-10389,-104,-45314]
[null,"Ann peak Heating load kBtu/hr",-10.603999999999999,-23.344999999999999,-11.516,-23.95,-1.4279999999999999,-13.593999999999999,-31.6,-13.948,-32.210999999999999,-29.376999999999999,-191.57299999999998]
[null,"HLH",76.480573368540178,326.408224459199,246.87391455366446,320.87682672233819,0.70028011204481799,131.30792996910401,334.05063291139237,252.36593059936908,322.529570643569,3.540184498076727,"1-334",236.53646390670923]
["Cooling","Ann Cool Energy kBtu",76897,170329,55980,163930,199797,83961,186669,63942,180799,228526,1410830]
[null,"Ann peak Cooling load kBtu/hr",36.311999999999998,92.197000000000003,28.486999999999998,92.941999999999993,102.746,38.207999999999998,95.284000000000006,31.367000000000001,100.658,124.489,742.68999999999994]
[null,"CLH",2117.6745979290595,1847.4462292699327,1965.1068908624989,1763.7881689655915,1944.5720514667239,2197.4717336683416,1959.0802233323536,2038.5118117767079,1796.1711935464643,1835.712392259557,"1764-2197",1899.6216456394998]
[]
["SCooper Office 6-21 7days wo setback - Baseline Design.SIM"]
[null,-1.405,-14.435,77.465999999999994,36.015000000000001]
[null,-7.87,-34.631999999999998,173.68100000000001,90.974999999999994]
[null,-3.7629999999999999,-17.638999999999999,56.936,27.954000000000001]
[null,-7.9160000000000004,-35.088999999999999,166.37700000000001,92.036000000000001]
[null,-0.16400000000000001,-18.439,214.59,101.524]
[null,-2.3380000000000001,-17.074000000000002,84.334000000000003,37.832000000000001]
[null,-9.9879999999999995,-43.302,189.447,93.771000000000001]
[null,-4.3470000000000004,-19.507999999999999,64.394000000000005,30.646000000000001]
[null,-9.9740000000000002,-43.122,182.161,99.376000000000005]
[null,-3.242,-77.686999999999998,248.20400000000001,120.422]
[]
[null,-1.405,-7.87,-3.7629999999999999,-7.9160000000000004,-0.16400000000000001,-2.3380000000000001,-9.9879999999999995,-4.3470000000000004,-9.9740000000000002,-3.242]
[null,-14.435,-34.631999999999998,-17.638999999999999,-35.088999999999999,-18.439,-17.074000000000002,-43.302,-19.507999999999999,-43.122,-77.686999999999998]
[null,77.465999999999994,173.68100000000001,56.936,166.37700000000001,214.59,84.334000000000003,189.447,64.394000000000005,182.161,248.20400000000001]
[null,36.015000000000001,90.974999999999994,27.954000000000001,92.036000000000001,101.524,37.832000000000001,93.771000000000001,30.646000000000001,99.376000000000005,120.422]
[]
[null,"=-1405","=-7870","=-3763","=-7916","=-164","=-2338","=-9988","=-4347","=-9974","=-3242"]
[null,-14.435,-34.631999999999998,-17.638999999999999,-35.088999999999999,-18.439,-17.074000000000002,-43.302,-19.507999999999999,-43.122,-77.686999999999998]
[null,"=77466","=173681","=56936","=166377","=214590","=84334","=189447","=64394","=182161","=248204"]
[null,36.015000000000001,90.974999999999994,27.954000000000001,92.036000000000001,101.524,37.832000000000001,93.771000000000001,30.646000000000001,99.376000000000005,120.422]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1405,-7870,-3763,-7916,-164,-2338,-9988,-4347,-9974,-3242,-51007]
[null,"Ann peak Heating load kBtu/hr",-14.435,-34.631999999999998,-17.638999999999999,-35.088999999999999,-18.439,-17.074000000000002,-43.302,-19.507999999999999,-43.122,-77.686999999999998,-320.92700000000002]
[null,"HLH",97.332871492899201,227.24647724647727,213.33408923408356,225.59776568155263,8.8941916589836758,136.93334895162235,230.65909195880099,222.83165880664345,231.29724966374474,41.731563839509832,"9-231",158.93645595415779]
["Cooling","Ann Cool Energy kBtu",77466,173681,56936,166377,214590,84334,189447,64394,182161,248204,1457590]
[null,"Ann peak Cooling load kBtu/hr",36.015000000000001,90.974999999999994,27.954000000000001,92.036000000000001,101.524,37.832000000000001,93.771000000000001,30.646000000000001,99.376000000000005,120.422,730.55100000000004]
[null,"CLH",2150.9371095376928,1909.1068974993132,2036.7747012949847,1807.7382763266548,2113.687403963595,2229.1710721082682,2020.3154493393479,2101.2203876525482,1833.048220898406,2061.1184002923055,"1808-2229",1995.1926696425026]
[]
["SCooper Office 6-19 7days wo setback - Baseline Design.SIM"]
[null,-1.3520000000000001,-15.215999999999999,74.304000000000002,36.125999999999998]
[null,-8.3360000000000003,-36.890999999999998,165.18899999999999,91.763000000000005]
[null,-3.754,-17.802,53.911000000000001,28.271000000000001]
[null,-8.423,-37.270000000000003,158.053,93.668999999999997]
[null,-0.20100000000000001,-20.02,191.03899999999999,101.208]
[null,-2.3889999999999998,-18.050999999999998,81.58,38.070999999999998]
[null,-10.481999999999999,-46.420999999999999,182.011,95.057000000000002]
[null,-4.3659999999999997,-19.831,61.570999999999998,31.468]
[null,-10.558999999999999,-45.780999999999999,174.702,101.652]
[null,-3.7,-170.87200000000001,216.83699999999999,123.94]
[]
[null,-1.3520000000000001,-8.3360000000000003,-3.754,-8.423,-0.20100000000000001,-2.3889999999999998,-10.481999999999999,-4.3659999999999997,-10.558999999999999,-3.7]
[null,-15.215999999999999,-36.890999999999998,-17.802,-37.270000000000003,-20.02,-18.050999999999998,-46.420999999999999,-19.831,-45.780999999999999,-170.87200000000001]
[null,74.304000000000002,165.18899999999999,53.911000000000001,158.053,191.03899999999999,81.58,182.011,61.570999999999998,174.702,216.83699999999999]
[null,36.125999999999998,91.763000000000005,28.271000000000001,93.668999999999997,101.208,38.070999999999998,95.057000000000002,31.468,101.652,123.94]
[]
[null,"=-1352","=-8336","=-3754","=-8423","=-201","=-2389","=-10482","=-4366","=-10559","=-3700"]
[null,-15.215999999999999,-36.890999999999998,-17.802,-37.270000000000003,-20.02,-18.050999999999998,-46.420999999999999,-19.831,-45.780999999999999,-170.87200000000001]
[null,"=74304","=165189","=53911","=158053","=191039","=81580","=182011","=61571","=174702","=216837"]
[null,36.125999999999998,91.763000000000005,28.271000000000001,93.668999999999997,101.208,38.070999999999998,95.057000000000002,31.468,101.652,123.94]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1352,-8336,-3754,-8423,-201,-2389,-10482,-4366,-10559,-3700,-53562]
[null,"Ann peak Heating load kBtu/hr",-15.215999999999999,-36.890999999999998,-17.802,-37.270000000000003,-20.02,-18.050999999999998,-46.420999999999999,-19.831,-45.780999999999999,-170.87200000000001,-428.15499999999997]
[null,"HLH",88.853838065194537,225.96297199859046,210.87518256375688,225.99946337536892,10.039960039960039,132.34723838014514,225.80297710088107,220.16035499974788,230.64153251348813,21.653635469825364,"10-231",125.0995550676741]
["Cooling","Ann Cool Energy kBtu",74304,165189,53911,158053,191039,81580,182011,61571,174702,216837,1359197]
[null,"Ann peak Cooling load kBtu/hr",36.125999999999998,91.763000000000005,28.271000000000001,93.668999999999997,101.208,38.070999999999998,95.057000000000002,31.468,101.652,123.94,741.22500000000014]
[null,"CLH",2056.801195814649,1800.170003160315,1906.9364366311768,1687.3565427195765,1887.5879377124338,2142.8383809198604,1914.7564093123074,1956.6226007372568,1718.6282611261952,1749.5320316282073,"1687-2143",1833.7171574083441]
[]
["SCooper Office 5-23 7days wo setback - Baseline Design.SIM"]
[null,-1.607,-14.516999999999999,81.480999999999995,36.436]
[null,-6.9729999999999999,-35.101999999999997,185.52199999999999,92.662000000000006]
[null,-3.9540000000000002,-17.355,60.393999999999998,28.673999999999999]
[null,-6.9850000000000003,-35.49,178.339,93.363]
[null,-0.11700000000000001,-13.412000000000001,258.95299999999997,104.197]
[null,-2.3610000000000002,-16.93,88.962000000000003,38.343000000000004]
[null,-8.6890000000000001,-42.652999999999999,203.23599999999999,94.503]
[null,-4.2880000000000003,-19.11,68.766999999999996,31.498000000000001]
[null,-8.6790000000000003,-42.362000000000002,195.99600000000001,100.929]
[null,-3.7280000000000002,-173.333,290.74900000000002,125.471]
[]
[null,-1.607,-6.9729999999999999,-3.9540000000000002,-6.9850000000000003,-0.11700000000000001,-2.3610000000000002,-8.6890000000000001,-4.2880000000000003,-8.6790000000000003,-3.7280000000000002]
[null,-14.516999999999999,-35.101999999999997,-17.355,-35.49,-13.412000000000001,-16.93,-42.652999999999999,-19.11,-42.362000000000002,-173.333]
[null,81.480999999999995,185.52199999999999,60.393999999999998,178.339,258.95299999999997,88.962000000000003,203.23599999999999,68.766999999999996,195.99600000000001,290.74900000000002]
[null,36.436,92.662000000000006,28.673999999999999,93.363,104.197,38.343000000000004,94.503,31.498000000000001,100.929,125.471]
[]
[null,"=-1607","=-6973","=-3954","=-6985","=-117","=-2361","=-8689","=-4288","=-8679","=-3728"]
[null,-14.516999999999999,-35.101999999999997,-17.355,-35.49,-13.412000000000001,-16.93,-42.652999999999999,-19.11,-42.362000000000002,-173.333]
[null,"=81481","=185522","=60394","=178339","=258953","=88962","=203236","=68767","=195996","=290749"]
[null,36.436,92.662000000000006,28.673999999999999,93.363,104.197,38.343000000000004,94.503,31.498000000000001,100.929,125.471]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1607,-6973,-3954,-6985,-117,-2361,-8689,-4288,-8679,-3728,-47381]
[null,"Ann peak Heating load kBtu/hr",-14.516999999999999,-35.101999999999997,-17.355,-35.49,-13.412000000000001,-16.93,-42.652999999999999,-19.11,-42.362000000000002,-173.333,-410.26400000000001]
[null,"HLH",110.69780257628987,198.64964959261582,227.8305963699222,196.81600450831218,8.7235311661198924,139.4565859421146,203.71368954118117,224.38513867085297,204.87701241678863,21.507733668718593,"9-228",115.48905095255738]
["Cooling","Ann Cool Energy kBtu",81481,185522,60394,178339,258953,88962,203236,68767,195996,290749,1612399]
[null,"Ann peak Cooling load kBtu/hr",36.436,92.662000000000006,28.673999999999999,93.363,104.197,38.343000000000004,94.503,31.498000000000001,100.929,125.471,746.07600000000002]
[null,"CLH",2236.277308156768,2002.1367982560271,2106.2286391853249,1910.1678395081562,2485.2251024501666,2320.162741569517,2150.5772303524755,2183.217982094101,1941.9195672205212,2317.260562201624,"1910-2485",2161.1725883153995]
[]
["SCooper Office 24 7days wo setback - Baseline Design.SIM"]
[null,-1.871,-14.037000000000001,87.328000000000003,36.311999999999998]
[null,-6.5149999999999997,-34.423999999999999,202.16300000000001,92.38]
[null,-4.2629999999999999,-17.166,65.617999999999995,28.896000000000001]
[null,-6.5090000000000003,-34.677999999999997,195.256,94.08]
[null,-2E-3,-0.34300000000000003,319.63099999999997,107.523]
[null,-2.3479999999999999,-16.498000000000001,95.16,38.198999999999998]
[null,-7.867,-41.927,221.08799999999999,94.376000000000005]
[null,-4.3090000000000002,-18.936,74.411000000000001,31.791]
[null,-7.718,-41.677999999999997,213.52,101.479]
[null,-3.4329999999999998,-175.22200000000001,356.07400000000001,128.851]
[]
[null,-1.871,-6.5149999999999997,-4.2629999999999999,-6.5090000000000003,-2E-3,-2.3479999999999999,-7.867,-4.3090000000000002,-7.718,-3.4329999999999998]
[null,-14.037000000000001,-34.423999999999999,-17.166,-34.677999999999997,-0.34300000000000003,-16.498000000000001,-41.927,-18.936,-41.677999999999997,-175.22200000000001]
[null,87.328000000000003,202.16300000000001,65.617999999999995,195.256,319.63099999999997,95.16,221.08799999999999,74.411000000000001,213.52,356.07400000000001]
[null,36.311999999999998,92.38,28.896000000000001,94.08,107.523,38.198999999999998,94.376000000000005,31.791,101.479,128.851]
[]
[null,"=-1871","=-6515","=-4263","=-6509","=-2","=-2348","=-7867","=-4309","=-7718","=-3433"]
[null,-14.037000000000001,-34.423999999999999,-17.166,-34.677999999999997,-0.34300000000000003,-16.498000000000001,-41.927,-18.936,-41.677999999999997,-175.22200000000001]
[null,"=87328","=202163","=65618","=195256","=319631","=95160","=221088","=74411","=213520","=356074"]
[null,36.311999999999998,92.38,28.896000000000001,94.08,107.523,38.198999999999998,94.376000000000005,31.791,101.479,128.851]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1871,-6515,-4263,-6509,-2,-2348,-7867,-4309,-7718,-3433,-44835]
[null,"Ann peak Heating load kBtu/hr",-14.037000000000001,-34.423999999999999,-17.166,-34.677999999999997,-0.34300000000000003,-16.498000000000001,-41.927,-18.936,-41.677999999999997,-175.22200000000001,-394.90899999999999]
[null,"HLH",133.29058915722732,189.25749477108994,248.33974134917861,187.69825249437685,5.8309037900874632,142.32028124621166,187.63565244353282,227.55597803126321,185.18163059647776,19.592288639554393,"6-248",113.5324846990066]
["Cooling","Ann Cool Energy kBtu",87328,202163,65618,195256,319631,95160,221088,74411,213520,356074,1830249]
[null,"Ann peak Cooling load kBtu/hr",36.311999999999998,92.38,28.896000000000001,94.08,107.523,38.198999999999998,94.376000000000005,31.791,101.479,128.851,753.88700000000017]
[null,"CLH",2404.9350077109498,2188.3849318034208,2270.8333333333335,2075.4251700680275,2972.6756135896508,2491.1646901751355,2342.629482071713,2340.6309961938914,2104.0806472275053,2763.4554640631427,"2075-2973",2427.7497821291513]
[]
[]
["SCooper Rest 9-18 wo setback - Baseline Design.SIM"]
[null,-5.4649999999999999,-14.725,101.55200000000001,56.593000000000004]
[null,-7.008,-13.856999999999999,92.763000000000005,56.500999999999998]
[null,-9.2100000000000009,-14.645,80.015000000000001,57.978999999999999]
[null,-7.38,-14.151999999999999,88.778000000000006,66.016999999999996]
[null,-2E-3,-1.462,42.334000000000003,27.619]
[]
[]
[]
[]
[]
[]
[null,-5.4649999999999999,-7.008,-9.2100000000000009,-7.38,-2E-3]
[null,-14.725,-13.856999999999999,-14.645,-14.151999999999999,-1.462]
[null,101.55200000000001,92.763000000000005,80.015000000000001,88.778000000000006,42.334000000000003]
[null,56.593000000000004,56.500999999999998,57.978999999999999,66.016999999999996,27.619]
[]
[null,"=-5465","=-7008","=-9210","=-7380","=-2","=0","=0","=0","=0","=0"]
[null,-14.725,-13.856999999999999,-14.645,-14.151999999999999,-1.462,0,0,0,0,0]
[null,"=101552","=92763","=80015","=88778","=42334","=0","=0","=0","=0","=0"]
[null,56.593000000000004,56.500999999999998,57.978999999999999,66.016999999999996,27.619,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-5465,-7008,-9210,-7380,-2,0,0,0,0,0,-29065]
[null,"Ann peak Heating load kBtu/hr",-14.725,-13.856999999999999,-14.645,-14.151999999999999,-1.462,0,0,0,0,0,-58.841000000000008]
[null,"HLH",371.1375212224109,505.73717254817063,628.88357801297377,521.48106274731492,1.3679890560875514,"","","","","","1-629",493.9582943865671]
["Cooling","Ann Cool Energy kBtu",101552,92763,80015,88778,42334,0,0,0,0,0,405442]
[null,"Ann peak Cooling load kBtu/hr",56.593000000000004,56.500999999999998,57.978999999999999,66.016999999999996,27.619,0,0,0,0,0,264.70899999999995]
[null,"CLH",1794.4268725814145,1641.7939505495478,1380.0686455440764,1344.7748307254194,1532.7854013541403,"","","","","","1345-1794",1531.6517383239711]
[]
["SCooper Rest 8-20 wo setback - Baseline Design.SIM"]
[null,-4.9829999999999997,-14.585000000000001,109.18899999999999,56.073999999999998]
[null,-6.4249999999999998,-13.736000000000001,100.551,55.881999999999998]
[null,-8.4339999999999993,-17.911000000000001,87.867999999999995,54.061999999999998]
[null,-6.7130000000000001,-14.012,96.67,65.12]
[null,-4.0000000000000001E-3,-2.4390000000000001,48.774999999999999,26.059000000000001]
[]
[]
[]
[]
[]
[]
[null,-4.9829999999999997,-6.4249999999999998,-8.4339999999999993,-6.7130000000000001,-4.0000000000000001E-3]
[null,-14.585000000000001,-13.736000000000001,-17.911000000000001,-14.012,-2.4390000000000001]
[null,109.18899999999999,100.551,87.867999999999995,96.67,48.774999999999999]
[null,56.073999999999998,55.881999999999998,54.061999999999998,65.12,26.059000000000001]
[]
[null,"=-4983","=-6425","=-8434","=-6713","=-4","=0","=0","=0","=0","=0"]
[null,-14.585000000000001,-13.736000000000001,-17.911000000000001,-14.012,-2.4390000000000001,0,0,0,0,0]
[null,"=109189","=100551","=87868","=96670","=48775","=0","=0","=0","=0","=0"]
[null,56.073999999999998,55.881999999999998,54.061999999999998,65.12,26.059000000000001,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-4983,-6425,-8434,-6713,-4,0,0,0,0,0,-26559]
[null,"Ann peak Heating load kBtu/hr",-14.585000000000001,-13.736000000000001,-17.911000000000001,-14.012,-2.4390000000000001,0,0,0,0,0,-62.683]
[null,"HLH",341.65238258484743,467.74898078043094,470.88381441572216,479.08935198401366,1.6400164001640016,"","","","","","2-479",423.70339645517925]
["Cooling","Ann Cool Energy kBtu",109189,100551,87868,96670,48775,0,0,0,0,0,443053]
[null,"Ann peak Cooling load kBtu/hr",56.073999999999998,55.881999999999998,54.061999999999998,65.12,26.059000000000001,0,0,0,0,0,257.197]
[null,"CLH",1947.2304454827549,1799.3450484950431,1625.3190780955201,1484.4901719901718,1871.7141870371081,"","","","","","1484-1947",1722.6211814290214]
[]
["SCooper Rest 7-22 wo setback - Baseline Design.SIM"]
[null,-4.5010000000000003,-14.429,116.417,56.854999999999997]
[null,-5.8810000000000002,-19.818000000000001,107.96899999999999,57.942]
[null,-7.718,-28.260999999999999,95.289000000000001,54.430999999999997]
[null,-6.0380000000000003,-18.178000000000001,104.224,61.707000000000001]
[null,-7.0000000000000001E-3,-4.7610000000000001,55.115000000000002,25.7]
[]
[]
[]
[]
[]
[]
[null,-4.5010000000000003,-5.8810000000000002,-7.718,-6.0380000000000003,-7.0000000000000001E-3]
[null,-14.429,-19.818000000000001,-28.260999999999999,-18.178000000000001,-4.7610000000000001]
[null,116.417,107.96899999999999,95.289000000000001,104.224,55.115000000000002]
[null,56.854999999999997,57.942,54.430999999999997,61.707000000000001,25.7]
[]
[null,"=-4501","=-5881","=-7718","=-6038","=-7","=0","=0","=0","=0","=0"]
[null,-14.429,-19.818000000000001,-28.260999999999999,-18.178000000000001,-4.7610000000000001,0,0,0,0,0]
[null,"=116417","=107969","=95289","=104224","=55115","=0","=0","=0","=0","=0"]
[null,56.854999999999997,57.942,54.430999999999997,61.707000000000001,25.7,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-4501,-5881,-7718,-6038,-7,0,0,0,0,0,-24145]
[null,"Ann peak Heating load kBtu/hr",-14.429,-19.818000000000001,-28.260999999999999,-18.178000000000001,-4.7610000000000001,0,0,0,0,0,-85.446999999999989]
[null,"HLH",311.94122946843163,296.75042890301745,273.09720108984112,332.15975354824513,1.4702793530770846,"","","","","","1-332",282.57282291947058]
["Cooling","Ann Cool Energy kBtu",116417,107969,95289,104224,55115,0,0,0,0,0,479014]
[null,"Ann peak Cooling load kBtu/hr",56.854999999999997,57.942,54.430999999999997,61.707000000000001,25.7,0,0,0,0,0,256.63499999999999]
[null,"CLH",2047.6123471990152,1863.3978806392599,1750.638422957506,1689.0142123259923,2144.5525291828794,"","","","","","1689-2145",1866.5185964502114]
[]
["SCooper Rest 9-22 7days wo setback - Baseline Design.SIM"]
[null,-2.86,-13.798999999999999,137.559,56.463999999999999]
[null,-3.4359999999999999,-12.981999999999999,128.565,59.744999999999997]
[null,-4.9749999999999996,-32.97,116.178,52.984999999999999]
[null,-3.899,-26.495000000000001,125.506,61.564999999999998]
[null,0,0,72.733999999999995,25.321999999999999]
[]
[]
[]
[]
[]
[]
[null,-2.86,-3.4359999999999999,-4.9749999999999996,-3.899,0]
[null,-13.798999999999999,-12.981999999999999,-32.97,-26.495000000000001,0]
[null,137.559,128.565,116.178,125.506,72.733999999999995]
[null,56.463999999999999,59.744999999999997,52.984999999999999,61.564999999999998,25.321999999999999]
[]
[null,"=-2860","=-3436","=-4975","=-3899","=0","=0","=0","=0","=0","=0"]
[null,-13.798999999999999,-12.981999999999999,-32.97,-26.495000000000001,0,0,0,0,0,0]
[null,"=137559","=128565","=116178","=125506","=72734","=0","=0","=0","=0","=0"]
[null,56.463999999999999,59.744999999999997,52.984999999999999,61.564999999999998,25.321999999999999,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-2860,-3436,-4975,-3899,0,0,0,0,0,0,-15170]
[null,"Ann peak Heating load kBtu/hr",-13.798999999999999,-12.981999999999999,-32.97,-26.495000000000001,0,0,0,0,0,0,-86.245999999999995]
[null,"HLH",207.26139575331547,264.67416422739177,150.89475280558085,147.15984147952443,"","","","","","","147-265",175.89221529114394]
["Cooling","Ann Cool Energy kBtu",137559,128565,116178,125506,72734,0,0,0,0,0,580542]
[null,"Ann peak Cooling load kBtu/hr",56.463999999999999,59.744999999999997,52.984999999999999,61.564999999999998,25.321999999999999,0,0,0,0,0,256.08100000000002]
[null,"CLH",2436.2248512326437,2151.8955561134826,2192.6582995187318,2038.5933566149599,2872.3639522944477,"","","","","","2039-2872",2267.0248866569559]
[]
["SCooper Rest 8-22 7days wo setback - Baseline Design.SIM"]
[null,-2.8479999999999999,-26.471,140.93700000000001,56.710999999999999]
[null,-3.4460000000000002,-27.402000000000001,132.054,62.081000000000003]
[null,-4.8819999999999997,-35.055,119.652,53.841000000000001]
[null,-3.7509999999999999,-33.896999999999998,128.78399999999999,61.741]
[null,0,0,75.736999999999995,25.411000000000001]
[]
[]
[]
[]
[]
[]
[null,-2.8479999999999999,-3.4460000000000002,-4.8819999999999997,-3.7509999999999999,0]
[null,-26.471,-27.402000000000001,-35.055,-33.896999999999998,0]
[null,140.93700000000001,132.054,119.652,128.78399999999999,75.736999999999995]
[null,56.710999999999999,62.081000000000003,53.841000000000001,61.741,25.411000000000001]
[]
[null,"=-2848","=-3446","=-4882","=-3751","=0","=0","=0","=0","=0","=0"]
[null,-26.471,-27.402000000000001,-35.055,-33.896999999999998,0,0,0,0,0,0]
[null,"=140937","=132054","=119652","=128784","=75737","=0","=0","=0","=0","=0"]
[null,56.710999999999999,62.081000000000003,53.841000000000001,61.741,25.411000000000001,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-2848,-3446,-4882,-3751,0,0,0,0,0,0,-14927]
[null,"Ann peak Heating load kBtu/hr",-26.471,-27.402000000000001,-35.055,-33.896999999999998,0,0,0,0,0,0,-122.82499999999999]
[null,"HLH",107.58943749763893,125.75724399678855,139.26686635287405,110.65876036227395,"","","","","","","108-139",121.53063301445147]
["Cooling","Ann Cool Energy kBtu",140937,132054,119652,128784,75737,0,0,0,0,0,597164]
[null,"Ann peak Cooling load kBtu/hr",56.710999999999999,62.081000000000003,53.841000000000001,61.741,25.411000000000001,0,0,0,0,0,259.78500000000003]
[null,"CLH",2485.1792421223395,2127.1242409110678,2222.3212793224493,2085.8748643526992,2980.4808941009796,"","","","","","2086-2980",2298.6854514309907]
[]
["SCooper Rest 5-23 7days wo setback - Baseline Design.SIM"]
[null,-1.89,-28.297000000000001,153.15299999999999,57.56]
[null,-2.4860000000000002,-30.596,144.24100000000001,63.978000000000002]
[null,-3.621,-35.658999999999999,131.745,54.938000000000002]
[null,-2.5339999999999998,-34.46,141.24799999999999,59.875999999999998]
[null,0,0,86.638000000000005,25.364999999999998]
[]
[]
[]
[]
[]
[]
[null,-1.89,-2.4860000000000002,-3.621,-2.5339999999999998,0]
[null,-28.297000000000001,-30.596,-35.658999999999999,-34.46,0]
[null,153.15299999999999,144.24100000000001,131.745,141.24799999999999,86.638000000000005]
[null,57.56,63.978000000000002,54.938000000000002,59.875999999999998,25.364999999999998]
[]
[null,"=-1890","=-2486","=-3621","=-2534","=0","=0","=0","=0","=0","=0"]
[null,-28.297000000000001,-30.596,-35.658999999999999,-34.46,0,0,0,0,0,0]
[null,"=153153","=144241","=131745","=141248","=86638","=0","=0","=0","=0","=0"]
[null,57.56,63.978000000000002,54.938000000000002,59.875999999999998,25.364999999999998,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-1890,-2486,-3621,-2534,0,0,0,0,0,0,-10531]
[null,"Ann peak Heating load kBtu/hr",-28.297000000000001,-30.596,-35.658999999999999,-34.46,0,0,0,0,0,0,-129.012]
[null,"HLH",66.791532671307905,81.252451300823637,101.54519195714967,73.534532791642476,"","","","","","","67-102",81.628065606300183]
["Cooling","Ann Cool Energy kBtu",153153,144241,131745,141248,86638,0,0,0,0,0,657025]
[null,"Ann peak Cooling load kBtu/hr",57.56,63.978000000000002,54.938000000000002,59.875999999999998,25.364999999999998,0,0,0,0,0,261.71699999999998]
[null,"CLH",2660.7539958304378,2254.5406233392728,2398.066911791474,2359.008617810141,3415.6514882712399,"","","","","","2255-3416",2510.4406668271454]
[]
["SCooper Rest 24 7days wo setback - Baseline Design.SIM"]
[null,-0.17599999999999999,-9.4949999999999992,215.97200000000001,64.628]
[null,-0.25700000000000001,-9.01,206.779,68.506]
[null,-0.48299999999999998,-26.591999999999999,191.92599999999999,58.758000000000003]
[null,-0.25700000000000001,-11.17,203.387,65.144999999999996]
[null,0,0,113.761,28.693000000000001]
[]
[]
[]
[]
[]
[]
[null,-0.17599999999999999,-0.25700000000000001,-0.48299999999999998,-0.25700000000000001,0]
[null,-9.4949999999999992,-9.01,-26.591999999999999,-11.17,0]
[null,215.97200000000001,206.779,191.92599999999999,203.387,113.761]
[null,64.628,68.506,58.758000000000003,65.144999999999996,28.693000000000001]
[]
[null,"=-176","=-257","=-483","=-257","=0","=0","=0","=0","=0","=0"]
[null,-9.4949999999999992,-9.01,-26.591999999999999,-11.17,0,0,0,0,0,0]
[null,"=215972","=206779","=191926","=203387","=113761","=0","=0","=0","=0","=0"]
[null,64.628,68.506,58.758000000000003,65.144999999999996,28.693000000000001,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-176,-257,-483,-257,0,0,0,0,0,0,-1173]
[null,"Ann peak Heating load kBtu/hr",-9.4949999999999992,-9.01,-26.591999999999999,-11.17,0,0,0,0,0,0,-56.266999999999996]
[null,"HLH",18.536071616640339,28.523862375138734,18.163357400722024,23.008057296329454,"","","","","","","18-29",20.847032896724546]
["Cooling","Ann Cool Energy kBtu",215972,206779,191926,203387,113761,0,0,0,0,0,931825]
[null,"Ann peak Cooling load kBtu/hr",64.628,68.506,58.758000000000003,65.144999999999996,28.693000000000001,0,0,0,0,0,285.73]
[null,"CLH",3341.7713684471128,3018.4071468192569,3266.3807481534427,3122.0661601043826,3964.7649252430906,"","","","","","3018-3965",3261.2081335526545]
[]
["SCooper Rest 10-23 7day Hol1 wo setback - Baseline Design.SIM"]
[null,-7.4029999999999996,-15.582000000000001,121.752,58.524999999999999]
[null,-10.220000000000001,-14.811,113.792,56.597000000000001]
[null,-13.021000000000001,-15.622999999999999,104.042,53.438000000000002]
[null,-10.811,-15.023,111.252,59.470999999999997]
[null,-0.56799999999999995,-4.5940000000000003,59.417000000000002,25.116]
[]
[]
[]
[]
[]
[]
[null,-7.4029999999999996,-10.220000000000001,-13.021000000000001,-10.811,-0.56799999999999995]
[null,-15.582000000000001,-14.811,-15.622999999999999,-15.023,-4.5940000000000003]
[null,121.752,113.792,104.042,111.252,59.417000000000002]
[null,58.524999999999999,56.597000000000001,53.438000000000002,59.470999999999997,25.116]
[]
[null,"=-7403","=-10220","=-13021","=-10811","=-568","=0","=0","=0","=0","=0"]
[null,-15.582000000000001,-14.811,-15.622999999999999,-15.023,-4.5940000000000003,0,0,0,0,0]
[null,"=121752","=113792","=104042","=111252","=59417","=0","=0","=0","=0","=0"]
[null,58.524999999999999,56.597000000000001,53.438000000000002,59.470999999999997,25.116,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-7403,-10220,-13021,-10811,-568,0,0,0,0,0,-42023]
[null,"Ann peak Heating load kBtu/hr",-15.582000000000001,-14.811,-15.622999999999999,-15.023,-4.5940000000000003,0,0,0,0,0,-65.632999999999996]
[null,"HLH",475.09947375176483,690.02768212814794,833.45068168725595,719.62990081874466,123.6395298215063,"","","","","","124-833",640.27242393308245]
["Cooling","Ann Cool Energy kBtu",121752,113792,104042,111252,59417,0,0,0,0,0,510255]
[null,"Ann peak Cooling load kBtu/hr",58.524999999999999,56.597000000000001,53.438000000000002,59.470999999999997,25.116,0,0,0,0,0,253.14699999999999]
[null,"CLH",2080.3417343015803,2010.5659310564163,1946.9665780904973,1870.6932790771973,2365.7031374422677,"","","","","","1871-2366",2015.6470351218857]
[]
["SCooper Rest 8-23 12-20 Hol2 wo setback - Baseline Design.SIM"]
[null,-3.359,-14.095000000000001,134.16399999999999,58.426000000000002]
[null,-4.0860000000000003,-13.332000000000001,124.82299999999999,62.176000000000002]
[null,-6.0519999999999996,-14.161,113.89700000000001,54.232999999999997]
[null,-4.8970000000000002,-13.521000000000001,122.452,59.658000000000001]
[null,0,0,71.188999999999993,25.286000000000001]
[]
[]
[]
[]
[]
[]
[null,-3.359,-4.0860000000000003,-6.0519999999999996,-4.8970000000000002,0]
[null,-14.095000000000001,-13.332000000000001,-14.161,-13.521000000000001,0]
[null,134.16399999999999,124.82299999999999,113.89700000000001,122.452,71.188999999999993]
[null,58.426000000000002,62.176000000000002,54.232999999999997,59.658000000000001,25.286000000000001]
[]
[null,"=-3359","=-4086","=-6052","=-4897","=0","=0","=0","=0","=0","=0"]
[null,-14.095000000000001,-13.332000000000001,-14.161,-13.521000000000001,0,0,0,0,0,0]
[null,"=134164","=124823","=113897","=122452","=71189","=0","=0","=0","=0","=0"]
[null,58.426000000000002,62.176000000000002,54.232999999999997,59.658000000000001,25.286000000000001,0,0,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-3359,-4086,-6052,-4897,0,0,0,0,0,0,-18394]
[null,"Ann peak Heating load kBtu/hr",-14.095000000000001,-13.332000000000001,-14.161,-13.521000000000001,0,0,0,0,0,0,-55.109000000000002]
[null,"HLH",238.31145796381693,306.48064806480647,427.37094837935177,362.17735374602466,"","","","","","","238-427",333.77488250557985]
["Cooling","Ann Cool Energy kBtu",134164,124823,113897,122452,71189,0,0,0,0,0,566525]
[null,"Ann peak Cooling load kBtu/hr",58.426000000000002,62.176000000000002,54.232999999999997,59.658000000000001,25.286000000000001,0,0,0,0,0,259.779]
[null,"CLH",2296.3064389141819,2007.5752702007205,2100.1419799752921,2052.5662945455765,2815.3523688997861,"","","","","","2008-2815",2180.7959842789446]
[]
[]
["SCooper Htl 9-18 wo setback - Baseline Design.SIM"]
[null,-7.2249999999999996,-15.151,57.978000000000002,37.743000000000002]
[null,-11.643000000000001,-19.236999999999998,38.085000000000001,29.38]
[null,-12.419,-19.135000000000002,37.395000000000003,31.51]
[null,-10.457000000000001,-16.073,51.045999999999999,43.820999999999998]
[null,-0.161,-3.52,7.6779999999999999,4.34]
[null,-8.18,-17.148,81.510999999999996,58.488]
[null,-10.89,-17.896000000000001,54.276000000000003,37.652999999999999]
[null,-11.048,-17.779,55.235999999999997,41.468000000000004]
[null,-10.113,-17.395,71.064999999999998,61.790999999999997]
[null,-0.68,-4.742,7.5350000000000001,5.4240000000000004]
[]
[null,-7.2249999999999996,-11.643000000000001,-12.419,-10.457000000000001,-0.161,-8.18,-10.89,-11.048,-10.113,-0.68]
[null,-15.151,-19.236999999999998,-19.135000000000002,-16.073,-3.52,-17.148,-17.896000000000001,-17.779,-17.395,-4.742]
[null,57.978000000000002,38.085000000000001,37.395000000000003,51.045999999999999,7.6779999999999999,81.510999999999996,54.276000000000003,55.235999999999997,71.064999999999998,7.5350000000000001]
[null,37.743000000000002,29.38,31.51,43.820999999999998,4.34,58.488,37.652999999999999,41.468000000000004,61.790999999999997,5.4240000000000004]
[]
[null,"=-7225","=-11643","=-12419","=-10457","=-161","=-8180","=-10890","=-11048","=-10113","=-680"]
[null,-15.151,-19.236999999999998,-19.135000000000002,-16.073,-3.52,-17.148,-17.896000000000001,-17.779,-17.395,-4.742]
[null,"=57978","=38085","=37395","=51046","=7678","=81511","=54276","=55236","=71065","=7535"]
[null,37.743000000000002,29.38,31.51,43.820999999999998,4.34,58.488,37.652999999999999,41.468000000000004,61.790999999999997,5.4240000000000004]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-7225,-11643,-12419,-10457,-161,-8180,-10890,-11048,-10113,-680,-82816]
[null,"Ann peak Heating load kBtu/hr",-15.151,-19.236999999999998,-19.135000000000002,-16.073,-3.52,-17.148,-17.896000000000001,-17.779,-17.395,-4.742,-148.07599999999999]
[null,"HLH",476.86621345125735,605.23990227166405,649.02012019858887,650.59416412617429,45.738636363636367,477.02355959878702,608.51586946803752,621.40727824962039,581.3739580339178,143.39940953184311,"46-651",559.28036953996593]
["Cooling","Ann Cool Energy kBtu",57978,38085,37395,51046,7678,81511,54276,55236,71065,7535,461805]
[null,"Ann peak Cooling load kBtu/hr",37.743000000000002,29.38,31.51,43.820999999999998,4.34,58.488,37.652999999999999,41.468000000000004,61.790999999999997,5.4240000000000004,351.61799999999999]
[null,"CLH",1536.1259041411652,1296.2899931926481,1186.7661059980958,1164.8752881038772,1769.1244239631337,1393.6363014635481,1441.4787666321408,1332.0150477476607,1150.0865821883447,1389.1961651917404,"1150-1769",1313.371329112844]
[]
["SCooper Htl 8-21 wo setback - Baseline Design.SIM"]
[null,-7.7869999999999999,-16.492999999999999,59.01,37.634]
[null,-12.507,-19.483000000000001,39.186,29.492999999999999]
[null,-13.27,-19.382000000000001,38.515000000000001,31.55]
[null,-11.122999999999999,-17.59,52.423999999999999,43.823999999999998]
[null,-0.308,-3.609,7.84,5.274]
[null,-8.4550000000000001,-17.145,83.025999999999996,58.421999999999997]
[null,-11.583,-18.768000000000001,55.537999999999997,37.671999999999997]
[null,-11.702,-18.576000000000001,56.539000000000001,41.478999999999999]
[null,-10.47,-17.393000000000001,72.846000000000004,61.790999999999997]
[null,-0.92800000000000005,-5.2290000000000001,8.1010000000000009,7.0309999999999997]
[]
[null,-7.7869999999999999,-12.507,-13.27,-11.122999999999999,-0.308,-8.4550000000000001,-11.583,-11.702,-10.47,-0.92800000000000005]
[null,-16.492999999999999,-19.483000000000001,-19.382000000000001,-17.59,-3.609,-17.145,-18.768000000000001,-18.576000000000001,-17.393000000000001,-5.2290000000000001]
[null,59.01,39.186,38.515000000000001,52.423999999999999,7.84,83.025999999999996,55.537999999999997,56.539000000000001,72.846000000000004,8.1010000000000009]
[null,37.634,29.492999999999999,31.55,43.823999999999998,5.274,58.421999999999997,37.671999999999997,41.478999999999999,61.790999999999997,7.0309999999999997]
[]
[null,"=-7787","=-12507","=-13270","=-11123","=-308","=-8455","=-11583","=-11702","=-10470","=-928"]
[null,-16.492999999999999,-19.483000000000001,-19.382000000000001,-17.59,-3.609,-17.145,-18.768000000000001,-18.576000000000001,-17.393000000000001,-5.2290000000000001]
[null,"=59010","=39186","=38515","=52424","=7840","=83026","=55538","=56539","=72846","=8101"]
[null,37.634,29.492999999999999,31.55,43.823999999999998,5.274,58.421999999999997,37.671999999999997,41.478999999999999,61.790999999999997,7.0309999999999997]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-7787,-12507,-13270,-11123,-308,-8455,-11583,-11702,-10470,-928,-88133]
[null,"Ann peak Heating load kBtu/hr",-16.492999999999999,-19.483000000000001,-19.382000000000001,-17.59,-3.609,-17.145,-18.768000000000001,-18.576000000000001,-17.393000000000001,-5.2290000000000001,-153.66800000000001]
[null,"HLH",472.13969562844846,641.94425909767483,684.65586626767094,632.34792495736212,85.34220005541701,493.14668999708368,617.1675191815857,629.95262704565027,601.96630828494222,177.47179192962327,"85-685",573.52864617226749]
["Cooling","Ann Cool Energy kBtu",59010,39186,38515,52424,7840,83026,55538,56539,72846,8101,473025]
[null,"Ann peak Cooling load kBtu/hr",37.634,29.492999999999999,31.55,43.823999999999998,5.274,58.421999999999997,37.671999999999997,41.478999999999999,61.790999999999997,7.0309999999999997,354.16999999999996]
[null,"CLH",1567.9970239676888,1328.6542569423254,1220.7606973058637,1196.2395034684191,1486.5377322715206,1421.1427202081409,1474.2514334253558,1363.0752911111647,1178.9095499344564,1152.1831887355995,"1152-1568",1335.587429765367]
[]
["SCooper Htl 9-22 7days wo setback - Baseline Design.SIM"]
[null,-6.8490000000000002,-17.221,64.808000000000007,37.692999999999998]
[null,-11.65,-19.451000000000001,44.51,30.847999999999999]
[null,-12.324999999999999,-19.332000000000001,43.701999999999998,31.751999999999999]
[null,-10.144,-20.652999999999999,58.091000000000001,43.823999999999998]
[null,-0.41,-4.2279999999999998,11.143000000000001,5.3419999999999996]
[null,-7.2839999999999998,-16.026,90.061000000000007,59.83]
[null,-10.564,-19.091000000000001,61.512,38.844000000000001]
[null,-10.64,-18.847999999999999,62.594999999999999,42.142000000000003]
[null,-9.3209999999999997,-20.611000000000001,79.539000000000001,61.79]
[null,-0.88300000000000001,-5.6180000000000003,11.1,7.0259999999999998]
[]
[null,-6.8490000000000002,-11.65,-12.324999999999999,-10.144,-0.41,-7.2839999999999998,-10.564,-10.64,-9.3209999999999997,-0.88300000000000001]
[null,-17.221,-19.451000000000001,-19.332000000000001,-20.652999999999999,-4.2279999999999998,-16.026,-19.091000000000001,-18.847999999999999,-20.611000000000001,-5.6180000000000003]
[null,64.808000000000007,44.51,43.701999999999998,58.091000000000001,11.143000000000001,90.061000000000007,61.512,62.594999999999999,79.539000000000001,11.1]
[null,37.692999999999998,30.847999999999999,31.751999999999999,43.823999999999998,5.3419999999999996,59.83,38.844000000000001,42.142000000000003,61.79,7.0259999999999998]
[]
[null,"=-6849","=-11650","=-12325","=-10144","=-410","=-7284","=-10564","=-10640","=-9321","=-883"]
[null,-17.221,-19.451000000000001,-19.332000000000001,-20.652999999999999,-4.2279999999999998,-16.026,-19.091000000000001,-18.847999999999999,-20.611000000000001,-5.6180000000000003]
[null,"=64808","=44510","=43702","=58091","=11143","=90061","=61512","=62595","=79539","=11100"]
[null,37.692999999999998,30.847999999999999,31.751999999999999,43.823999999999998,5.3419999999999996,59.83,38.844000000000001,42.142000000000003,61.79,7.0259999999999998]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-6849,-11650,-12325,-10144,-410,-7284,-10564,-10640,-9321,-883,-80070]
[null,"Ann peak Heating load kBtu/hr",-17.221,-19.451000000000001,-19.332000000000001,-20.652999999999999,-4.2279999999999998,-16.026,-19.091000000000001,-18.847999999999999,-20.611000000000001,-5.6180000000000003,-161.07899999999995]
[null,"HLH",397.71209569711397,598.94092848696721,637.54396854955507,491.16351135428272,96.972563859981079,454.51141894421568,553.34974595359063,564.51612903225805,452.23424385037117,157.17337130651475,"97-638",497.08528113534368]
["Cooling","Ann Cool Energy kBtu",64808,44510,43702,58091,11143,90061,61512,62595,79539,11100,527061]
[null,"Ann peak Cooling load kBtu/hr",37.692999999999998,30.847999999999999,31.751999999999999,43.823999999999998,5.3419999999999996,59.83,38.844000000000001,42.142000000000003,61.79,7.0259999999999998,359.09100000000001]
[null,"CLH",1719.3643382060332,1442.8812240663901,1376.3542454018645,1325.5522088353414,2085.9228753275929,1505.2816312886512,1583.5650293481619,1485.3352949551515,1287.2471273668878,1579.8462852263024,"1287-2086",1467.7644385406484]
[]
["SCooper Htl 8-22 7days wo setback - Baseline Design.SIM"]
[null,-7.1909999999999998,-20.548999999999999,64.997,37.630000000000003]
[null,-12.099,-22.465,44.826000000000001,30.863]
[null,-12.78,-22.626000000000001,44.036999999999999,31.72]
[null,-10.541,-22.59,58.295999999999999,43.825000000000003]
[null,-0.52600000000000002,-4.484,11.147,5.3440000000000003]
[null,-7.4980000000000002,-21.170999999999999,90.403000000000006,59.83]
[null,-10.945,-23.12,61.904000000000003,38.86]
[null,-10.997,-23.254999999999999,63.012999999999998,42.131]
[null,-9.5960000000000001,-23.015000000000001,79.832999999999998,61.790999999999997]
[null,-1.0960000000000001,-5.9660000000000002,11.188000000000001,7.0270000000000001]
[]
[null,-7.1909999999999998,-12.099,-12.78,-10.541,-0.52600000000000002,-7.4980000000000002,-10.945,-10.997,-9.5960000000000001,-1.0960000000000001]
[null,-20.548999999999999,-22.465,-22.626000000000001,-22.59,-4.484,-21.170999999999999,-23.12,-23.254999999999999,-23.015000000000001,-5.9660000000000002]
[null,64.997,44.826000000000001,44.036999999999999,58.295999999999999,11.147,90.403000000000006,61.904000000000003,63.012999999999998,79.832999999999998,11.188000000000001]
[null,37.630000000000003,30.863,31.72,43.825000000000003,5.3440000000000003,59.83,38.86,42.131,61.790999999999997,7.0270000000000001]
[]
[null,"=-7191","=-12099","=-12780","=-10541","=-526","=-7498","=-10945","=-10997","=-9596","=-1096"]
[null,-20.548999999999999,-22.465,-22.626000000000001,-22.59,-4.484,-21.170999999999999,-23.12,-23.254999999999999,-23.015000000000001,-5.9660000000000002]
[null,"=64997","=44826","=44037","=58296","=11147","=90403","=61904","=63013","=79833","=11188"]
[null,37.630000000000003,30.863,31.72,43.825000000000003,5.3440000000000003,59.83,38.86,42.131,61.790999999999997,7.0270000000000001]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-7191,-12099,-12780,-10541,-526,-7498,-10945,-10997,-9596,-1096,-83269]
[null,"Ann peak Heating load kBtu/hr",-20.548999999999999,-22.465,-22.626000000000001,-22.59,-4.484,-21.170999999999999,-23.12,-23.254999999999999,-23.015000000000001,-5.9660000000000002,-189.24099999999999]
[null,"HLH",349.94403620614145,538.5711106165146,564.83691328560064,466.62239929172199,117.30597680642283,354.16371451513862,473.39965397923874,472.88755106428727,416.94547034542688,183.7076768354006,"117-565",440.0156414307682]
["Cooling","Ann Cool Energy kBtu",64997,44826,44037,58296,11147,90403,61904,63013,79833,11188,529644]
[null,"Ann peak Cooling load kBtu/hr",37.630000000000003,30.863,31.72,43.825000000000003,5.3440000000000003,59.83,38.86,42.131,61.790999999999997,7.0270000000000001,359.02099999999996]
[null,"CLH",1727.2654796704755,1452.4187538476492,1388.3039092055485,1330.1996577296063,2085.8907185628741,1510.9978271770015,1593.0005146680392,1495.6445372765897,1291.9842695538186,1592.1445851714814,"1292-2086",1475.2451806440295]
[]
["SCooper Htl 5-23 7days wo setback - Baseline Design.SIM"]
[null,-8.6150000000000002,-22.581,65.73,37.615000000000002]
[null,-14.048,-24.216999999999999,45.337000000000003,30.853999999999999]
[null,-14.664,-24.091999999999999,44.566000000000003,31.675999999999998]
[null,-12.073,-23.602,59.005000000000003,43.826000000000001]
[null,-1.0149999999999999,-4.4740000000000002,10.968999999999999,5.367]
[null,-8.3010000000000002,-23.138999999999999,91.777000000000001,59.831000000000003]
[null,-12.586,-25.029,62.555999999999997,38.832999999999998]
[null,-12.523,-24.779,63.735999999999997,42.122]
[null,-10.603999999999999,-23.815000000000001,81.004999999999995,61.790999999999997]
[null,-1.9279999999999999,-6.1390000000000002,11.494,7.0279999999999996]
[]
[null,-8.6150000000000002,-14.048,-14.664,-12.073,-1.0149999999999999,-8.3010000000000002,-12.586,-12.523,-10.603999999999999,-1.9279999999999999]
[null,-22.581,-24.216999999999999,-24.091999999999999,-23.602,-4.4740000000000002,-23.138999999999999,-25.029,-24.779,-23.815000000000001,-6.1390000000000002]
[null,65.73,45.337000000000003,44.566000000000003,59.005000000000003,10.968999999999999,91.777000000000001,62.555999999999997,63.735999999999997,81.004999999999995,11.494]
[null,37.615000000000002,30.853999999999999,31.675999999999998,43.826000000000001,5.367,59.831000000000003,38.832999999999998,42.122,61.790999999999997,7.0279999999999996]
[]
[null,"=-8615","=-14048","=-14664","=-12073","=-1015","=-8301","=-12586","=-12523","=-10604","=-1928"]
[null,-22.581,-24.216999999999999,-24.091999999999999,-23.602,-4.4740000000000002,-23.138999999999999,-25.029,-24.779,-23.815000000000001,-6.1390000000000002]
[null,"=65730","=45337","=44566","=59005","=10969","=91777","=62556","=63736","=81005","=11494"]
[null,37.615000000000002,30.853999999999999,31.675999999999998,43.826000000000001,5.367,59.831000000000003,38.832999999999998,42.122,61.790999999999997,7.0279999999999996]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-8615,-14048,-14664,-12073,-1015,-8301,-12586,-12523,-10604,-1928,-96357]
[null,"Ann peak Heating load kBtu/hr",-22.581,-24.216999999999999,-24.091999999999999,-23.602,-4.4740000000000002,-23.138999999999999,-25.029,-24.779,-23.815000000000001,-6.1390000000000002,-201.86700000000002]
[null,"HLH",381.51543332890486,580.08836767559978,608.66677735347832,511.52444708075586,226.86633884666963,358.74497601452094,502.85668624395703,505.38762661931474,445.26558891454965,314.05766411467664,"227-609",477.32913254766748]
["Cooling","Ann Cool Energy kBtu",65730,45337,44566,59005,10969,91777,62556,63736,81005,11494,536175]
[null,"Ann peak Cooling load kBtu/hr",37.615000000000002,30.853999999999999,31.675999999999998,43.826000000000001,5.367,59.831000000000003,38.832999999999998,42.122,61.790999999999997,7.0279999999999996,358.94299999999998]
[null,"CLH",1747.4411803801675,1469.4042911778051,1406.9326935219094,1346.3469173549947,2043.786100242221,1533.9372566061072,1610.8979476218681,1513.128531408765,1310.9514330565942,1635.4581673306775,"1311-2044",1493.7608478226348]
[]
["SCooper Htl 24 7days wo setback - Baseline Design.SIM"]
[null,-10.093999999999999,-22.568999999999999,66.811000000000007,37.610999999999997]
[null,-16.138999999999999,-24.207000000000001,46.026000000000003,30.856999999999999]
[null,-16.678000000000001,-24.082000000000001,45.281999999999996,31.678999999999998]
[null,-13.646000000000001,-23.59,59.993000000000002,43.825000000000003]
[null,-1.659,-4.4820000000000002,10.875999999999999,5.3719999999999999]
[null,-8.9659999999999993,-23.094000000000001,93.628,59.838000000000001]
[null,-14.271000000000001,-24.986000000000001,63.43,38.835000000000001]
[null,-14.069000000000001,-24.734999999999999,64.706000000000003,42.125]
[null,-11.512,-23.77,82.522999999999996,61.792000000000002]
[null,-2.944,-6.1870000000000003,11.975,7.03]
[]
[null,-10.093999999999999,-16.138999999999999,-16.678000000000001,-13.646000000000001,-1.659,-8.9659999999999993,-14.271000000000001,-14.069000000000001,-11.512,-2.944]
[null,-22.568999999999999,-24.207000000000001,-24.082000000000001,-23.59,-4.4820000000000002,-23.094000000000001,-24.986000000000001,-24.734999999999999,-23.77,-6.1870000000000003]
[null,66.811000000000007,46.026000000000003,45.281999999999996,59.993000000000002,10.875999999999999,93.628,63.43,64.706000000000003,82.522999999999996,11.975]
[null,37.610999999999997,30.856999999999999,31.678999999999998,43.825000000000003,5.3719999999999999,59.838000000000001,38.835000000000001,42.125,61.792000000000002,7.03]
[]
[null,"=-10094","=-16139","=-16678","=-13646","=-1659","=-8966","=-14271","=-14069","=-11512","=-2944"]
[null,-22.568999999999999,-24.207000000000001,-24.082000000000001,-23.59,-4.4820000000000002,-23.094000000000001,-24.986000000000001,-24.734999999999999,-23.77,-6.1870000000000003]
[null,"=66811","=46026","=45282","=59993","=10876","=93628","=63430","=64706","=82523","=11975"]
[null,37.610999999999997,30.856999999999999,31.678999999999998,43.825000000000003,5.3719999999999999,59.838000000000001,38.835000000000001,42.125,61.792000000000002,7.03]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-10094,-16139,-16678,-13646,-1659,-8966,-14271,-14069,-11512,-2944,-109978]
[null,"Ann peak Heating load kBtu/hr",-22.568999999999999,-24.207000000000001,-24.082000000000001,-23.59,-4.4820000000000002,-23.094000000000001,-24.986000000000001,-24.734999999999999,-23.77,-6.1870000000000003,-201.70200000000003]
[null,"HLH",447.25065355133148,666.70797703143717,692.55045262021429,578.46545146248411,370.14725568942436,388.23936953321208,571.15984951572875,568.78916515059632,484.30795119899034,475.8364312267658,"370-693",545.24992315395968]
["Cooling","Ann Cool Energy kBtu",66811,46026,45282,59993,10876,93628,63430,64706,82523,11975,545250]
[null,"Ann peak Cooling load kBtu/hr",37.610999999999997,30.856999999999999,31.678999999999998,43.825000000000003,5.3719999999999999,59.838000000000001,38.835000000000001,42.125,61.792000000000002,7.03,358.96399999999994]
[null,"CLH",1776.3686155645955,1491.5902388436984,1429.4011805928219,1368.9218482601254,2024.571854058079,1564.6913332664863,1633.3204583494271,1536.0474777448071,1335.4965044018643,1703.4139402560454,"1335-2025",1518.9545469740701]
[]
[]
["SCooper Rtl 9-18 wo setback - Baseline Design.SIM"]
[null,-13.013,-36.314,168.83099999999999,119.559]
[null,-7.4160000000000004,-15.86,79.677000000000007,48.908999999999999]
[null,-6.9130000000000003,-22.606000000000002,111.598,79.64]
[null,-5.1310000000000002,-22.353000000000002,133.786,84.436999999999998]
[null,-8.0429999999999993,-17.291,61.155000000000001,44.341999999999999]
[null,-14.888,-37.226999999999997,213.048,141.14699999999999]
[null,-0.17599999999999999,-9.5280000000000005,16.908999999999999,15.243]
[]
[]
[]
[]
[null,-13.013,-7.4160000000000004,-6.9130000000000003,-5.1310000000000002,-8.0429999999999993,-14.888,-0.17599999999999999]
[null,-36.314,-15.86,-22.606000000000002,-22.353000000000002,-17.291,-37.226999999999997,-9.5280000000000005]
[null,168.83099999999999,79.677000000000007,111.598,133.786,61.155000000000001,213.048,16.908999999999999]
[null,119.559,48.908999999999999,79.64,84.436999999999998,44.341999999999999,141.14699999999999,15.243]
[]
[null,"=-13013","=-7416","=-6913","=-5131","=-8043","=-14888","=-176","=0","=0","=0"]
[null,-36.314,-15.86,-22.606000000000002,-22.353000000000002,-17.291,-37.226999999999997,-9.5280000000000005,0,0,0]
[null,"=168831","=79677","=111598","=133786","=61155","=213048","=16909","=0","=0","=0"]
[null,119.559,48.908999999999999,79.64,84.436999999999998,44.341999999999999,141.14699999999999,15.243,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-13013,-7416,-6913,-5131,-8043,-14888,-176,0,0,0,-55580]
[null,"Ann peak Heating load kBtu/hr",-36.314,-15.86,-22.606000000000002,-22.353000000000002,-17.291,-37.226999999999997,-9.5280000000000005,0,0,0,-161.179]
[null,"HLH",358.34664316792424,467.59142496847414,305.80376891090856,229.54413277859794,465.15528309525183,399.92478577376636,18.47187237615449,"","","","18-468",344.83400442985749]
["Cooling","Ann Cool Energy kBtu",168831,79677,111598,133786,61155,213048,16909,0,0,0,785004]
[null,"Ann peak Cooling load kBtu/hr",119.559,48.908999999999999,79.64,84.436999999999998,44.341999999999999,141.14699999999999,15.243,0,0,0,533.27700000000004]
[null,"CLH",1412.1145208641758,1629.0866711648164,1401.2807634354594,1584.4475762994896,1379.1664787334807,1509.4050883121852,1109.2960703273634,"","","","1109-1629",1472.0379840120611]
[]
["SCooper Rtl 8-20 wo setback - Baseline Design.SIM"]
[null,-10.997,-32.35,201.58600000000001,122.21299999999999]
[null,-6.6970000000000001,-13.56,89.462999999999994,49.892000000000003]
[null,-5.8479999999999999,-19.413,134.96199999999999,82.465000000000003]
[null,-4.2690000000000001,-19.183,157.172,85.822000000000003]
[null,-7.1550000000000002,-14.569000000000001,70.486000000000004,45.6]
[null,-13.132999999999999,-33.100999999999999,246.334,158.34200000000001]
[null,-0.73199999999999998,-11.776999999999999,21.619,16.126000000000001]
[]
[]
[]
[]
[null,-10.997,-6.6970000000000001,-5.8479999999999999,-4.2690000000000001,-7.1550000000000002,-13.132999999999999,-0.73199999999999998]
[null,-32.35,-13.56,-19.413,-19.183,-14.569000000000001,-33.100999999999999,-11.776999999999999]
[null,201.58600000000001,89.462999999999994,134.96199999999999,157.172,70.486000000000004,246.334,21.619]
[null,122.21299999999999,49.892000000000003,82.465000000000003,85.822000000000003,45.6,158.34200000000001,16.126000000000001]
[]
[null,"=-10997","=-6697","=-5848","=-4269","=-7155","=-13133","=-732","=0","=0","=0"]
[null,-32.35,-13.56,-19.413,-19.183,-14.569000000000001,-33.100999999999999,-11.776999999999999,0,0,0]
[null,"=201586","=89463","=134962","=157172","=70486","=246334","=21619","=0","=0","=0"]
[null,122.21299999999999,49.892000000000003,82.465000000000003,85.822000000000003,45.6,158.34200000000001,16.126000000000001,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-10997,-6697,-5848,-4269,-7155,-13133,-732,0,0,0,-48831]
[null,"Ann peak Heating load kBtu/hr",-32.35,-13.56,-19.413,-19.183,-14.569000000000001,-33.100999999999999,-11.776999999999999,0,0,0,-143.95299999999997]
[null,"HLH",339.93817619783613,493.87905604719759,301.24143615103281,222.54079132565292,491.11126364197952,396.75538503368477,62.155047974866271,"","","","62-494",339.21488263530466]
["Cooling","Ann Cool Energy kBtu",201586,89463,134962,157172,70486,246334,21619,0,0,0,921622]
[null,"Ann peak Cooling load kBtu/hr",122.21299999999999,49.892000000000003,82.465000000000003,85.822000000000003,45.6,158.34200000000001,16.126000000000001,0,0,0,560.46]
[null,"CLH",1649.464459591042,1793.1331676421069,1636.5973443278965,1831.3719093006455,1545.7456140350878,1555.7085296383775,1340.6300384472279,"","","","1341-1831",1644.4028119758768]
[]
["SCooper Rtl 7-22 wo setback - Baseline Design.SIM"]
[null,-8.9760000000000009,-42.521999999999998,234.12,122.70699999999999]
[null,-5.9420000000000002,-16.402999999999999,98.808000000000007,50.883000000000003]
[null,-4.593,-23.876999999999999,158.20500000000001,84.751000000000005]
[null,-3.5470000000000002,-23.068999999999999,179.999,87.638999999999996]
[null,-6.1909999999999998,-18.981000000000002,79.703999999999994,46.209000000000003]
[null,-10.776999999999999,-37.552999999999997,279.10399999999998,160.405]
[null,-0.72799999999999998,-12.49,26.754999999999999,16.943999999999999]
[]
[]
[]
[]
[null,-8.9760000000000009,-5.9420000000000002,-4.593,-3.5470000000000002,-6.1909999999999998,-10.776999999999999,-0.72799999999999998]
[null,-42.521999999999998,-16.402999999999999,-23.876999999999999,-23.068999999999999,-18.981000000000002,-37.552999999999997,-12.49]
[null,234.12,98.808000000000007,158.20500000000001,179.999,79.703999999999994,279.10399999999998,26.754999999999999]
[null,122.70699999999999,50.883000000000003,84.751000000000005,87.638999999999996,46.209000000000003,160.405,16.943999999999999]
[]
[null,"=-8976","=-5942","=-4593","=-3547","=-6191","=-10777","=-728","=0","=0","=0"]
[null,-42.521999999999998,-16.402999999999999,-23.876999999999999,-23.068999999999999,-18.981000000000002,-37.552999999999997,-12.49,0,0,0]
[null,"=234120","=98808","=158205","=179999","=79704","=279104","=26755","=0","=0","=0"]
[null,122.70699999999999,50.883000000000003,84.751000000000005,87.638999999999996,46.209000000000003,160.405,16.943999999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-8976,-5942,-4593,-3547,-6191,-10777,-728,0,0,0,-40754]
[null,"Ann peak Heating load kBtu/hr",-42.521999999999998,-16.402999999999999,-23.876999999999999,-23.068999999999999,-18.981000000000002,-37.552999999999997,-12.49,0,0,0,-174.89500000000001]
[null,"HLH",211.09072950472697,362.25080777906481,192.3608493529338,153.75612293554121,326.16827353669458,286.98106675898066,58.286629303442751,"","","","58-362",233.01981188713228]
["Cooling","Ann Cool Energy kBtu",234120,98808,158205,179999,79704,279104,26755,0,0,0,1056695]
[null,"Ann peak Cooling load kBtu/hr",122.70699999999999,50.883000000000003,84.751000000000005,87.638999999999996,46.209000000000003,160.405,16.943999999999999,0,0,0,569.53800000000001]
[null,"CLH",1907.959611106131,1941.8666352219798,1866.7036377151892,2053.8687114184327,1724.8587937414788,1739.9956360462579,1579.0250236071768,"","","","1579-2054",1855.3546909951574]
[]
["SCooper Rtl 9-22 7days wo setback - Baseline Design.SIM"]
[null,-9.2119999999999997,-39.600999999999999,235.7,122.042]
[null,-5.7069999999999999,-16.289000000000001,99.637,49.622999999999998]
[null,-4.5609999999999999,-24.768000000000001,159.84399999999999,84.105000000000004]
[null,-3.157,-24.593,182.006,86.091999999999999]
[null,-6.3760000000000003,-18.122,80.879000000000005,45.942]
[null,-11.087999999999999,-36.570999999999998,280.63,159.245]
[null,-0.90900000000000003,-10.766,29.248000000000001,16.914999999999999]
[]
[]
[]
[]
[null,-9.2119999999999997,-5.7069999999999999,-4.5609999999999999,-3.157,-6.3760000000000003,-11.087999999999999,-0.90900000000000003]
[null,-39.600999999999999,-16.289000000000001,-24.768000000000001,-24.593,-18.122,-36.570999999999998,-10.766]
[null,235.7,99.637,159.84399999999999,182.006,80.879000000000005,280.63,29.248000000000001]
[null,122.042,49.622999999999998,84.105000000000004,86.091999999999999,45.942,159.245,16.914999999999999]
[]
[null,"=-9212","=-5707","=-4561","=-3157","=-6376","=-11088","=-909","=0","=0","=0"]
[null,-39.600999999999999,-16.289000000000001,-24.768000000000001,-24.593,-18.122,-36.570999999999998,-10.766,0,0,0]
[null,"=235700","=99637","=159844","=182006","=80879","=280630","=29248","=0","=0","=0"]
[null,122.042,49.622999999999998,84.105000000000004,86.091999999999999,45.942,159.245,16.914999999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-9212,-5707,-4561,-3157,-6376,-11088,-909,0,0,0,-41010]
[null,"Ann peak Heating load kBtu/hr",-39.600999999999999,-16.289000000000001,-24.768000000000001,-24.593,-18.122,-36.570999999999998,-10.766,0,0,0,-170.71]
[null,"HLH",232.62038837403097,350.35913806863522,184.14890180878552,128.36986134265848,351.83754552477654,303.19105302015259,84.43247259892253,"","","","84-352",240.23197235077029]
["Cooling","Ann Cool Energy kBtu",235700,99637,159844,182006,80879,280630,29248,0,0,0,1067944]
[null,"Ann peak Cooling load kBtu/hr",122.042,49.622999999999998,84.105000000000004,86.091999999999999,45.942,159.245,16.914999999999999,0,0,0,563.96399999999994]
[null,"CLH",1931.3023385391914,2007.8794107571086,1900.5291005291003,2114.0872554941225,1760.4588394062077,1762.2531319664668,1729.1161690806978,"","","","1729-2114",1893.6386010454571]
[]
["SCooper Rtl 8-22 7days wo setback - Baseline Design.SIM"]
[null,-6.4729999999999999,-75.453999999999994,265.80599999999998,123.01600000000001]
[null,-4.7569999999999997,-25.888999999999999,108.001,54.762]
[null,-2.9159999999999999,-49.765000000000001,181.11600000000001,84.9]
[null,-2.016,-48.942999999999998,203.15700000000001,94.86]
[null,-5.1020000000000003,-26.263999999999999,89.221000000000004,46.268000000000001]
[null,-8.1940000000000008,-76.691000000000003,310.28899999999999,161.03399999999999]
[null,-0.82599999999999996,-11.79,32.432000000000002,17.181999999999999]
[]
[]
[]
[]
[null,-6.4729999999999999,-4.7569999999999997,-2.9159999999999999,-2.016,-5.1020000000000003,-8.1940000000000008,-0.82599999999999996]
[null,-75.453999999999994,-25.888999999999999,-49.765000000000001,-48.942999999999998,-26.263999999999999,-76.691000000000003,-11.79]
[null,265.80599999999998,108.001,181.11600000000001,203.15700000000001,89.221000000000004,310.28899999999999,32.432000000000002]
[null,123.01600000000001,54.762,84.9,94.86,46.268000000000001,161.03399999999999,17.181999999999999]
[]
[null,"=-6473","=-4757","=-2916","=-2016","=-5102","=-8194","=-826","=0","=0","=0"]
[null,-75.453999999999994,-25.888999999999999,-49.765000000000001,-48.942999999999998,-26.263999999999999,-76.691000000000003,-11.79,0,0,0]
[null,"=265806","=108001","=181116","=203157","=89221","=310289","=32432","=0","=0","=0"]
[null,123.01600000000001,54.762,84.9,94.86,46.268000000000001,161.03399999999999,17.181999999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-6473,-4757,-2916,-2016,-5102,-8194,-826,0,0,0,-30284]
[null,"Ann peak Heating load kBtu/hr",-75.453999999999994,-25.888999999999999,-49.765000000000001,-48.942999999999998,-26.263999999999999,-76.691000000000003,-11.79,0,0,0,-314.79599999999999]
[null,"HLH",85.787367137593776,183.74599250646995,58.595398372350047,41.190772939950556,194.2583003350594,106.84434940214628,70.059372349448694,"","","","41-194",96.201984777443172]
["Cooling","Ann Cool Energy kBtu",265806,108001,181116,203157,89221,310289,32432,0,0,0,1190022]
[null,"Ann peak Cooling load kBtu/hr",123.01600000000001,54.762,84.9,94.86,46.268000000000001,161.03399999999999,17.181999999999999,0,0,0,582.02200000000005]
[null,"CLH",2160.7433179423815,1972.1887440195756,2133.2862190812721,2141.6508538899429,1928.3522088700613,1926.8539563073637,1887.5567454312654,"","","","1888-2161",2044.6340516337868]
[]
["SCooper Rtl 5-23 7days wo setback - Baseline Design.SIM"]
[null,-3.5979999999999999,-53.731000000000002,314.988,123.804]
[null,-3.1640000000000001,-19.117000000000001,122.39400000000001,52.234000000000002]
[null,-1.593,-27.571000000000002,216.703,85.281999999999996]
[null,-1.3260000000000001,-27.709,237.374,90.766999999999996]
[null,-3.3319999999999999,-23.021000000000001,103.794,46.402999999999999]
[null,-4.4939999999999998,-46.076999999999998,358.96,161.387]
[null,-0.69299999999999995,-11.366,41.601999999999997,17.123999999999999]
[]
[]
[]
[]
[null,-3.5979999999999999,-3.1640000000000001,-1.593,-1.3260000000000001,-3.3319999999999999,-4.4939999999999998,-0.69299999999999995]
[null,-53.731000000000002,-19.117000000000001,-27.571000000000002,-27.709,-23.021000000000001,-46.076999999999998,-11.366]
[null,314.988,122.39400000000001,216.703,237.374,103.794,358.96,41.601999999999997]
[null,123.804,52.234000000000002,85.281999999999996,90.766999999999996,46.402999999999999,161.387,17.123999999999999]
[]
[null,"=-3598","=-3164","=-1593","=-1326","=-3332","=-4494","=-693","=0","=0","=0"]
[null,-53.731000000000002,-19.117000000000001,-27.571000000000002,-27.709,-23.021000000000001,-46.076999999999998,-11.366,0,0,0]
[null,"=314988","=122394","=216703","=237374","=103794","=358960","=41602","=0","=0","=0"]
[null,123.804,52.234000000000002,85.281999999999996,90.766999999999996,46.402999999999999,161.387,17.123999999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-3598,-3164,-1593,-1326,-3332,-4494,-693,0,0,0,-18200]
[null,"Ann peak Heating load kBtu/hr",-53.731000000000002,-19.117000000000001,-27.571000000000002,-27.709,-23.021000000000001,-46.076999999999998,-11.366,0,0,0,-208.59199999999998]
[null,"HLH",66.963205598257986,165.5071402416697,57.778100177722969,47.85448771157386,144.73741366578341,97.532391431733842,60.971317965863101,"","","","48-166",87.251668328603216]
["Cooling","Ann Cool Energy kBtu",314988,122394,216703,237374,103794,358960,41602,0,0,0,1395815]
[null,"Ann peak Cooling load kBtu/hr",123.804,52.234000000000002,85.281999999999996,90.766999999999996,46.402999999999999,161.387,17.123999999999999,0,0,0,577.00099999999998]
[null,"CLH",2544.2473587283125,2343.1864302944441,2541.0168617058703,2615.2015600383402,2236.7950348037843,2224.2188032493323,2429.455734641439,"","","","2224-2615",2419.0859287938842]
[]
["SCooper Rtl 24 7days wo setback - Baseline Design.SIM"]
[null,-9.2119999999999997,-39.600999999999999,235.7,122.042]
[null,-5.7069999999999999,-16.289000000000001,99.637,49.622999999999998]
[null,-4.5609999999999999,-24.768000000000001,159.84399999999999,84.105000000000004]
[null,-3.157,-24.593,182.006,86.091999999999999]
[null,-6.3760000000000003,-18.122,80.879000000000005,45.942]
[null,-11.087999999999999,-36.570999999999998,280.63,159.245]
[null,-0.90900000000000003,-10.766,29.248000000000001,16.914999999999999]
[]
[]
[]
[]
[null,-9.2119999999999997,-5.7069999999999999,-4.5609999999999999,-3.157,-6.3760000000000003,-11.087999999999999,-0.90900000000000003]
[null,-39.600999999999999,-16.289000000000001,-24.768000000000001,-24.593,-18.122,-36.570999999999998,-10.766]
[null,235.7,99.637,159.84399999999999,182.006,80.879000000000005,280.63,29.248000000000001]
[null,122.042,49.622999999999998,84.105000000000004,86.091999999999999,45.942,159.245,16.914999999999999]
[]
[null,"=-9212","=-5707","=-4561","=-3157","=-6376","=-11088","=-909","=0","=0","=0"]
[null,-39.600999999999999,-16.289000000000001,-24.768000000000001,-24.593,-18.122,-36.570999999999998,-10.766,0,0,0]
[null,"=235700","=99637","=159844","=182006","=80879","=280630","=29248","=0","=0","=0"]
[null,122.042,49.622999999999998,84.105000000000004,86.091999999999999,45.942,159.245,16.914999999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-9212,-5707,-4561,-3157,-6376,-11088,-909,0,0,0,-41010]
[null,"Ann peak Heating load kBtu/hr",-39.600999999999999,-16.289000000000001,-24.768000000000001,-24.593,-18.122,-36.570999999999998,-10.766,0,0,0,-170.71]
[null,"HLH",232.62038837403097,350.35913806863522,184.14890180878552,128.36986134265848,351.83754552477654,303.19105302015259,84.43247259892253,"","","","84-352",240.23197235077029]
["Cooling","Ann Cool Energy kBtu",235700,99637,159844,182006,80879,280630,29248,0,0,0,1067944]
[null,"Ann peak Cooling load kBtu/hr",122.042,49.622999999999998,84.105000000000004,86.091999999999999,45.942,159.245,16.914999999999999,0,0,0,563.96399999999994]
[null,"CLH",1931.3023385391914,2007.8794107571086,1900.5291005291003,2114.0872554941225,1760.4588394062077,1762.2531319664668,1729.1161690806978,"","","","1729-2114",1893.6386010454571]
[]
["SCooper Rtl 10-23 7day Hol1 wo setback - Baseline Design.SIM"]
[null,-12.91,-33.476999999999997,168.50399999999999,119.354]
[null,-7.3920000000000003,-13.831,79.677999999999997,49.002000000000002]
[null,-7.0289999999999999,-20.12,111.47799999999999,79.614000000000004]
[null,-5.2409999999999997,-19.911999999999999,133.80600000000001,84.513000000000005]
[null,-8.0830000000000002,-12.781000000000001,60.982999999999997,44.344000000000001]
[null,-14.994,-33.648000000000003,212.25700000000001,141.11799999999999]
[null,-0.60699999999999998,-10.516999999999999,16.343,15.231]
[]
[]
[]
[]
[null,-12.91,-7.3920000000000003,-7.0289999999999999,-5.2409999999999997,-8.0830000000000002,-14.994,-0.60699999999999998]
[null,-33.476999999999997,-13.831,-20.12,-19.911999999999999,-12.781000000000001,-33.648000000000003,-10.516999999999999]
[null,168.50399999999999,79.677999999999997,111.47799999999999,133.80600000000001,60.982999999999997,212.25700000000001,16.343]
[null,119.354,49.002000000000002,79.614000000000004,84.513000000000005,44.344000000000001,141.11799999999999,15.231]
[]
[null,"=-12910","=-7392","=-7029","=-5241","=-8083","=-14994","=-607","=0","=0","=0"]
[null,-33.476999999999997,-13.831,-20.12,-19.911999999999999,-12.781000000000001,-33.648000000000003,-10.516999999999999,0,0,0]
[null,"=168504","=79678","=111478","=133806","=60983","=212257","=16343","=0","=0","=0"]
[null,119.354,49.002000000000002,79.614000000000004,84.513000000000005,44.344000000000001,141.11799999999999,15.231,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-12910,-7392,-7029,-5241,-8083,-14994,-607,0,0,0,-56256]
[null,"Ann peak Heating load kBtu/hr",-33.476999999999997,-13.831,-20.12,-19.911999999999999,-12.781000000000001,-33.648000000000003,-10.516999999999999,0,0,0,-144.286]
[null,"HLH",385.63790064820626,534.45159424481244,349.35387673956262,263.20811570912014,632.42312808074485,445.61340941512123,57.716078729675765,"","","","58-632",389.89229724297576]
["Cooling","Ann Cool Energy kBtu",168504,79678,111478,133806,60983,212257,16343,0,0,0,783049]
[null,"Ann peak Cooling load kBtu/hr",119.354,49.002000000000002,79.614000000000004,84.513000000000005,44.344000000000001,141.11799999999999,15.231,0,0,0,533.17599999999993]
[null,"CLH",1411.8001910283695,1626.0152646830741,1400.2311151305046,1583.2593802136948,1375.2255096518131,1504.1100355730666,1073.0089948132099,"","","","1073-1626",1468.6501267874025]
[]
["SCooper Rtl 9-24 10-18 Hol2 wo setback - Baseline Design.SIM"]
[null,-6.4729999999999999,-75.453999999999994,265.80599999999998,123.01600000000001]
[null,-4.7569999999999997,-25.888999999999999,108.001,54.762]
[null,-2.9159999999999999,-49.765000000000001,181.11600000000001,84.9]
[null,-2.016,-48.942999999999998,203.15700000000001,94.86]
[null,-5.1020000000000003,-26.263999999999999,89.221000000000004,46.268000000000001]
[null,-8.1940000000000008,-76.691000000000003,310.28899999999999,161.03399999999999]
[null,-0.82599999999999996,-11.79,32.432000000000002,17.181999999999999]
[]
[]
[]
[]
[null,-6.4729999999999999,-4.7569999999999997,-2.9159999999999999,-2.016,-5.1020000000000003,-8.1940000000000008,-0.82599999999999996]
[null,-75.453999999999994,-25.888999999999999,-49.765000000000001,-48.942999999999998,-26.263999999999999,-76.691000000000003,-11.79]
[null,265.80599999999998,108.001,181.11600000000001,203.15700000000001,89.221000000000004,310.28899999999999,32.432000000000002]
[null,123.01600000000001,54.762,84.9,94.86,46.268000000000001,161.03399999999999,17.181999999999999]
[]
[null,"=-6473","=-4757","=-2916","=-2016","=-5102","=-8194","=-826","=0","=0","=0"]
[null,-75.453999999999994,-25.888999999999999,-49.765000000000001,-48.942999999999998,-26.263999999999999,-76.691000000000003,-11.79,0,0,0]
[null,"=265806","=108001","=181116","=203157","=89221","=310289","=32432","=0","=0","=0"]
[null,123.01600000000001,54.762,84.9,94.86,46.268000000000001,161.03399999999999,17.181999999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-6473,-4757,-2916,-2016,-5102,-8194,-826,0,0,0,-30284]
[null,"Ann peak Heating load kBtu/hr",-75.453999999999994,-25.888999999999999,-49.765000000000001,-48.942999999999998,-26.263999999999999,-76.691000000000003,-11.79,0,0,0,-314.79599999999999]
[null,"HLH",85.787367137593776,183.74599250646995,58.595398372350047,41.190772939950556,194.2583003350594,106.84434940214628,70.059372349448694,"","","","41-194",96.201984777443172]
["Cooling","Ann Cool Energy kBtu",265806,108001,181116,203157,89221,310289,32432,0,0,0,1190022]
[null,"Ann peak Cooling load kBtu/hr",123.01600000000001,54.762,84.9,94.86,46.268000000000001,161.03399999999999,17.181999999999999,0,0,0,582.02200000000005]
[null,"CLH",2160.7433179423815,1972.1887440195756,2133.2862190812721,2141.6508538899429,1928.3522088700613,1926.8539563073637,1887.5567454312654,"","","","1888-2161",2044.6340516337868]
[]
[]
["SCooper Sch 7-16 wo setback - Baseline Design.SIM"]
[null,-12.063000000000001,-106.05200000000001,534.50800000000004,372.06]
[null,-6.9340000000000002,-61.939,215,155]
[null,-8.4920000000000009,-88.153999999999996,313.67,233.297]
[null,-8.0459999999999994,-84.503,323.22199999999998,232.756]
[null,-7.2009999999999996,-66.552000000000007,208.053,154.41]
[null,-17.510000000000002,-138.58699999999999,528.101,387.33199999999999]
[null,-5.4180000000000001,-698.76300000000003,1423.761,1181.2719999999999]
[]
[]
[]
[]
[null,-12.063000000000001,-6.9340000000000002,-8.4920000000000009,-8.0459999999999994,-7.2009999999999996,-17.510000000000002,-5.4180000000000001]
[null,-106.05200000000001,-61.939,-88.153999999999996,-84.503,-66.552000000000007,-138.58699999999999,-698.76300000000003]
[null,534.50800000000004,215,313.67,323.22199999999998,208.053,528.101,1423.761]
[null,372.06,155,233.297,232.756,154.41,387.33199999999999,1181.2719999999999]
[]
[null,"=-12063","=-6934","=-8492","=-8046","=-7201","=-17510","=-5418","=0","=0","=0"]
[null,-106.05200000000001,-61.939,-88.153999999999996,-84.503,-66.552000000000007,-138.58699999999999,-698.76300000000003,0,0,0]
[null,"=534508","=215000","=313670","=323222","=208053","=528101","=1423761","=0","=0","=0"]
[null,372.06,155,233.297,232.756,154.41,387.33199999999999,1181.2719999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-12063,-6934,-8492,-8046,-7201,-17510,-5418,0,0,0,-65664]
[null,"Ann peak Heating load kBtu/hr",-106.05200000000001,-61.939,-88.153999999999996,-84.503,-66.552000000000007,-138.58699999999999,-698.76300000000003,0,0,0,-1244.5500000000002]
[null,"HLH",113.74608682533096,111.94885290366328,96.331420014973801,95.215554477355838,108.2011059021517,126.34662702850918,7.7537018989271038,"","","","8-126",52.761239002048924]
["Cooling","Ann Cool Energy kBtu",534508,215000,313670,323222,208053,528101,1423761,0,0,0,3546315]
[null,"Ann peak Cooling load kBtu/hr",372.06,155,233.297,232.756,154.41,387.33199999999999,1181.2719999999999,0,0,0,2716.127]
[null,"CLH",1436.6177498252971,1387.0967741935483,1344.5093593145218,1388.6731169121313,1347.4062560714981,1363.4324042423555,1205.2778699571311,"","","","1205-1437",1305.6513925895217]
[]
["SCooper Sch 6-20 wo setback - Baseline Design.SIM"]
[null,-8.8160000000000007,-101.304,675.827,392.65100000000001]
[null,-5.2850000000000001,-59.058,270.52699999999999,161.47999999999999]
[null,-6.4,-85.320999999999998,400.536,253.565]
[null,-6.032,-80.06,409.72199999999998,245.18]
[null,-5.468,-64.935000000000002,263.798,166.32499999999999]
[null,-13.129,-108.49299999999999,675.34900000000005,438.13799999999998]
[null,-3.25,-441.71800000000002,1899.114,1321.26]
[]
[]
[]
[]
[null,-8.8160000000000007,-5.2850000000000001,-6.4,-6.032,-5.468,-13.129,-3.25]
[null,-101.304,-59.058,-85.320999999999998,-80.06,-64.935000000000002,-108.49299999999999,-441.71800000000002]
[null,675.827,270.52699999999999,400.536,409.72199999999998,263.798,675.34900000000005,1899.114]
[null,392.65100000000001,161.47999999999999,253.565,245.18,166.32499999999999,438.13799999999998,1321.26]
[]
[null,"=-8816","=-5285","=-6400","=-6032","=-5468","=-13129","=-3250","=0","=0","=0"]
[null,-101.304,-59.058,-85.320999999999998,-80.06,-64.935000000000002,-108.49299999999999,-441.71800000000002,0,0,0]
[null,"=675827","=270527","=400536","=409722","=263798","=675349","=1899114","=0","=0","=0"]
[null,392.65100000000001,161.47999999999999,253.565,245.18,166.32499999999999,438.13799999999998,1321.26,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-8816,-5285,-6400,-6032,-5468,-13129,-3250,0,0,0,-48380]
[null,"Ann peak Heating load kBtu/hr",-101.304,-59.058,-85.320999999999998,-80.06,-64.935000000000002,-108.49299999999999,-441.71800000000002,0,0,0,-940.88900000000001]
[null,"HLH",87.025191502803438,89.488299637644346,75.01084141067264,75.343492380714466,84.207284207284204,121.01241554754685,7.357635414449943,"","","","7-121",51.419455429917875]
["Cooling","Ann Cool Energy kBtu",675827,270527,400536,409722,263798,675349,1899114,0,0,0,4594873]
[null,"Ann peak Cooling load kBtu/hr",392.65100000000001,161.47999999999999,253.565,245.18,166.32499999999999,438.13799999999998,1321.26,0,0,0,2978.5990000000002]
[null,"CLH",1721.1900644592781,1675.2972504334903,1579.6186382189971,1671.1069418386492,1586.0393807304977,1541.4070452688422,1437.3507106852551,"","","","1437-1721",1542.6289339384052]
[]
["SCooper Sch 7-21 7days wo setback - Baseline Design.SIM"]
[null,-8.8160000000000007,-101.304,675.827,392.65100000000001]
[null,-5.2850000000000001,-59.058,270.52699999999999,161.47999999999999]
[null,-6.4,-85.320999999999998,400.536,253.565]
[null,-6.032,-80.06,409.72199999999998,245.18]
[null,-5.468,-64.935000000000002,263.798,166.32499999999999]
[null,-13.129,-108.49299999999999,675.34900000000005,438.13799999999998]
[null,-3.25,-441.71800000000002,1899.114,1321.26]
[]
[]
[]
[]
[null,-8.8160000000000007,-5.2850000000000001,-6.4,-6.032,-5.468,-13.129,-3.25]
[null,-101.304,-59.058,-85.320999999999998,-80.06,-64.935000000000002,-108.49299999999999,-441.71800000000002]
[null,675.827,270.52699999999999,400.536,409.72199999999998,263.798,675.34900000000005,1899.114]
[null,392.65100000000001,161.47999999999999,253.565,245.18,166.32499999999999,438.13799999999998,1321.26]
[]
[null,"=-8816","=-5285","=-6400","=-6032","=-5468","=-13129","=-3250","=0","=0","=0"]
[null,-101.304,-59.058,-85.320999999999998,-80.06,-64.935000000000002,-108.49299999999999,-441.71800000000002,0,0,0]
[null,"=675827","=270527","=400536","=409722","=263798","=675349","=1899114","=0","=0","=0"]
[null,392.65100000000001,161.47999999999999,253.565,245.18,166.32499999999999,438.13799999999998,1321.26,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-8816,-5285,-6400,-6032,-5468,-13129,-3250,0,0,0,-48380]
[null,"Ann peak Heating load kBtu/hr",-101.304,-59.058,-85.320999999999998,-80.06,-64.935000000000002,-108.49299999999999,-441.71800000000002,0,0,0,-940.88900000000001]
[null,"HLH",87.025191502803438,89.488299637644346,75.01084141067264,75.343492380714466,84.207284207284204,121.01241554754685,7.357635414449943,"","","","7-121",51.419455429917875]
["Cooling","Ann Cool Energy kBtu",675827,270527,400536,409722,263798,675349,1899114,0,0,0,4594873]
[null,"Ann peak Cooling load kBtu/hr",392.65100000000001,161.47999999999999,253.565,245.18,166.32499999999999,438.13799999999998,1321.26,0,0,0,2978.5990000000002]
[null,"CLH",1721.1900644592781,1675.2972504334903,1579.6186382189971,1671.1069418386492,1586.0393807304977,1541.4070452688422,1437.3507106852551,"","","","1437-1721",1542.6289339384052]
[]
["SCooper Sch 8-22 7days 12mths wo setback - Baseline Design.SIM"]
[null,-11.260999999999999,-244.26599999999999,882.02,416.322]
[null,-6.8559999999999999,-99.411000000000001,354.38299999999998,165.744]
[null,-9.6159999999999997,-297.64699999999999,531.50900000000001,261.29199999999997]
[null,-8.1620000000000008,-148.619,540.35699999999997,253.96600000000001]
[null,-7.9050000000000002,-99.465999999999994,348.29300000000001,172.154]
[null,-17.105,-248.23500000000001,881.69399999999996,428.34399999999999]
[null,-9.5500000000000007,-161.33099999999999,2635.3690000000001,1347.193]
[]
[]
[]
[]
[null,-11.260999999999999,-6.8559999999999999,-9.6159999999999997,-8.1620000000000008,-7.9050000000000002,-17.105,-9.5500000000000007]
[null,-244.26599999999999,-99.411000000000001,-297.64699999999999,-148.619,-99.465999999999994,-248.23500000000001,-161.33099999999999]
[null,882.02,354.38299999999998,531.50900000000001,540.35699999999997,348.29300000000001,881.69399999999996,2635.3690000000001]
[null,416.322,165.744,261.29199999999997,253.96600000000001,172.154,428.34399999999999,1347.193]
[]
[null,"=-11261","=-6856","=-9616","=-8162","=-7905","=-17105","=-9550","=0","=0","=0"]
[null,-244.26599999999999,-99.411000000000001,-297.64699999999999,-148.619,-99.465999999999994,-248.23500000000001,-161.33099999999999,0,0,0]
[null,"=882020","=354383","=531509","=540357","=348293","=881694","=2635369","=0","=0","=0"]
[null,416.322,165.744,261.29199999999997,253.96600000000001,172.154,428.34399999999999,1347.193,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-11261,-6856,-9616,-8162,-7905,-17105,-9550,0,0,0,-70455]
[null,"Ann peak Heating load kBtu/hr",-244.26599999999999,-99.411000000000001,-297.64699999999999,-148.619,-99.465999999999994,-248.23500000000001,-161.33099999999999,0,0,0,-1298.9750000000001]
[null,"HLH",46.101381281062451,68.966210982688025,32.306725752317341,54.918953834973991,79.474393260008455,68.906479747013918,59.195071003093027,"","","","32-79",54.238919147789595]
["Cooling","Ann Cool Energy kBtu",882020,354383,531509,540357,348293,881694,2635369,0,0,0,6173625]
[null,"Ann peak Cooling load kBtu/hr",416.322,165.744,261.29199999999997,253.96600000000001,172.154,428.34399999999999,1347.193,0,0,0,3045.0150000000003]
[null,"CLH",2118.6005063388434,2138.134713775461,2034.1571881266937,2127.674570611814,2023.1478792244154,2058.3783127579704,1956.1926167965541,"","","","1956-2138",2027.4530667336612]
[]
["SCooper Sch 5-23 7days 12 mths wo setback - Baseline Design.SIM"]
[null,-12.241,-249.03800000000001,1018.008,422.9]
[null,-7.4340000000000002,-101.459,407.50299999999999,167.489]
[null,-10.831,-315.38299999999998,614.67399999999998,265.94099999999997]
[null,-9.3689999999999998,-324.24599999999998,623.35400000000004,257.10700000000003]
[null,-8.3290000000000006,-210.97900000000001,401.589,174.84299999999999]
[null,-17.22,-251.56299999999999,1018.841,435.87200000000001]
[null,-11.535,-261.09500000000003,3088.223,1377.942]
[]
[]
[]
[]
[null,-12.241,-7.4340000000000002,-10.831,-9.3689999999999998,-8.3290000000000006,-17.22,-11.535]
[null,-249.03800000000001,-101.459,-315.38299999999998,-324.24599999999998,-210.97900000000001,-251.56299999999999,-261.09500000000003]
[null,1018.008,407.50299999999999,614.67399999999998,623.35400000000004,401.589,1018.841,3088.223]
[null,422.9,167.489,265.94099999999997,257.10700000000003,174.84299999999999,435.87200000000001,1377.942]
[]
[null,"=-12241","=-7434","=-10831","=-9369","=-8329","=-17220","=-11535","=0","=0","=0"]
[null,-249.03800000000001,-101.459,-315.38299999999998,-324.24599999999998,-210.97900000000001,-251.56299999999999,-261.09500000000003,0,0,0]
[null,"=1018008","=407503","=614674","=623354","=401589","=1018841","=3088223","=0","=0","=0"]
[null,422.9,167.489,265.94099999999997,257.10700000000003,174.84299999999999,435.87200000000001,1377.942,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-12241,-7434,-10831,-9369,-8329,-17220,-11535,0,0,0,-76959]
[null,"Ann peak Heating load kBtu/hr",-249.03800000000001,-101.459,-315.38299999999998,-324.24599999999998,-210.97900000000001,-251.56299999999999,-261.09500000000003,0,0,0,-1713.7630000000001]
[null,"HLH",49.15314128767497,73.270976453542815,34.342371021900355,28.894728076830557,39.477862725674115,68.45203785930363,44.179321702828467,"","","","29-73",44.906442722826895]
["Cooling","Ann Cool Energy kBtu",1018008,407503,614674,623354,401589,1018841,3088223,0,0,0,7172192]
[null,"Ann peak Cooling load kBtu/hr",422.9,167.489,265.94099999999997,257.10700000000003,174.84299999999999,435.87200000000001,1377.942,0,0,0,3102.0940000000001]
[null,"CLH",2407.2073776306456,2433.0135113350725,2311.3171718539079,2424.492526457856,2296.8548926751428,2337.477516335071,2241.1850426215328,"","","","2241-2433",2312.0485710619987]
[]
["SCooper Sch 24h 7days 12 mths wo setback - Baseline Design.SIM"]
[null,-12.287000000000001,-243.56800000000001,1218.585,440.98700000000002]
[null,-7.407,-98.566999999999993,486.53,175.809]
[null,-10.263999999999999,-146.857,737.03399999999999,276.822]
[null,-9.3919999999999995,-147.33699999999999,746.11800000000005,270.16300000000001]
[null,-8.0879999999999992,-98.022000000000006,480.31599999999997,181.86600000000001]
[null,-16.722999999999999,-246.36699999999999,1221.2329999999999,455.04399999999998]
[null,-11.222,-159.63300000000001,3781.5140000000001,1454.7639999999999]
[]
[]
[]
[]
[null,-12.287000000000001,-7.407,-10.263999999999999,-9.3919999999999995,-8.0879999999999992,-16.722999999999999,-11.222]
[null,-243.56800000000001,-98.566999999999993,-146.857,-147.33699999999999,-98.022000000000006,-246.36699999999999,-159.63300000000001]
[null,1218.585,486.53,737.03399999999999,746.11800000000005,480.31599999999997,1221.2329999999999,3781.5140000000001]
[null,440.98700000000002,175.809,276.822,270.16300000000001,181.86600000000001,455.04399999999998,1454.7639999999999]
[]
[null,"=-12287","=-7407","=-10264","=-9392","=-8088","=-16723","=-11222","=0","=0","=0"]
[null,-243.56800000000001,-98.566999999999993,-146.857,-147.33699999999999,-98.022000000000006,-246.36699999999999,-159.63300000000001,0,0,0]
[null,"=1218585","=486530","=737034","=746118","=480316","=1221233","=3781514","=0","=0","=0"]
[null,440.98700000000002,175.809,276.822,270.16300000000001,181.86600000000001,455.04399999999998,1454.7639999999999,0,0,0]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","Total"]
["Heating","Ann Heat Energy kBtu",-12287,-7407,-10264,-9392,-8088,-16723,-11222,0,0,0,-75383]
[null,"Ann peak Heating load kBtu/hr",-243.56800000000001,-98.566999999999993,-146.857,-147.33699999999999,-98.022000000000006,-246.36699999999999,-159.63300000000001,0,0,0,-1140.3509999999999]
[null,"HLH",50.445871378834653,75.146854423894411,69.891118571127009,63.745019920318732,82.512089122849972,67.878409040171775,70.298747752657661,"","","","50-83",66.105085188683134]
["Cooling","Ann Cool Energy kBtu",1218585,486530,737034,746118,480316,1221233,3781514,0,0,0,8671330]
[null,"Ann peak Cooling load kBtu/hr",440.98700000000002,175.809,276.822,270.16300000000001,181.86600000000001,455.04399999999998,1454.7639999999999,0,0,0,3255.4549999999999]
[null,"CLH",2763.3127507160075,2767.3782343338512,2662.4834731343608,2761.7327317212203,2641.0434055843311,2683.769042114609,2599.4003151026559,"","","","2599-2767",2663.6307367172944]
[]
[]
["SCooper Tech Col 7-16 wo setback - Baseline Design.SIM"]
[null,-1.0249999999999999,-68.408000000000001,783.08199999999999,435.43900000000002]
[null,-0.28000000000000003,-51.314999999999998,283.44299999999998,163.416]
[null,-3.7879999999999998,-107.946,767.17399999999998,473.80900000000003]
[null,-0.31,-72.424999999999997,275.41300000000001,159.447]
[null,-0.111,-53.834000000000003,950.072,557.476]
[null,-1.4590000000000001,-195.339,1694.2329999999999,869.05200000000002]
[null,-0.82199999999999995,-132.51900000000001,619.67999999999995,321.59199999999998]
[null,-3.887,-285.32799999999997,1662.6569999999999,934.48]
[null,-0.66100000000000003,-139.90199999999999,605.58299999999997,314.928]
[null,-1.0249999999999999,-241.06200000000001,2044.48,1116.75]
[null,-8.5289999999999999,-131.58099999999999,853.81899999999996,456.42]
[null,-2.0430000000000001,-74.828000000000003,310.19200000000001,166.125]
[null,-15.013999999999999,-174.59700000000001,842.65800000000002,486.29399999999998]
[null,-1.8580000000000001,-69.712999999999994,302.94900000000001,165.22200000000001]
[null,-2.7280000000000002,-267.33999999999997,1028.123,607.86400000000003]
[]
[null,-1.0249999999999999,-0.28000000000000003,-3.7879999999999998,-0.31,-0.111,-1.4590000000000001,-0.82199999999999995,-3.887,-0.66100000000000003,-1.0249999999999999,-8.5289999999999999,-2.0430000000000001,-15.013999999999999,-1.8580000000000001,-2.7280000000000002]
[null,-68.408000000000001,-51.314999999999998,-107.946,-72.424999999999997,-53.834000000000003,-195.339,-132.51900000000001,-285.32799999999997,-139.90199999999999,-241.06200000000001,-131.58099999999999,-74.828000000000003,-174.59700000000001,-69.712999999999994,-267.33999999999997]
[null,783.08199999999999,283.44299999999998,767.17399999999998,275.41300000000001,950.072,1694.2329999999999,619.67999999999995,1662.6569999999999,605.58299999999997,2044.48,853.81899999999996,310.19200000000001,842.65800000000002,302.94900000000001,1028.123]
[null,435.43900000000002,163.416,473.80900000000003,159.447,557.476,869.05200000000002,321.59199999999998,934.48,314.928,1116.75,456.42,166.125,486.29399999999998,165.22200000000001,607.86400000000003]
[]
[null,"=-1025","=-280","=-3788","=-310","=-111","=-1459","=-822","=-3887","=-661","=-1025","=-8529","=-2043","=-15014","=-1858","=-2728"]
[null,-68.408000000000001,-51.314999999999998,-107.946,-72.424999999999997,-53.834000000000003,-195.339,-132.51900000000001,-285.32799999999997,-139.90199999999999,-241.06200000000001,-131.58099999999999,-74.828000000000003,-174.59700000000001,-69.712999999999994,-267.33999999999997]
[null,"=783082","=283443","=767174","=275413","=950072","=1694233","=619680","=1662657","=605583","=2044480","=853819","=310192","=842658","=302949","=1028123"]
[null,435.43900000000002,163.416,473.80900000000003,159.447,557.476,869.05200000000002,321.59199999999998,934.48,314.928,1116.75,456.42,166.125,486.29399999999998,165.22200000000001,607.86400000000003]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann Heat Energy kBtu",-1025,-280,-3788,-310,-111,-1459,-822,-3887,-661,-1025,-8529,-2043,-15014,-1858,-2728,-13368]
[null,"Ann peak Heating load kBtu/hr",-68.408000000000001,-51.314999999999998,-107.946,-72.424999999999997,-53.834000000000003,-195.339,-132.51900000000001,-285.32799999999997,-139.90199999999999,-241.06200000000001,-131.58099999999999,-74.828000000000003,-174.59700000000001,-69.712999999999994,-267.33999999999997,-1348.078]
[null,"HLH",14.983627645889369,5.4564942024749099,35.091619884016083,4.2802899551259923,2.0618939703533083,7.4690665970441135,6.2028841147307174,13.622918185386643,4.7247358865491567,4.2520181530062802,64.819388817534445,27.30261399476132,85.992313728185479,26.652130879462945,10.204234308371364,"2-35",9.9163401524244144]
["Cooling","Ann Cool Energy kBtu",783082,283443,767174,275413,950072,1694233,619680,1662657,605583,2044480,853819,310192,842658,302949,1028123,9685817]
[null,"Ann peak Cooling load kBtu/hr",435.43900000000002,163.416,473.80900000000003,159.447,557.476,869.05200000000002,321.59199999999998,934.48,314.928,1116.75,456.42,166.125,486.29399999999998,165.22200000000001,607.86400000000003,5346.3890000000001]
[null,"CLH",1798.3735953830501,1734.4874430900279,1619.1629960595935,1727.3012348930993,1704.2383887378112,1949.5185558516637,1926.9136048160403,1779.2323003167537,1922.9252400548696,1830.7409894783971,1870.6870864554576,1867.2204665161776,1732.8159508445508,1833.5875367687111,1691.370109103352,"1619-1950",1811.6558671656701]
[]
["SCooper Tech Col 6-20 wo setback - Baseline Design.SIM"]
[null,-0.48099999999999998,-59.741,1001.697,446.64400000000001]
[null,-0.216,-39.491,355.21699999999998,162.34200000000001]
[null,-2.5859999999999999,-74.998000000000005,985.72,474.435]
[null,-0.20899999999999999,-39.71,350.98899999999998,167.24]
[null,-0.10100000000000001,-52.646000000000001,1288.3579999999999,571.56299999999999]
[null,-0.93899999999999995,-151.221,2153.3789999999999,904.36800000000005]
[null,-0.63500000000000001,-90.977000000000004,769.70899999999995,325.73200000000003]
[null,-2.4809999999999999,-175.99700000000001,2125.444,961.48199999999997]
[null,-0.51300000000000001,-85.49,761.72,338.49299999999999]
[null,-0.76300000000000001,-172.31800000000001,2794.3009999999999,1161.9290000000001]
[null,-6.6459999999999999,-103.876,1081.8820000000001,477.51600000000002]
[null,-1.522,-51.619,385.64699999999999,171.44900000000001]
[null,-11.737,-126.721,1072.7650000000001,504.255]
[null,-1.196,-54.536000000000001,381.577,177.304]
[null,-2.012,-193.447,1404.9749999999999,647.94899999999996]
[]
[null,-0.48099999999999998,-0.216,-2.5859999999999999,-0.20899999999999999,-0.10100000000000001,-0.93899999999999995,-0.63500000000000001,-2.4809999999999999,-0.51300000000000001,-0.76300000000000001,-6.6459999999999999,-1.522,-11.737,-1.196,-2.012]
[null,-59.741,-39.491,-74.998000000000005,-39.71,-52.646000000000001,-151.221,-90.977000000000004,-175.99700000000001,-85.49,-172.31800000000001,-103.876,-51.619,-126.721,-54.536000000000001,-193.447]
[null,1001.697,355.21699999999998,985.72,350.98899999999998,1288.3579999999999,2153.3789999999999,769.70899999999995,2125.444,761.72,2794.3009999999999,1081.8820000000001,385.64699999999999,1072.7650000000001,381.577,1404.9749999999999]
[null,446.64400000000001,162.34200000000001,474.435,167.24,571.56299999999999,904.36800000000005,325.73200000000003,961.48199999999997,338.49299999999999,1161.9290000000001,477.51600000000002,171.44900000000001,504.255,177.304,647.94899999999996]
[]
[null,"=-481","=-216","=-2586","=-209","=-101","=-939","=-635","=-2481","=-513","=-763","=-6646","=-1522","=-11737","=-1196","=-2012"]
[null,-59.741,-39.491,-74.998000000000005,-39.71,-52.646000000000001,-151.221,-90.977000000000004,-175.99700000000001,-85.49,-172.31800000000001,-103.876,-51.619,-126.721,-54.536000000000001,-193.447]
[null,"=1001697","=355217","=985720","=350989","=1288358","=2153379","=769709","=2125444","=761720","=2794301","=1081882","=385647","=1072765","=381577","=1404975"]
[null,446.64400000000001,162.34200000000001,474.435,167.24,571.56299999999999,904.36800000000005,325.73200000000003,961.48199999999997,338.49299999999999,1161.9290000000001,477.51600000000002,171.44900000000001,504.255,177.304,647.94899999999996]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann Heat Energy kBtu",-481,-216,-2586,-209,-101,-939,-635,-2481,-513,-763,-6646,-1522,-11737,-1196,-2012,-8924]
[null,"Ann peak Heating load kBtu/hr",-59.741,-39.491,-74.998000000000005,-39.71,-52.646000000000001,-151.221,-90.977000000000004,-175.99700000000001,-85.49,-172.31800000000001,-103.876,-51.619,-126.721,-54.536000000000001,-193.447,-942.58899999999994]
[null,"HLH",8.0514219715103525,5.4696006685067484,34.480919491186427,5.2631578947368416,1.9184743380313793,6.2094550360069034,6.9797860997834613,14.096831195986294,6.0007018364721025,4.4278601190821618,63.980130155185023,29.485267052829386,92.620796868711579,21.930467947777615,10.400781609433075,"2-34",9.4675409961287489]
["Cooling","Ann Cool Energy kBtu",1001697,355217,985720,350989,1288358,2153379,769709,2125444,761720,2794301,1081882,385647,1072765,381577,1404975,12586534]
[null,"Ann peak Cooling load kBtu/hr",446.64400000000001,162.34200000000001,474.435,167.24,571.56299999999999,904.36800000000005,325.73200000000003,961.48199999999997,338.49299999999999,1161.9290000000001,477.51600000000002,171.44900000000001,504.255,177.304,647.94899999999996,5514.2280000000001]
[null,"CLH",2242.7190335031928,2188.0782545490383,2077.6713353778705,2098.7144223869886,2254.096223863336,2381.0871238256991,2363.0131519162992,2210.591565936752,2250.327185495712,2404.8810211295181,2265.6455490496651,2249.3394537150989,2127.4256080752793,2152.1059874565717,2168.3419528388808,"2078-2405",2282.55596250282]
[]
["SCooper Tech Col 9-21 7days wo setback - Baseline Design.SIM"]
[null,-1.988,-81.382000000000005,916.98299999999995,438.88499999999999]
[null,-1.794,-31.702999999999999,326.678,159.72200000000001]
[null,-5.7519999999999998,-250.089,909.41499999999996,466.44299999999998]
[null,-2.0139999999999998,-95.88,323.017,165.88900000000001]
[null,-0.68400000000000005,-70.272999999999996,1202.05,553.42100000000005]
[null,-3.4159999999999999,-155.34,1974.029,882.18299999999999]
[null,-3.0840000000000001,-70.858000000000004,707.71500000000003,320.34500000000003]
[null,-9.859,-318.81799999999998,1957.1969999999999,943.90599999999995]
[null,-3.9590000000000001,-151.97399999999999,699.57600000000002,334.36700000000002]
[null,-2.6560000000000001,-165.77099999999999,2582.395,1128.7539999999999]
[null,-8.7370000000000001,-177.679,994.57899999999995,467.20699999999999]
[null,-3.5510000000000002,-78.132000000000005,356.70800000000003,169.02699999999999]
[null,-16.306000000000001,-265.85700000000003,990.38900000000001,496.11900000000003]
[null,-4.4000000000000004,-101.247,352.596,175.27600000000001]
[null,-13.433999999999999,-217.73599999999999,1309.519,643.81799999999998]
[]
[null,-1.988,-1.794,-5.7519999999999998,-2.0139999999999998,-0.68400000000000005,-3.4159999999999999,-3.0840000000000001,-9.859,-3.9590000000000001,-2.6560000000000001,-8.7370000000000001,-3.5510000000000002,-16.306000000000001,-4.4000000000000004,-13.433999999999999]
[null,-81.382000000000005,-31.702999999999999,-250.089,-95.88,-70.272999999999996,-155.34,-70.858000000000004,-318.81799999999998,-151.97399999999999,-165.77099999999999,-177.679,-78.132000000000005,-265.85700000000003,-101.247,-217.73599999999999]
[null,916.98299999999995,326.678,909.41499999999996,323.017,1202.05,1974.029,707.71500000000003,1957.1969999999999,699.57600000000002,2582.395,994.57899999999995,356.70800000000003,990.38900000000001,352.596,1309.519]
[null,438.88499999999999,159.72200000000001,466.44299999999998,165.88900000000001,553.42100000000005,882.18299999999999,320.34500000000003,943.90599999999995,334.36700000000002,1128.7539999999999,467.20699999999999,169.02699999999999,496.11900000000003,175.27600000000001,643.81799999999998]
[]
[null,"=-1988","=-1794","=-5752","=-2014","=-684","=-3416","=-3084","=-9859","=-3959","=-2656","=-8737","=-3551","=-16306","=-4400","=-13434"]
[null,-81.382000000000005,-31.702999999999999,-250.089,-95.88,-70.272999999999996,-155.34,-70.858000000000004,-318.81799999999998,-151.97399999999999,-165.77099999999999,-177.679,-78.132000000000005,-265.85700000000003,-101.247,-217.73599999999999]
[null,"=916983","=326678","=909415","=323017","=1202050","=1974029","=707715","=1957197","=699576","=2582395","=994579","=356708","=990389","=352596","=1309519"]
[null,438.88499999999999,159.72200000000001,466.44299999999998,165.88900000000001,553.42100000000005,882.18299999999999,320.34500000000003,943.90599999999995,334.36700000000002,1128.7539999999999,467.20699999999999,169.02699999999999,496.11900000000003,175.27600000000001,643.81799999999998]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann Heat Energy kBtu",-1988,-1794,-5752,-2014,-684,-3416,-3084,-9859,-3959,-2656,-8737,-3551,-16306,-4400,-13434,-35206]
[null,"Ann peak Heating load kBtu/hr",-81.382000000000005,-31.702999999999999,-250.089,-95.88,-70.272999999999996,-155.34,-70.858000000000004,-318.81799999999998,-151.97399999999999,-165.77099999999999,-177.679,-78.132000000000005,-265.85700000000003,-101.247,-217.73599999999999,-1392.088]
[null,"HLH",24.428006193015651,56.587704633630885,22.999812066904184,21.005423445974134,9.7334680460489817,21.99047251190936,43.523667052414687,30.923599043968661,26.05050863963573,16.022102780341555,49.172946718520478,45.448727793989654,61.333724521077116,43.458077770205534,61.698570746224789,"10-57",25.290067869272633]
["Cooling","Ann Cool Energy kBtu",916983,326678,909415,323017,1202050,1974029,707715,1957197,699576,2582395,994579,356708,990389,352596,1309519,11599055]
[null,"Ann peak Cooling load kBtu/hr",438.88499999999999,159.72200000000001,466.44299999999998,165.88900000000001,553.42100000000005,882.18299999999999,320.34500000000003,943.90599999999995,334.36700000000002,1128.7539999999999,467.20699999999999,169.02699999999999,496.11900000000003,175.27600000000001,643.81799999999998,5393.915]
[null,"CLH",2089.3468676304728,2045.2911934486169,1949.6808827659543,1947.1875772353801,2172.0353943923342,2237.66384072239,2209.2275515459892,2073.5083790123172,2092.2399638720326,2287.8279944079936,2128.7758959090938,2110.3610665751626,1996.2730715816165,2011.6616079782741,2033.9894193700704,"1947-2288",2150.3963262305765]
[]
["SCooper Tech Col 8-22 7days wo setback - Baseline Design.SIM"]
[null,-2.7509999999999999,-274.23399999999998,1009.997,443.86]
[null,-2.3330000000000002,-99.003,357.29300000000001,163.41]
[null,-6.3719999999999999,-278.20699999999999,1001.727,472.44]
[null,-2.5630000000000002,-101.039,353.52,168.27500000000001]
[null,-0.60399999999999998,-65.832999999999998,1348.923,562.33000000000004]
[null,-5.3639999999999999,-310.10599999999999,2171.4690000000001,895.15]
[null,-4.1829999999999998,-180.52,770.9,323.45999999999998]
[null,-11.776999999999999,-428.245,2153.2919999999999,959.98099999999999]
[null,-4.8760000000000003,-175.751,763.08699999999999,339.45400000000001]
[null,-2.266,-162.667,2905.1889999999999,1148.692]
[null,-9.3930000000000007,-320.04700000000003,1092.2550000000001,473.49799999999999]
[null,-4.2009999999999996,-113.637,388.541,170.5]
[null,-16.391999999999999,-321.44900000000001,1086.5809999999999,503.81099999999998]
[null,-4.9930000000000003,-115.48,384.49200000000002,177.78700000000001]
[null,-14.121,-249.25399999999999,1473.203,653.65099999999995]
[]
[null,-2.7509999999999999,-2.3330000000000002,-6.3719999999999999,-2.5630000000000002,-0.60399999999999998,-5.3639999999999999,-4.1829999999999998,-11.776999999999999,-4.8760000000000003,-2.266,-9.3930000000000007,-4.2009999999999996,-16.391999999999999,-4.9930000000000003,-14.121]
[null,-274.23399999999998,-99.003,-278.20699999999999,-101.039,-65.832999999999998,-310.10599999999999,-180.52,-428.245,-175.751,-162.667,-320.04700000000003,-113.637,-321.44900000000001,-115.48,-249.25399999999999]
[null,1009.997,357.29300000000001,1001.727,353.52,1348.923,2171.4690000000001,770.9,2153.2919999999999,763.08699999999999,2905.1889999999999,1092.2550000000001,388.541,1086.5809999999999,384.49200000000002,1473.203]
[null,443.86,163.41,472.44,168.27500000000001,562.33000000000004,895.15,323.45999999999998,959.98099999999999,339.45400000000001,1148.692,473.49799999999999,170.5,503.81099999999998,177.78700000000001,653.65099999999995]
[]
[null,"=-2751","=-2333","=-6372","=-2563","=-604","=-5364","=-4183","=-11777","=-4876","=-2266","=-9393","=-4201","=-16392","=-4993","=-14121"]
[null,-274.23399999999998,-99.003,-278.20699999999999,-101.039,-65.832999999999998,-310.10599999999999,-180.52,-428.245,-175.751,-162.667,-320.04700000000003,-113.637,-321.44900000000001,-115.48,-249.25399999999999]
[null,"=1009997","=357293","=1001727","=353520","=1348923","=2171469","=770900","=2153292","=763087","=2905189","=1092255","=388541","=1086581","=384492","=1473203"]
[null,443.86,163.41,472.44,168.27500000000001,562.33000000000004,895.15,323.45999999999998,959.98099999999999,339.45400000000001,1148.692,473.49799999999999,170.5,503.81099999999998,177.78700000000001,653.65099999999995]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann Heat Energy kBtu",-2751,-2333,-6372,-2563,-604,-5364,-4183,-11777,-4876,-2266,-9393,-4201,-16392,-4993,-14121,-43089]
[null,"Ann peak Heating load kBtu/hr",-274.23399999999998,-99.003,-278.20699999999999,-101.039,-65.832999999999998,-310.10599999999999,-180.52,-428.245,-175.751,-162.667,-320.04700000000003,-113.637,-321.44900000000001,-115.48,-249.25399999999999,-2075.605]
[null,"HLH",10.031578870599562,23.564942476490611,22.903809034280229,25.366442660754757,9.1747299986329054,17.297311241962426,23.171947706625303,27.500612966876439,27.743796621356349,13.930299323157124,29.348814392886041,36.968592975879332,50.994092375462358,43.236924142708695,56.653052709284509,"9-28",20.759730295504202]
["Cooling","Ann Cool Energy kBtu",1009997,357293,1001727,353520,1348923,2171469,770900,2153292,763087,2905189,1092255,388541,1086581,384492,1473203,12835397]
[null,"Ann peak Cooling load kBtu/hr",443.86,163.41,472.44,168.27500000000001,562.33000000000004,895.15,323.45999999999998,959.98099999999999,339.45400000000001,1148.692,473.49799999999999,170.5,503.81099999999998,177.78700000000001,653.65099999999995,5477.0519999999997]
[null,"CLH",2275.4855134501868,2186.4818554556027,2120.3263906527814,2100.8468281087503,2398.810307115039,2425.8157850639559,2383.2931428924753,2243.0568938343572,2247.983526486652,2529.1279124430221,2306.7784869207471,2278.8328445747802,2156.7234538348707,2162.6553122556766,2253.8066950100283,"2101-2529",2343.4864229881332]
[]
["SCooper Tech Col 5-23 7days wo setback - Baseline Design.SIM"]
[null,-4.3899999999999997,-167.44800000000001,1174.8579999999999,452.48399999999998]
[null,-3.5209999999999999,-78.391000000000005,410.80399999999997,164.36699999999999]
[null,-8.4139999999999997,-279.185,1164.4179999999999,482.95100000000002]
[null,-3.5739999999999998,-81.679000000000002,407.084,171.43899999999999]
[null,-0.28699999999999998,-50.304000000000002,1619.8240000000001,576.91]
[null,-8.8040000000000003,-194.702,2521.6979999999999,916.91099999999994]
[null,-6.452,-108.29900000000001,883.72299999999996,329.34199999999998]
[null,-16.065999999999999,-271.19,2499.6930000000002,981.899]
[null,-6.4320000000000004,-108.482,875.73,346.40499999999997]
[null,-0.90900000000000003,-113.874,3501.76,1173.9359999999999]
[null,-10.922000000000001,-225.79499999999999,1266.7660000000001,483.887]
[null,-5.9539999999999997,-106.474,445.31599999999997,173.20599999999999]
[null,-17.946000000000002,-303.95299999999997,1259.354,514.18600000000004]
[null,-6.3330000000000002,-101.081,441.26299999999998,181.15700000000001]
[null,-14.881,-143.608,1774.528,665.74599999999998]
[]
[null,-4.3899999999999997,-3.5209999999999999,-8.4139999999999997,-3.5739999999999998,-0.28699999999999998,-8.8040000000000003,-6.452,-16.065999999999999,-6.4320000000000004,-0.90900000000000003,-10.922000000000001,-5.9539999999999997,-17.946000000000002,-6.3330000000000002,-14.881]
[null,-167.44800000000001,-78.391000000000005,-279.185,-81.679000000000002,-50.304000000000002,-194.702,-108.29900000000001,-271.19,-108.482,-113.874,-225.79499999999999,-106.474,-303.95299999999997,-101.081,-143.608]
[null,1174.8579999999999,410.80399999999997,1164.4179999999999,407.084,1619.8240000000001,2521.6979999999999,883.72299999999996,2499.6930000000002,875.73,3501.76,1266.7660000000001,445.31599999999997,1259.354,441.26299999999998,1774.528]
[null,452.48399999999998,164.36699999999999,482.95100000000002,171.43899999999999,576.91,916.91099999999994,329.34199999999998,981.899,346.40499999999997,1173.9359999999999,483.887,173.20599999999999,514.18600000000004,181.15700000000001,665.74599999999998]
[]
[null,"=-4390","=-3521","=-8414","=-3574","=-287","=-8804","=-6452","=-16066","=-6432","=-909","=-10922","=-5954","=-17946","=-6333","=-14881"]
[null,-167.44800000000001,-78.391000000000005,-279.185,-81.679000000000002,-50.304000000000002,-194.702,-108.29900000000001,-271.19,-108.482,-113.874,-225.79499999999999,-106.474,-303.95299999999997,-101.081,-143.608]
[null,"=1174858","=410804","=1164418","=407084","=1619824","=2521698","=883723","=2499693","=875730","=3501760","=1266766","=445316","=1259354","=441263","=1774528"]
[null,452.48399999999998,164.36699999999999,482.95100000000002,171.43899999999999,576.91,916.91099999999994,329.34199999999998,981.899,346.40499999999997,1173.9359999999999,483.887,173.20599999999999,514.18600000000004,181.15700000000001,665.74599999999998]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann Heat Energy kBtu",-4390,-3521,-8414,-3574,-287,-8804,-6452,-16066,-6432,-909,-10922,-5954,-17946,-6333,-14881,-58849]
[null,"Ann peak Heating load kBtu/hr",-167.44800000000001,-78.391000000000005,-279.185,-81.679000000000002,-50.304000000000002,-194.702,-108.29900000000001,-271.19,-108.482,-113.874,-225.79499999999999,-106.474,-303.95299999999997,-101.081,-143.608,-1453.5539999999999]
[null,"HLH",26.217094262099277,44.915870444311203,30.137722298834106,43.756657157898601,5.7053117048346049,45.217820053209522,59.575804024044537,59.24259744090859,59.290942276137976,7.9825069814004959,48.371310259306007,55.919755057572736,59.042022944336793,62.652724052987203,103.62236087126065,"6-60",40.486283963306491]
["Cooling","Ann Cool Energy kBtu",1174858,410804,1164418,407084,1619824,2521698,883723,2499693,875730,3501760,1266766,445316,1259354,441263,1774528,15059592]
[null,"Ann peak Cooling load kBtu/hr",452.48399999999998,164.36699999999999,482.95100000000002,171.43899999999999,576.91,916.91099999999994,329.34199999999998,981.899,346.40499999999997,1173.9359999999999,483.887,173.20599999999999,514.18600000000004,181.15700000000001,665.74599999999998,5596.6440000000002]
[null,"CLH",2596.4630793575025,2499.3094720959807,2411.0479116929046,2374.5122171734552,2807.758575861053,2750.2102166949685,2683.2988200715367,2545.7740561911155,2528.0524241855633,2982.9224080358726,2617.8963270350309,2571.0194796946989,2449.218765193918,2435.8043023454793,2665.4730182381868,"2375-2983",2690.8254303829221]
[]
["SCooper Tech Col 24h 7days wo setback - Baseline Design.SIM"]
[null,-4.67,-80.366,1469.723,477.19900000000001]
[null,-3.859,-51.281999999999996,508.77499999999998,172.92500000000001]
[null,-8.5500000000000007,-137.357,1456.72,508.964]
[null,-3.8479999999999999,-53.838000000000001,505.245,179.989]
[null,-4.0000000000000001E-3,-0.76800000000000002,2082.3069999999998,619.11099999999999]
[null,-9.7349999999999994,-134.53700000000001,3135.203,969.75300000000004]
[null,-7.3650000000000002,-78.658000000000001,1089.6420000000001,347.27699999999999]
[null,-17.922000000000001,-180.49199999999999,3113.3380000000002,1031.2059999999999]
[null,-6.93,-83.206000000000003,1081.5809999999999,363.35599999999999]
[null,0,0,4527.259,1252.9169999999999]
[null,-11.27,-171.27,1578.259,509.976]
[null,-6.4340000000000002,-73.442999999999998,548.72500000000002,182.03399999999999]
[null,-18.041,-220.57900000000001,1568.941,538.46600000000001]
[null,-6.5979999999999999,-74.290999999999997,544.80700000000002,189.40199999999999]
[null,-13.169,-77.272000000000006,2292.4870000000001,704.50699999999995]
[]
[null,-4.67,-3.859,-8.5500000000000007,-3.8479999999999999,-4.0000000000000001E-3,-9.7349999999999994,-7.3650000000000002,-17.922000000000001,-6.93,0,-11.27,-6.4340000000000002,-18.041,-6.5979999999999999,-13.169]
[null,-80.366,-51.281999999999996,-137.357,-53.838000000000001,-0.76800000000000002,-134.53700000000001,-78.658000000000001,-180.49199999999999,-83.206000000000003,0,-171.27,-73.442999999999998,-220.57900000000001,-74.290999999999997,-77.272000000000006]
[null,1469.723,508.77499999999998,1456.72,505.245,2082.3069999999998,3135.203,1089.6420000000001,3113.3380000000002,1081.5809999999999,4527.259,1578.259,548.72500000000002,1568.941,544.80700000000002,2292.4870000000001]
[null,477.19900000000001,172.92500000000001,508.964,179.989,619.11099999999999,969.75300000000004,347.27699999999999,1031.2059999999999,363.35599999999999,1252.9169999999999,509.976,182.03399999999999,538.46600000000001,189.40199999999999,704.50699999999995]
[]
[null,"=-4670","=-3859","=-8550","=-3848","=-4","=-9735","=-7365","=-17922","=-6930","=0","=-11270","=-6434","=-18041","=-6598","=-13169"]
[null,-80.366,-51.281999999999996,-137.357,-53.838000000000001,-0.76800000000000002,-134.53700000000001,-78.658000000000001,-180.49199999999999,-83.206000000000003,0,-171.27,-73.442999999999998,-220.57900000000001,-74.290999999999997,-77.272000000000006]
[null,"=1469723","=508775","=1456720","=505245","=2082307","=3135203","=1089642","=3113338","=1081581","=4527259","=1578259","=548725","=1568941","=544807","=2292487"]
[null,477.19900000000001,172.92500000000001,508.964,179.989,619.11099999999999,969.75300000000004,347.27699999999999,1031.2059999999999,363.35599999999999,1252.9169999999999,509.976,182.03399999999999,538.46600000000001,189.40199999999999,704.50699999999995]
[]
[null,null,"SYS1","SYS2","SYS3","SYS4","SYS5","SYS6","SYS7","SYS8","SYS9","SYS10","SYS11","SYS12","SYS13","SYS14","SYS15","Total"]
["Heating","Ann Heat Energy kBtu",-4670,-3859,-8550,-3848,-4,-9735,-7365,-17922,-6930,0,-11270,-6434,-18041,-6598,-13169,-62883]
[null,"Ann peak Heating load kBtu/hr",-80.366,-51.281999999999996,-137.357,-53.838000000000001,-0.76800000000000002,-134.53700000000001,-78.658000000000001,-180.49199999999999,-83.206000000000003,0,-171.27,-73.442999999999998,-220.57900000000001,-74.290999999999997,-77.272000000000006,-800.50400000000002]
[null,"HLH",58.109150635841026,75.250575250575253,62.246554598600724,71.473680300159742,5.208333333333333,72.359276630220677,93.633196877622112,99.295259623695244,83.287262937768901,"",65.802534010626488,87.605353811799631,81.789290911646162,88.812911388997321,170.42395693135933,"5-99",78.554260815686121]
["Cooling","Ann Cool Energy kBtu",1469723,508775,1456720,505245,2082307,3135203,1089642,3113338,1081581,4527259,1578259,548725,1568941,544807,2292487,18969793]
[null,"Ann peak Cooling load kBtu/hr",477.19900000000001,172.92500000000001,508.964,179.989,619.11099999999999,969.75300000000004,347.27699999999999,1031.2059999999999,363.35599999999999,1252.9169999999999,509.976,182.03399999999999,538.46600000000001,189.40199999999999,704.50699999999995,5922.6970000000001]
[null,"CLH",3079.8953895544623,2942.1714616163076,2862.1277732806248,2807.0882109462245,3363.3823337010649,3232.9912874721708,3137.6739605559828,3019.1232401673383,2976.6427415537378,3613.3750280345789,3094.7711264843838,3014.4093960468927,2913.7234291487298,2876.4585379246259,3254.0301231925305,"2807-3613",3202.8977676892805]

{"sheet":"SC Test Runs","index":2,"n_rows":117,"n_cols":16,"rows_kept":117,"cut":false,"hidden":true,"merged":[[0,13,0,15],[1,0,7,0],[1,4,43,4],[1,13,1,15],[8,0,16,0],[17,0,22,0],[23,0,31,0],[32,0,37,0],[38,0,43,0],[46,0,52,0],[46,4,88,4],[53,0,61,0],[62,0,67,0],[68,0,76,0],[77,0,82,0],[83,0,88,0],[105,1,105,6],[105,7,105,12],[92,1,92,6],[92,7,92,12],[45,13,45,15],[48,13,48,15]]}
["Facility Type","Schedule","Hours/year","W/O Setback","W/ Setback","EFLCH","EFLHH","Year-round","Close Summer","Extended Summer Hours","Summer Only","File Name",null,"HVAC Calculator Input"]
["Office","8a-5p, M-F",{"$f":"(17-8)*5*52","v":2340},"Clg 72F/Htg 70F","OCC: Clg 72F/Htg 70F, \nUNOCC: Clg 80F/Htg 62F",1065,34,"X",null,null,null,"SCooper Office 8-17 w setback - Baseline Design.SIM",null,"Typical Operating Schedule"]
[null,"7a-7p, M-F",{"$f":"(19-7)*5*52","v":3120},"Clg 72F/Htg 70F",null,1438,29,"X",null,null,null,"SCooper Office 7-19 w setback - Baseline Design.SIM",null,null,"Open","Close"]
[null,"7a - 10p, M-F",{"$f":"(22-7)*5*52","v":3900},"Clg 72F/Htg 70F",null,1255,31,"X",null,null,null,"SCooper Office 7-22 w setback - Baseline Design.SIM",null,"Mon"]
[null,"6a-7p, 7 days",{"$f":"(19-6)*365","v":4745},"Clg 72F/Htg 70F",null,1651,93,"X",null,null,null,"SCooper Office 6-19 7days w setback - Baseline Design.SIM",null,"Tue"]
[null,"6a-9p, 7 days",{"$f":"(21-6)*365","v":5475},"Clg 72F/Htg 70F",null,1501,78,"X",null,null,null,"SCooper Office 6-21 7days w setback - Baseline Design.SIM",null,"Wed"]
[null,"5a - 11p, 7 days",{"$f":"(23-5)*365","v":6570},"Clg 72F/Htg 70F",null,1851,123,"X",null,null,null,"SCooper Office 5-23 7days w setback - Baseline Design.SIM",null,"Thur"]
[null,"24/7",8760,"Clg 72F/Htg 70F",null,2117,199,"X",null,null,null,"SCooper Office 24 7days w setback - Baseline Design.SIM",null,"Fri"]
["Restaurant","9a-6p, M-F",{"$f":"(18-9)*5*52","v":2340},"Clg 72F/Htg 70F",null,1082,125,"X",null,null,null,"SCooper Rest 9-18 w setback - Baseline Design.SIM",null,"Sat"]
[null,"8a-8p, M-F",{"$f":"(20-8)*5*52","v":3120},"Clg 72F/Htg 70F",null,1263,111,"X",null,null,null,"SCooper Rest 8-20 w setback - Baseline Design.SIM",null,"Sun"]
[null,"7a - 10p, M-F",{"$f":"(22-7)*5*52","v":3900},"Clg 72F/Htg 70F",null,1431,100,"X",null,null,null,"SCooper Rest 7-22 w setback - Baseline Design.SIM",null,null,"Extended Summer Hours"]
[null,"9a-10p, 7 days",{"$f":"(22-9)*365","v":4745},"Clg 72F/Htg 70F",null,1789,42,"X",null,null,null,"SCooper Rest 9-22 7days w setback - Baseline Design.SIM",null,null,"Summer Only"]
[null,"8a-10p, 7days",{"$f":"(22-8)*365","v":5110},"Clg 72F/Htg 70F",null,1855,47,"X",null,null,null,"SCooper Rest 8-22 7days w setback - Baseline Design.SIM",null,null,"Close Summer"]
[null,"5a - 11p, 7 days",{"$f":"(23-5)*365","v":6570},"Clg 72F/Htg 70F",null,2129,51,"X",null,null,null,"SCooper Rest 5-23 7days w setback - Baseline Design.SIM"]
[null,"24/7",8760,"Clg 72F/Htg 70F",null,2788,12,"X",null,null,null,"SCooper Rest 24 7days w setback - Baseline Design.SIM"]
[null,"Mar - Oct, 10a-11p,7 days",{"$f":"(13*7*8*4)","v":2912},null,null,1562,228,null,null,null,"X","SCooper Rest 10-23 7day Hol1 w setback - Baseline Design.SIM"]
[null,"Apr - Sep, 8a-11p,7day\nOct -Mar, 12a-8p,7days",{"$f":"(23-8)*7*28+(20-12)*7*6*4","v":4284},null,null,1194,71,null,null,"X",null,"SCooper Rest 8-23 12-20 Hol2 w setback - Baseline Design.SIM"]
["Hotel","9a-6p, M-F",{"$f":"(18-9)*5*52","v":2340},"Clg 72F/Htg 70F",null,1140,150,"X",null,null,null,"SCooper Htl 9-18 w setback - Baseline Design.SIM"]
[null,"8a-9p, M-F",{"$f":"(21-8)*5*52","v":3380},"Clg 72F/Htg 70F",null,1334,192,"X",null,null,null,"SCooper Htl 8-21 w setback - Baseline Design.SIM"]
[null,"9a-10p, 7 days",{"$f":"(22-9)*365","v":4745},"Clg 72F/Htg 70F",null,1622,207,"X",null,null,null,"SCooper Htl 9-22 7days w setback - Baseline Design.SIM"]
[null,"8a-10p, 7days",{"$f":"(22-8)*365","v":5110},"Clg 72F/Htg 70F",null,1701,212,"X",null,null,null,"SCooper Htl 8-22 7days w setback - Baseline Design.SIM"]
[null,"5a - 11p, 7 days",{"$f":"(23-5)*365","v":6570},"Clg 72F/Htg 70F",null,1881,294,"X",null,null,null,"SCooper Htl 5-23 7days w setback - Baseline Design.SIM"]
[null,"24/7",8760,"Clg 72F/Htg 70F",null,2040,468,"X",null,null,null,"SCooper Htl 24 7days w setback - Baseline Design.SIM"]
["Retail","9a-6p, M-F",{"$f":"(18-9)*5*52","v":2340},"Clg 72F/Htg 70F",null,1006,45,"X",null,null,null,"SCooper Rtl 9-18 w setback - Baseline Design.SIM"]
[null,"8a-8p, M-F",{"$f":"(20-8)*5*52","v":3120},"Clg 72F/Htg 70F",null,1208,48,"X",null,null,null,"SCooper Rtl 8-20 w setback - Baseline Design.SIM"]
[null,"7a - 10p, M-F",{"$f":"(22-7)*5*52","v":3900},"Clg 72F/Htg 70F",null,1412,39,"X",null,null,null,"SCooper Rtl 7-22 w setback - Baseline Design.SIM"]
[null,"9a-10p, 7 days",{"$f":"(22-9)*365","v":4745},"Clg 72F/Htg 70F",null,1494,39,"X",null,null,null,"SCooper Rtl 9-22 7days w setback - Baseline Design.SIM"]
[null,"8a-10p, 7days",{"$f":"(22-8)*365","v":5110},"Clg 72F/Htg 70F",null,1653,29,"X",null,null,null,"SCooper Rtl 8-22 7days w setback - Baseline Design.SIM"]
[null,"5a - 11p, 7 days",{"$f":"(23-5)*365","v":6570},"Clg 72F/Htg 70F",null,1906,54,"X",null,null,null,"SCooper Rtl 5-23 7days w setback - Baseline Design.SIM"]
[null,"24/7",8760,"Clg 72F/Htg 70F",null,2768,18,"X",null,null,null,"SCooper Rtl 24 7days w setback - Baseline Design.SIM"]
[null,"Mar - Oct, 10a-11p,7 days",{"$f":"(13*7*8*4)","v":2912},null,null,1484,94,null,null,null,"X","SCooper Rtl 10-23 7day Hol1 w setback - Baseline Design.SIM"]
[null,"Apr - Sep, 9a-midnight,7day\nOct -Mar, 10a-6p,7days",{"$f":"(24-9)*7*28+(18-10)*7*6*4","v":4284},null,null,1543,32,null,null,"X",null,"SCooper Rtl 9-24 10-18 Hol2 w setback - Baseline Design.SIM"]
["K-12 School","7a-4p, M-F, 10 mos (close July & August)",{"$f":"(16-7)*5*40","v":1800},"Clg 72F/Htg 70F",null,954,4,null,"X",null,null,"SCooper Sch 7-16 w setback - Baseline Design.SIM"]
[null,"6a-8p, M-F, 10 mos (close July & August)",{"$f":"(20-6)*5*40","v":2800},"Clg 72F/Htg 70F",null,1273,6,null,"X",null,null,"SCooper Sch 6-20 w setback - Baseline Design.SIM"]
[null,"7a-9p, 7 days, 10 mos (close July & August)",{"$f":"(21-7)*7*40","v":3920},"Clg 72F/Htg 70F",null,1358,17,null,"X",null,null,"SCooper Sch 7-21 7days w setback - Baseline Design.SIM"]
[null,"8a-10p, 7days, 12 mos",{"$f":"(22-8)*365","v":5110},"Clg 72F/Htg 70F",null,1729,25,"X",null,null,null,"SCooper Sch 8-22 7days 12mths w setback - Baseline Design.SIM"]
[null,"5a - 11p, 7 days, 12 mos",{"$f":"(23-5)*365","v":6570},"Clg 72F/Htg 70F",null,2006,40,"X",null,null,null,"SCooper Sch 5-23 7days 12 mths w setback - Baseline Design.SIM"]
[null,"24/7",8760,"Clg 72F/Htg 70F",null,2355,100,"X",null,null,null,"SCooper Sch 24h 7days 12 mths w setback - Baseline Design.SIM"]
["Tech College","7a-4p, Mon-Fri, 12months",{"$f":"(16-7)*5*52","v":2340},"Clg 72F/Htg 70F",null,1226,4,"X",null,null,null,"SCooper Tech Col 7-16 w setback - Baseline Design.SIM"]
[null,"6a-8p, M-F, 12 mos",{"$f":"(20-6)*5*52","v":3640},"Clg 72F/Htg 70F",null,1681,5,"X",null,null,null,"SCooper Tech Col 6-20 w setback - Baseline Design.SIM"]
[null,"9a-9p, 7 days, 12 mos",{"$f":"(21-9)*365","v":4380},"Clg 72F/Htg 70F",null,1630,50,"X",null,null,null,"SCooper Tech Col 9-21 7days w setback - Baseline Design.SIM"]
[null,"8a-10p, 7days, 12 mos",{"$f":"(22-8)*365","v":5110},"Clg 72F/Htg 70F",null,1824,45,"X",null,null,null,"SCooper Tech Col 8-22 7days w setback - Baseline Design.SIM"]
[null,"5a - 11p, 7 days, 12 mos",{"$f":"(23-5)*365","v":6570},"Clg 72F/Htg 70F",null,2190,81,"X",null,null,null,"SCooper Tech Col 5-23 7days w setback - Baseline Design.SIM"]
[null,"24/7",8760,"Clg 72F/Htg 70F",null,2656,169,"X",null,null,null,"SCooper Tech Col 24h 7days w setback - Baseline Design.SIM"]
[]
["Facility Type","Schedule","Hours/year","W/O Setback","W/o Setback","EFLCH","EFLHH","Year-round","Close Summer","Extended Summer Hours","Summer Only","File Name",null,"HVAC Calculator Input"]
["Office","8a-5p, M-F",{"$f":"(17-8)*5*52","v":2340},"Clg 72F/Htg 70F","OCC: Clg 72F/Htg 70F, \nUNOCC: Clg 72F/Htg 70F",1375,270,"X",null,null,null,"SCooper Office 8-17 wo  setback - Baseline Design.SIM",null,"Facility Type","Office"]
[null,"7a-7p, M-F",{"$f":"(19-7)*5*52","v":3120},"Clg 72F/Htg 70F",null,1507,236,"X",null,null,null,"SCooper Office 7-19 wo  setback - Baseline Design.SIM"]
[null,"7a - 10p, M-F",{"$f":"(22-7)*5*52","v":3900},"Clg 72F/Htg 70F",null,1669,215,"X",null,null,null,"SCooper Office 7-22 wo  setback - Baseline Design.SIM",null,"Typical Operating Schedule"]
[null,"6a-7p, 7 days",{"$f":"(19-6)*365","v":4745},"Clg 72F/Htg 70F",null,1612,114,"X",null,null,null,"SCooper Office 6-19 7days wo  setback - Baseline Design.SIM",null,null,"Open","Close"]
[null,"6a-9p, 7 days",{"$f":"(21-6)*365","v":5475},"Clg 72F/Htg 70F",null,1720,170,"X",null,null,null,"SCooper Office 6-21 7days wo  setback - Baseline Design.SIM",null,"Mon",7,19]
[null,"5a - 11p, 7 days",{"$f":"(23-5)*365","v":6570},"Clg 72F/Htg 70F",null,1881,114,"X",null,null,null,"SCooper Office 5-23 7days wo  setback - Baseline Design.SIM",null,"Tue",7,19]
[null,"24/7",8760,"Clg 72F/Htg 70F",null,2094,123,"X",null,null,null,"SCooper Office 24 7days wo  setback - Baseline Design.SIM",null,"Wed",7,19]
["Restaurant","9a-6p, M-F",{"$f":"(18-9)*5*52","v":2340},"Clg 72F/Htg 70F",null,1372,507,"X",null,null,null,"SCooper Rest 9-18 wo  setback - Baseline Design.SIM",null,"Thur",7,19]
[null,"8a-8p, M-F",{"$f":"(20-8)*5*52","v":3120},"Clg 72F/Htg 70F",null,1520,473,"X",null,null,null,"SCooper Rest 8-20 wo  setback - Baseline Design.SIM",null,"Fri",7,19]
[null,"7a - 10p, M-F",{"$f":"(22-7)*5*52","v":3900},"Clg 72F/Htg 70F",null,1654,326,"X",null,null,null,"SCooper Rest 7-22 wo  setback - Baseline Design.SIM",null,"Sat",0,0]
[null,"9a-10p, 7 days",{"$f":"(22-9)*365","v":4745},"Clg 72F/Htg 70F",null,2023,198,"X",null,null,null,"SCooper Rest 9-22 7days wo  setback - Baseline Design.SIM",null,"Sun",0,0]
[null,"8a-10p, 7days",{"$f":"(22-8)*365","v":5110},"Clg 72F/Htg 70F",null,2056,137,"X",null,null,null,"SCooper Rest 8-22 7days wo  setback - Baseline Design.SIM",null,"X","Occupied Year-round"]
[null,"5a - 11p, 7 days",{"$f":"(23-5)*365","v":6570},"Clg 72F/Htg 70F",null,2215,97,"X",null,null,null,"SCooper Rest 5-23 7days wo  setback - Baseline Design.SIM",null,null,"Close Summer"]
[null,"24/7",8760,"Clg 72F/Htg 70F",null,2791,26,"X",null,null,null,"SCooper Rest 24 7days wo  setback - Baseline Design.SIM",null,null,"Extended Summer Hours"]
[null,"Mar - Oct, 10a-11p,7 days",{"$f":"(13*7*8*4)","v":2912},null,null,1798,627,null,null,null,"X","SCooper Rest 10-23 7day Hol1 wo  setback - Baseline Design.SIM",null,null,"Summer Only"]
[null,"Apr - Sep, 8a-11p,7day\nOct -Mar, 12a-8p,7days",{"$f":"(23-8)*7*28+(20-12)*7*6*4","v":4284},null,null,1951,352,null,null,"X",null,"SCooper Rest 8-23 12-20 Hol2 wo  setback - Baseline Design.SIM"]
["Hotel","9a-6p, M-F",{"$f":"(18-9)*5*52","v":2340},"Clg 72F/Htg 70F",null,1770,490,"X",null,null,null,"SCooper Htl 9-18 wo  setback - Baseline Design.SIM"]
[null,"8a-9p, M-F",{"$f":"(21-8)*5*52","v":3380},"Clg 72F/Htg 70F",null,1790,500,"X",null,null,null,"SCooper Htl 8-21 wo  setback - Baseline Design.SIM"]
[null,"9a-10p, 7 days",{"$f":"(22-9)*365","v":4745},"Clg 72F/Htg 70F",null,1947,442,"X",null,null,null,"SCooper Htl 9-22 7days wo  setback - Baseline Design.SIM"]
[null,"8a-10p, 7days",{"$f":"(22-8)*365","v":5110},"Clg 72F/Htg 70F",null,1952,391,"X",null,null,null,"SCooper Htl 8-22 7days wo  setback - Baseline Design.SIM"]
[null,"5a - 11p, 7 days",{"$f":"(23-5)*365","v":6570},"Clg 72F/Htg 70F",null,1987,417,"X",null,null,null,"SCooper Htl 5-23 7days wo  setback - Baseline Design.SIM"]
[null,"24/7",8760,"Clg 72F/Htg 70F",null,2040,468,"X",null,null,null,"SCooper Htl 24 7days wo  setback - Baseline Design.SIM"]
["Retail","9a-6p, M-F",{"$f":"(18-9)*5*52","v":2340},"Clg 72F/Htg 70F",null,1323,346,"X",null,null,null,"SCooper Rtl 9-18 wo  setback - Baseline Design.SIM"]
[null,"8a-8p, M-F",{"$f":"(20-8)*5*52","v":3120},"Clg 72F/Htg 70F",null,1468,322,"X",null,null,null,"SCooper Rtl 8-20 wo  setback - Baseline Design.SIM"]
[null,"7a - 10p, M-F",{"$f":"(22-7)*5*52","v":3900},"Clg 72F/Htg 70F",null,1624,246,"X",null,null,null,"SCooper Rtl 7-22 wo  setback - Baseline Design.SIM"]
[null,"9a-10p, 7 days",{"$f":"(22-9)*365","v":4745},"Clg 72F/Htg 70F",null,1655,265,"X",null,null,null,"SCooper Rtl 9-22 7days wo  setback - Baseline Design.SIM"]
[null,"8a-10p, 7days",{"$f":"(22-8)*365","v":5110},"Clg 72F/Htg 70F",null,1802,91,"X",null,null,null,"SCooper Rtl 8-22 7days wo  setback - Baseline Design.SIM"]
[null,"5a - 11p, 7 days",{"$f":"(23-5)*365","v":6570},"Clg 72F/Htg 70F",null,2095,104,"X",null,null,null,"SCooper Rtl 5-23 7days wo  setback - Baseline Design.SIM"]
[null,"24/7",8760,"Clg 72F/Htg 70F",null,1655,265,"X",null,null,null,"SCooper Rtl 24 7days wo  setback - Baseline Design.SIM",{"$f":"0.0695*8760+1317.4","v":1926.2200000000003}]
[null,"Mar - Oct, 10a-11p,7 days",{"$f":"(13*7*8*4)","v":2912},null,null,1318,357,null,null,null,"X","SCooper Rtl 10-23 7day Hol1 wo  setback - Baseline Design.SIM"]
[null,"Apr - Sep, 9a-midnight,7day\nOct -Mar, 10a-6p,7days",{"$f":"(24-9)*7*28+(18-10)*7*6*4","v":4284},null,null,1802,91,null,null,"X",null,"SCooper Rtl 9-24 10-18 Hol2 wo  setback - Baseline Design.SIM"]
["K-12 School","7a-4p, M-F, 10 mos (close July & August)",{"$f":"(16-7)*5*40","v":1800},"Clg 72F/Htg 70F",null,1210,64,null,"X",null,null,"SCooper Sch 7-16 wo  setback - Baseline Design.SIM"]
[null,"6a-8p, M-F, 10 mos (close July & August)",{"$f":"(20-6)*5*40","v":2800},"Clg 72F/Htg 70F",null,1502,67,null,"X",null,null,"SCooper Sch 6-20 wo  setback - Baseline Design.SIM"]
[null,"7a-9p, 7 days, 10 mos (close July & August)",{"$f":"(21-7)*7*40","v":3920},"Clg 72F/Htg 70F",null,1542,31,null,"X",null,null,"SCooper Sch 7-21 7days wo  setback - Baseline Design.SIM"]
[null,"8a-10p, 7days, 12 mos",{"$f":"(22-8)*365","v":5110},"Clg 72F/Htg 70F",null,1816,70,"X",null,null,null,"SCooper Sch 8-22 7days 12mths wo  setback - Baseline Design.SIM"]
[null,"5a - 11p, 7 days, 12 mos",{"$f":"(23-5)*365","v":6570},"Clg 72F/Htg 70F",null,2058,56,"X",null,null,null,"SCooper Sch 5-23 7days 12 mths wo  setback - Baseline Design.SIM"]
[null,"24/7",8760,"Clg 72F/Htg 70F",null,2355,100,"X",null,null,null,"SCooper Sch 24h 7days 12 mths wo  setback - Baseline Design.SIM"]
["Tech College","7a-4p, Mon-Fri, 12months",{"$f":"(16-7)*5*52","v":2340},"Clg 72F/Htg 70F",null,1560,22,"X",null,null,null,"SCooper Tech Col 7-16 wo  setback - Baseline Design.SIM"]
[null,"6a-8p, M-F, 12 mos",{"$f":"(20-6)*5*52","v":3640},"Clg 72F/Htg 70F",null,1935,23,"X",null,null,null,"SCooper Tech Col 6-20 wo  setback - Baseline Design.SIM"]
[null,"9a-9p, 7 days, 12 mos",{"$f":"(21-9)*365","v":4380},"Clg 72F/Htg 70F",null,1820,62,"X",null,null,null,"SCooper Tech Col 9-21 7days wo  setback - Baseline Design.SIM"]
[null,"8a-10p, 7days, 12 mos",{"$f":"(22-8)*365","v":5110},"Clg 72F/Htg 70F",null,1970,49,"X",null,null,null,"SCooper Tech Col 8-22 7days wo  setback - Baseline Design.SIM"]
[null,"5a - 11p, 7 days, 12 mos",{"$f":"(23-5)*365","v":6570},"Clg 72F/Htg 70F",null,2247,86,"X",null,null,null,"SCooper Tech Col 5-23 7days wo  setback - Baseline Design.SIM"]
[null,"24/7",8760,"Clg 72F/Htg 70F",null,2659,159,"X",null,null,null,"SCooper Tech Col 24h 7days wo  setback - Baseline Design.SIM"]
[]
[]
["Other"]
["Avg. Hours","Hours",null,null,null,null,null,"EFLCH",null,null,null,null,null,"Avg. EFCH"]
[{"$f":"AVERAGE(B94:G94)","v":2340},{"$f":"(17-8)*5*52","v":2340},{"$f":"(18-9)*5*52","v":2340},{"$f":"(18-9)*5*52","v":2340},{"$f":"(18-9)*5*52","v":2340},null,{"$f":"(16-7)*5*52","v":2340},1375,1372,1770,1323,null,1560,{"$f":"AVERAGE(H94:M94)","v":1480}]
[{"$f":"AVERAGE(B95:G95)","v":3120},{"$f":"(19-7)*5*52","v":3120},{"$f":"(20-8)*5*52","v":3120},null,{"$f":"(20-8)*5*52","v":3120},null,null,1507,1520,null,1468,null,null,{"$f":"AVERAGE(H95:M95)","v":1498.3333333333333}]
[3380,null,null,{"$f":"(21-8)*5*52","v":3380},null,null,null,null,null,1790,null,null,null,1790]
[3640,null,null,null,null,null,{"$f":"(20-6)*5*52","v":3640},null,null,null,null,null,1935,1935]
[3900,{"$f":"(22-7)*5*52","v":3900},{"$f":"(22-7)*5*52","v":3900},null,{"$f":"(22-7)*5*52","v":3900},null,null,1669,1654,null,1624,null,null,1649]
[4380,null,null,null,null,null,{"$f":"(21-9)*365","v":4380},null,null,null,null,null,1820,1820]
[4745,{"$f":"(19-6)*365","v":4745},{"$f":"(22-9)*365","v":4745},{"$f":"(22-9)*365","v":4745},{"$f":"(22-9)*365","v":4745},null,null,1612,2023,1947,1655,null,null,1809.25]
[5110,null,{"$f":"(22-8)*365","v":5110},{"$f":"(22-8)*365","v":5110},{"$f":"(22-8)*365","v":5110},{"$f":"(22-8)*365","v":5110},{"$f":"(22-8)*365","v":5110},null,2056,1952,1802,1816,1970,1919.2]
[5475,{"$f":"(21-6)*365","v":5475},null,null,null,null,null,1720,null,null,null,null,null,1720]
[6570,{"$f":"(23-5)*365","v":6570},6570,6570,6570,6570,6570,1881,2215,1987,2095,2058,2247,2080.5]
[8760,8760,8760,8760,8760,8760,8760,2094,2791,2040,1655,2355,2659,2265.6666666666665]
[]
["Avg. Hours","Hours",null,null,null,null,null,"EFLHH",null,null,null,null,null,"Avg. EFCH"]
[{"$f":"AVERAGE(B107:G107)","v":2340},{"$f":"(17-8)*5*52","v":2340},{"$f":"(18-9)*5*52","v":2340},{"$f":"(18-9)*5*52","v":2340},{"$f":"(18-9)*5*52","v":2340},null,{"$f":"(16-7)*5*52","v":2340},270,507,490,346,null,22,{"$f":"AVERAGE(H107:M107)","v":327}]
[{"$f":"AVERAGE(B108:G108)","v":3120},{"$f":"(19-7)*5*52","v":3120},{"$f":"(20-8)*5*52","v":3120},null,{"$f":"(20-8)*5*52","v":3120},null,null,236,473,null,322,null,null,{"$f":"AVERAGE(H108:M108)","v":343.66666666666669}]
[3380,null,null,{"$f":"(21-8)*5*52","v":3380},null,null,null,null,null,500]
[3640,null,null,null,null,null,{"$f":"(20-6)*5*52","v":3640},null,null,null,null,null,23]
[3900,{"$f":"(22-7)*5*52","v":3900},{"$f":"(22-7)*5*52","v":3900},null,{"$f":"(22-7)*5*52","v":3900},null,null,215,326,null,246,null,null,262.33333333333331]
[4380,null,null,null,null,null,{"$f":"(21-9)*365","v":4380},null,null,null,null,null,62]
[4745,{"$f":"(19-6)*365","v":4745},{"$f":"(22-9)*365","v":4745},{"$f":"(22-9)*365","v":4745},{"$f":"(22-9)*365","v":4745},null,null,114,198,442,265,null,null,{"$f":"AVERAGE(H113:M113)","v":254.75}]
[5110,null,{"$f":"(22-8)*365","v":5110},{"$f":"(22-8)*365","v":5110},{"$f":"(22-8)*365","v":5110},{"$f":"(22-8)*365","v":5110},{"$f":"(22-8)*365","v":5110},null,137,391,91,70,49,147.6]
[5475,{"$f":"(21-6)*365","v":5475},null,null,null,null,null,170,null,null,null,null,null,170]
[6570,{"$f":"(23-5)*365","v":6570},6570,6570,6570,6570,6570,114,97,417,104,56,86,145.66666666666666]
[8760,8760,8760,8760,8760,8760,8760,123,26,468,265,100,159,190.16666666666666]

{"sheet":"Original Schedule","index":3,"n_rows":8,"n_cols":4,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
["Operation Hours","Schedule","EFLCH","EFLHH"]
["Office","7a-7p, M-F",1624.5,270.8]
["Restaurant/Retail","8a-10p, 7days",2547.5,314.40000000000003]
["Hotel","24/7",3745.125,846.80000000000007]
["Retail 2","10a-9p, Mon-Sat; 12p-6p, Sun",1975.75,297.2]
["Restaurant 2","10a-10p, Mon-Sat",1932,206.6]
["K-12 School","7a-4p, Mon-Fri, 10months",1077.625,208.2]
["Tech College","7a-4p, Mon-Fri, 12months",1218.625,136.20000000000002]

{"sheet":"BINs","index":4,"n_rows":34,"n_cols":18,"rows_kept":34,"cut":false,"hidden":true,"merged":[[0,0,0,4],[0,6,0,10],[0,12,0,16]]}
["Class I",null,null,null,null,null,"Class II",null,null,null,null,null,"Class I"]
["TMY3 Dry Bulb BIN Data for CHARLESTON INTL ARPT",null,null,null,null,null,"TMY3 Dry Bulb BIN Data for MYRTLE BEACH AFB",null,null,null,null,null,"TMY3 Dry Bulb BIN Data for WILMINGTON INTL ARPT"]
["DB Temperature BIN","Occupied","Unoccupied","Total","MCWB",null,"DB Temperature BIN","Occupied","Unoccupied","Total","MCWB",null,"DB Temperature BIN","Occupied","Unoccupied","Total","MCWB"]
[107.5,0,0,0,"-","",107.5,0,0,0,"-",null,107.5,0,0,0,"-",""]
[102.5,2,0,2,83.09,2,102.5,0,0,0,"-",null,102.5,0,0,0,"-",""]
[97.5,14,0,14,81.92,1.8,97.5,5,0,5,76.847999999999999,null,97.5,19,2,21,80.119047619047592,3.2]
[92.5,62,38,100,78.67200000000004,1.7777777777777777,92.5,24,12,36,77.390277777777783,null,92.5,57,29,86,77.636976744186043,1.3888888888888888]
[87.5,361,137,498,75.623172690763141,0.95294117647058818,87.5,196,59,255,77.383647058823641,null,87.5,219,81,300,75.346766666666852,0.17647058823529413]
[82.5,544,335,879,73.779135381115026,-0.13484251968503938,82.5,618,398,1016,74.659862204724419,null,82.5,503,322,825,73.508424242424297,-0.18799212598425197]
[77.5,455,792,1247,71.740360866078603,7.5927523727351162E-2,77.5,420,739,1159,70.932381363244275,null,77.5,456,841,1297,72.018388589051497,0.11906816220880069]
[72.5,304,758,1062,67.864510357814851,3.9138943248532287E-2,72.5,301,721,1022,67.098825831702456,null,72.5,304,643,947,67.811172122491655,-7.3385518590998039E-2]
[67.5,376,705,1081,62.572340425531586,9.081735620585267E-2,67.5,339,652,991,62.002532795156263,null,67.5,335,498,833,61.949363745497813,-0.15943491422805248]
[62.5,303,773,1076,58.225157992565038,0.15080213903743314,62.5,271,664,935,56.904000000000053,null,62.5,321,720,1041,58.037396733909659,0.11336898395721925]
[57.5,184,485,669,52.939820627802419,-0.18810679611650485,57.5,269,555,824,52.075679611650386,null,57.5,251,482,733,52.79773533424261,-0.1104368932038835]
[52.5,154,450,604,48.03927152317867,-0.19034852546916889,52.5,267,479,746,47.026796246648644,null,52.5,236,520,756,48.192354497354216,1.3404825737265416E-2]
[47.5,104,284,388,43.173479381443244,-0.24806201550387597,47.5,160,356,516,42.480639534883736,null,47.5,191,399,590,43.716288135593096,0.1434108527131783]
[42.5,133,323,456,38.337587719298121,-8.617234468937876E-2,42.5,135,364,499,37.608897795591126,null,42.5,121,478,599,39.291368948247083,0.20040080160320642]
[37.5,93,298,391,33.601099744245523,-3.2178217821782179E-2,37.5,78,326,404,33.796509900990031,null,37.5,76,368,444,34.483603603603576,9.9009900990099015E-2]
[32.5,34,146,180,28.890166666666634,-0.2857142857142857,32.5,42,210,252,29.361984126984044,null,32.5,31,181,212,29.870047169811297,-0.15873015873015872]
[27.5,8,83,91,24.600769230769231,0.13750000000000001,27.5,7,73,80,24.259375000000013,null,27.5,11,58,69,25.253768115942023,-0.13750000000000001]
[22.5,1,21,22,20.307727272727274,0.46666666666666667,22.5,0,15,15,19.532666666666668,null,22.5,1,6,7,20.811428571428571,-0.53333333333333333]
[17.5,0,0,0,"-",-5,17.5,0,5,5,14.616000000000003,null,17.5,0,0,0,"-",-5]
[12.5,0,0,0,"-","",12.5,0,0,0,"-",null,12.5,0,0,0,"-",""]
[7.5,0,0,0,"-","",7.5,0,0,0,"-",null,7.5,0,0,0,"-",""]
[2.5,0,0,0,"-","",2.5,0,0,0,"-",null,2.5,0,0,0,"-",""]
[-2.5,0,0,0,"-","",-2.5,0,0,0,"-",null,-2.5,0,0,0,"-",""]
[-7.5,0,0,0,"-","",-7.5,0,0,0,"-",null,-7.5,0,0,0,"-",""]
[-12.5,0,0,0,"-","",-12.5,0,0,0,"-",null,-12.5,0,0,0,"-",""]
[-17.5,0,0,0,"-","",-17.5,0,0,0,"-",null,-17.5,0,0,0,"-",""]
[-22.5,0,0,0,"-","",-22.5,0,0,0,"-",null,-22.5,0,0,0,"-",""]
[-27.5,0,0,0,"-","",-27.5,0,0,0,"-",null,-27.5,0,0,0,"-",""]
[-32.5,0,0,0,"-","",-32.5,0,0,0,"-",null,-32.5,0,0,0,"-",""]
["Total Hours",3132,5628,8760,null,null,"Total Hours",3132,5628,8760,null,null,"Total Hours",3132,5628,8760]
["Occ. Hours: 7:00-19:00 M-F Closed Sat., and Closed Sun.",null,null,null,null,null,"Occ. Hours: 7:00-19:00 M-F Closed Sat., and Closed Sun.",null,null,null,null,null,"Occ. Hours: 7:00-19:00 M-F Closed Sat., and Closed Sun."]

{"sheet":"HVAC Calculator","index":5,"n_rows":84,"n_cols":55,"rows_kept":84,"cut":false,"hidden":true,"merged":[[7,1,7,2],[6,1,6,2],[17,6,18,7],[18,4,18,5],[10,1,10,2],[9,1,9,2],[8,1,8,2],[10,5,10,7],[33,1,34,4],[17,1,17,4],[26,7,26,8],[26,9,26,11],[34,7,34,8],[34,9,34,11],[25,1,26,4],[4,46,7,46],[16,26,18,26],[4,16,4,17],[0,6,1,11],[40,38,64,38],[8,3,8,7],[9,9,9,11],[7,3,7,7],[1,37,7,38],[13,5,13,11],[19,13,20,17],[33,13,33,17],[16,25,18,25],[16,24,18,24],[16,23,18,23],[16,22,18,22],[10,9,10,11],[11,9,11,11],[40,41,40,42],[16,32,17,33],[16,30,17,31],[23,41,23,42],[17,8,18,9],[17,10,18,11],[16,27,18,27],[16,19,18,20],[16,21,18,21],[16,29,18,29],[16,28,18,28],[65,38,81,38],[65,41,65,42],[82,38,83,38],[82,41,82,42],[8,41,8,42],[8,38,39,38],[4,1,5,4],[15,1,15,2],[13,1,13,2],[4,54,7,54],[4,51,7,51],[4,47,7,47],[4,48,7,48],[4,49,7,49],[4,52,7,52],[4,50,7,50],[4,13,5,13],[4,15,5,15],[6,9,6,11],[6,3,6,7],[7,9,7,11],[8,9,8,11],[1,39,1,54],[2,9,2,11],[4,9,4,11],[3,40,7,40],[3,41,3,42],[3,43,3,48],[3,49,3,54],[6,39,7,39],[5,9,5,11],[4,41,6,42],[4,43,7,43],[4,44,7,44],[4,45,7,45],[4,53,7,53],[0,15,1,17],[3,15,3,17]]}
[null,null,null,null,null,null,"HVAC Calculator",null,null,null,null,null,null,null,null,{"$f":"G1","v":"HVAC Calculator"},null,null,null,{"$f":"COLUMN()","v":20},{"$f":"COLUMN()","v":21},{"$f":"COLUMN()","v":22},{"$f":"COLUMN()","v":23},{"$f":"COLUMN()","v":24},{"$f":"COLUMN()","v":25},{"$f":"COLUMN()","v":26},{"$f":"COLUMN()","v":27},{"$f":"COLUMN()","v":28},{"$f":"COLUMN()","v":29},{"$f":"COLUMN()","v":30},{"$f":"COLUMN()","v":31},{"$f":"COLUMN()","v":32},{"$f":"COLUMN()","v":33},{"$f":"COLUMN()","v":34}]
[]
[null,null,null,null,null,null,null,null,null,"10.02.2024",null,null,null,null,null,null,null,{"$f":"J3","v":"10.02.2024"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Op Hrs",{"$f":"SUM(F$16:L$16)*52.14285714","v":0},null,null,"Occupied Year-round",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling",null,"IEEC 2009/IECC 2012",null,null,null,null,null,"Minimum Program Requirements"]
[null,"Customer Information",null,null,null,null,null,null,null,"Project Number",null,null,null,"Std Eff",null,"Hi Eff",{"$f":"IF(J6=\"\",\"\",J6)","v":""},null,null,null,"EFLCH",{"$f":"IF(AnnualHours=0, 0,EFLHCalculation(AnnualHours,D14,D16,\"EFLCH\"))","v":0},null,null,"Closed Summer",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No Code Min = Estimated Value",null,"Capacity",null,"Path A Full Load Cooling","Path A Part Load Cooling","Path A Full Load Heating","Path B Full Load Cooling","Path B Part Load Cooling","Path B Full Load Heating","Tier 1 Full Load Cooling","Tier 1 Full Part Cooling","Tier 1 Full Load Heating","Tier 2 Full Load Cooling","Tier 2 Full Part Cooling","Tier 3 Full Load Heating"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Annual Equip Operating Cost",null,null,"EFLHH",{"$f":"IF(AnnualHours=0, 0,EFLHCalculation(AnnualHours,D14,D16,\"EFLHH\"))","v":0},null,null,"Extended Summer Hours",null,"Cost","kWh","Demand",null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,"Project",null,null,null,null,null,null,null,"Account Number",null,null,null,{"$f":"J27","v":0},"Project Cost",{"$f":"J35","v":0},null,null,null,null,null,null,null,null,"Summer Only",null,{"$f":"J12","v":0},{"$f":"IF($AA$7=0,0,VLOOKUP($AA$7,$AA$8:$AC$14,2,0))","v":0},{"$f":"IF($AA$7=0,0,VLOOKUP($AA$7,$AA$8:$AC$14,3,0))","v":0}]
[null,"Business",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Hotel",null,null,null,"GA",9.9199999999999997E-2,0,null,null,null,null,null,null,null,null,null,null,null,null,">=","<"]
[null,"Address",null,null,null,null,null,null,null,"Meter Number",null,null,null,{"$f":"AJ33","v":0},"Total Project Rebate",{"$f":"AJ35","v":0},"Existing",{"$f":"AI25","v":0},null,null,null,null,"K-12 School",null,null,null,"GB",4.0800000000000003E-2,22.94,null,null,null,null,null,null,null,null,1,"< 65,000 BTU/HR HP and AC",null,null,"BTUh",null,{"$f":"\"\"","v":""},"SEER","HSPF",null,null,null,{"$f":"\"\"","v":""},"SEER","HSPF",{"$f":"\"\"","v":""},"SEER","HSPF"]
[null,"City",null,null,"State","SC","Zip",null,null,null,null,null,null,null,null,null,{"$f":"P5","v":"Hi Eff"},{"$f":"P13","v":0},null,null,null,null,"Office",null,null,null,"GV",4.0800000000000003E-2,24.6,null,null,null,null,null,null,null,null,1,null,"1 Phase Heat Pump Single Package","HP1SP65",0,65000,null,14,8,null,null,null,null,15,8.1999999999999993,null,17,9]
[null,"Contact",null,null,"Phone",null,null,null,null,"Rate Schedule",null,null,null,{"$f":"N7-N9","v":0},"Net Project Cost",{"$f":"P7-P9","v":0},{"$f":"N5","v":"Std Eff"},{"$f":"N13","v":0},null,null,null,null,"Restaurant",null,null,null,"GT",3.85E-2,14.519399999999999,null,null,null,null,null,null,null,null,1,null,"1 Phase Heat Pump Split System","HP1SS65",0,65000,null,14,8.1999999999999993,null,null,null,null,15,8.5,null,17,9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Retail",null,null,null,"GL",3.9800000000000002E-2,23.29,null,null,null,null,null,null,null,null,1,null,"3 Phase Heat Pump Single Package","HP3SP65",0,65000,null,13,7.7,null,null,null,null,{"$f":"AS12","v":13},7.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AI33","v":0},"Annual Op Cost",{"$f":"AI35","v":0},null,null,null,null,null,null,"Tech College",null,null,null,"TP",0.1273,0,null,null,null,null,null,null,null,null,1,null,"3 Phase Heat Pump Split System","HP3SS65",0,65000,null,13,7.7,null,null,null,null,13,7.7]
[null,"Building",null,null,null,"Op. Hours",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Other",null,null,null,"TA",6.8900000000000003E-2,9.75,null,null,null,null,null,null,null,null,1,null,"3 Phase Unitary AC Single Package","AC3SP65",0,65000,null,13,null,null,null,null,null,{"$f":"AS14","v":13}]
[null,null,null,null,null,"Mon","Tue","Wed","Thu","Fri","Sat","Sun",null,null,"Upgrade Cost From Std Eff",{"$f":"P11-N11","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"3 Phase Unitary AC Split System","AC3SS65",0,65000,null,13,null,null,null,null,null,{"$f":"AS15","v":13}]
[null,"Schedule",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"VRF/Mini-Split AC","ACVRF65",0,65000,null,13,null,null,null,null,null,14]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Annual Savings Over Std Eff",{"$f":"IF(N13<P13,0,N13-P13)","v":0},null,null,null,"Equipment Code",null,"Code Full Load Cooling","Code Part Load Cooling","Code Full Load Heating","Tier 1 Full Load Cooling","Tier 1 Part Load Cooling","Tier 1 Full Load Heating","Tier 2 Full Load Cooling","Tier 2 Part Load Cooling","Tier 2 Full Load Heating","Code Usage",null,"Equipment Usage",null,null,null,null,1,null,"VRF/Mini-Split HP","HPVRF65",0,65000,null,13,7.7,null,null,null,null,14,8]
[null,"Existing Equipment (Optional)",null,null,null,null,"Full Load Cooling",null,"Part Load Cooling",null,"Full Load Heating",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"(SEER2/HSPF2) 3 Phase Heat Pump Single Package","S2HP3SP65",0,65000,null,13.4,6.7,null,null,null,null,13.4,6.7]
[null,null,"Qty","HVAC Type","Cooling Capacity",null,null,null,null,null,null,null,null,null,"Simple Payback Over Std Eff",{"$f":"TEXT(N23,\"0.0\") & \" Years\"","v":"0.0 Years"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"kW","kWh","kW","kWh","Op Cost","Rebate",null,1,null,"(SEER2/HSPF2) 3 Phase Heat Pump Split System","S2HP3SS65",0,65000,null,14.3,7.5,null,null,null,null,14.3,7.5]
[null,1,null,null,null,{"$f":"IF($D20=\"\",\"\",FindIndex($D20,$E20,$G20,$I20,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D20=\"\",\"\",FindIndex($D20,$E20,$G20,$I20,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D20=\"\",\"\",FindIndex($D20,$E20,$G20,$I20,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D20=\"\",\"\",FindIndex($D20,$E20,$G20,$I20,K$18 &\" Units\"))","v":""},null,"Estimated Project and Operation Cost",null,null,null,null,null,1,{"$f":"IF($D20=\"\",\"\",FindIndex($D20,$E20,$G20,$I20,T$17))","v":""},{"$f":"IF(AND(E20=\"\",$D20=\"\"),\"\",FindIndex($D20,$E20,$G20,$I20,V$17))","v":""},{"$f":"IF(AND(E20=\"\",$D20=\"\"),\"\",FindIndex($D20,$E20,$G20,$I20,W$17))","v":""},{"$f":"IF(AND(E20=\"\",$D20=\"\"),\"\",FindIndex($D20,$E20,$G20,$I20,X$17))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF($U20=\"\",\"\",usage($C20,$E20,$G20,$H20,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U20=\"\",\"\",usage($C20,$E20,$I20,$J20,EFLCH,EFLHH,$AH$19)+ IF($K20=\"\",0,usage($C20,$E20,$K20,$L20,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF(AG20=\"\",\"\",AG20*DperKW*12+AH20*DperKWH)","v":""},null,null,1,null,"(SEER2) 3 Phase Unitary AC Single Package","S2AC3SP65",0,65000,null,13.4,null,null,null,null,null,13.4]
[null,2,null,null,null,{"$f":"IF($D21=\"\",\"\",FindIndex($D21,$E21,$G21,$I21,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D21=\"\",\"\",FindIndex($D21,$E21,$G21,$I21,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D21=\"\",\"\",FindIndex($D21,$E21,$G21,$I21,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D21=\"\",\"\",FindIndex($D21,$E21,$G21,$I21,K$18 &\" Units\"))","v":""},null,null,null,null,null,null,null,2,{"$f":"IF($D21=\"\",\"\",FindIndex($D21,$E21,$G21,$I21,T$17))","v":""},{"$f":"IF(AND(E21=\"\",$D21=\"\"),\"\",FindIndex($D21,$E21,$G21,$I21,V$17))","v":""},{"$f":"IF(AND(E21=\"\",$D21=\"\"),\"\",FindIndex($D21,$E21,$G21,$I21,W$17))","v":""},{"$f":"IF(AND(E21=\"\",$D21=\"\"),\"\",FindIndex($D21,$E21,$G21,$I21,X$17))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF($U21=\"\",\"\",usage($C21,$E21,$G21,$H21,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U21=\"\",\"\",usage($C21,$E21,$I21,$J21,EFLCH,EFLHH,$AH$19)+ IF($K21=\"\",0,usage($C21,$E21,$K21,$L21,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF(AG21=\"\",\"\",AG21*DperKW*12+AH21*DperKWH)","v":""},null,null,1,null,"(SEER2) 3 Phase Unitary AC Split System","S2AC3SS65",0,65000,null,13.4,null,null,null,null,null,13.4]
[null,3,null,null,null,{"$f":"IF($D22=\"\",\"\",FindIndex($D22,$E22,$G22,$I22,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D22=\"\",\"\",FindIndex($D22,$E22,$G22,$I22,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D22=\"\",\"\",FindIndex($D22,$E22,$G22,$I22,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D22=\"\",\"\",FindIndex($D22,$E22,$G22,$I22,K$18 &\" Units\"))","v":""},null,null,{"$f":"Q9","v":"Existing"},{"$f":"Q10","v":"Hi Eff"},{"$f":"Q11","v":"Std Eff"},null,null,3,{"$f":"IF($D22=\"\",\"\",FindIndex($D22,$E22,$G22,$I22,T$17))","v":""},{"$f":"IF(AND(E22=\"\",$D22=\"\"),\"\",FindIndex($D22,$E22,$G22,$I22,V$17))","v":""},{"$f":"IF(AND(E22=\"\",$D22=\"\"),\"\",FindIndex($D22,$E22,$G22,$I22,W$17))","v":""},{"$f":"IF(AND(E22=\"\",$D22=\"\"),\"\",FindIndex($D22,$E22,$G22,$I22,X$17))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF($U22=\"\",\"\",usage($C22,$E22,$G22,$H22,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U22=\"\",\"\",usage($C22,$E22,$I22,$J22,EFLCH,EFLHH,$AH$19)+ IF($K22=\"\",0,usage($C22,$E22,$K22,$L22,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF(AG22=\"\",\"\",AG22*DperKW*12+AH22*DperKWH)","v":""},null,null,1,null,"(SEER2) VRF/Mini-Split AC","S2ACVRF65",0,65000,null,13.4,null,null,null,null,null,13.4]
[null,4,null,null,null,{"$f":"IF($D23=\"\",\"\",FindIndex($D23,$E23,$G23,$I23,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D23=\"\",\"\",FindIndex($D23,$E23,$G23,$I23,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D23=\"\",\"\",FindIndex($D23,$E23,$G23,$I23,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D23=\"\",\"\",FindIndex($D23,$E23,$G23,$I23,K$18 &\" Units\"))","v":""},null,{"$f":"IF(P17=0,0,P15/P17)","v":0},null,{"$f":"$P$11+($P$13*$N23)","v":0},null,null,null,4,{"$f":"IF($D23=\"\",\"\",FindIndex($D23,$E23,$G23,$I23,T$17))","v":""},{"$f":"IF(AND(E23=\"\",$D23=\"\"),\"\",FindIndex($D23,$E23,$G23,$I23,V$17))","v":""},{"$f":"IF(AND(E23=\"\",$D23=\"\"),\"\",FindIndex($D23,$E23,$G23,$I23,W$17))","v":""},{"$f":"IF(AND(E23=\"\",$D23=\"\"),\"\",FindIndex($D23,$E23,$G23,$I23,X$17))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF($U23=\"\",\"\",usage($C23,$E23,$G23,$H23,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U23=\"\",\"\",usage($C23,$E23,$I23,$J23,EFLCH,EFLHH,$AH$19)+ IF($K23=\"\",0,usage($C23,$E23,$K23,$L23,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF(AG23=\"\",\"\",AG23*DperKW*12+AH23*DperKWH)","v":""},null,null,1,null,"(SEER2/HSPF2) VRF/Mini-Split HP","S2HPVRF65",0,65000,null,13.4,7.5,null,null,null,null,13.4,7.5]
[null,5,null,null,null,{"$f":"IF($D24=\"\",\"\",FindIndex($D24,$E24,$G24,$I24,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D24=\"\",\"\",FindIndex($D24,$E24,$G24,$I24,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D24=\"\",\"\",FindIndex($D24,$E24,$G24,$I24,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D24=\"\",\"\",FindIndex($D24,$E24,$G24,$I24,K$18 &\" Units\"))","v":""},null,0,{"$f":"$AI$25*N24","v":0},{"$f":"$P$11+($P$13*$N24)","v":0},{"$f":"$N$11+($N$13*$N24)","v":0},null,null,5,{"$f":"IF($D24=\"\",\"\",FindIndex($D24,$E24,$G24,$I24,T$17))","v":""},{"$f":"IF(AND(E24=\"\",$D24=\"\"),\"\",FindIndex($D24,$E24,$G24,$I24,V$17))","v":""},{"$f":"IF(AND(E24=\"\",$D24=\"\"),\"\",FindIndex($D24,$E24,$G24,$I24,W$17))","v":""},{"$f":"IF(AND(E24=\"\",$D24=\"\"),\"\",FindIndex($D24,$E24,$G24,$I24,X$17))","v":""},null,null,null,null,null,null,null,null,{"$f":"IF($U24=\"\",\"\",usage($C24,$E24,$G24,$H24,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U24=\"\",\"\",usage($C24,$E24,$I24,$J24,EFLCH,EFLHH,$AH$19)+ IF($K24=\"\",0,usage($C24,$E24,$K24,$L24,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF(AG24=\"\",\"\",AG24*DperKW*12+AH24*DperKWH)","v":""},null,null,1,null,null,null,"BTUh",null,"EER",{"$f":"\"\"","v":""},"COP",null,null,null,"EER",{"$f":"\"\"","v":""},"COP","EER",{"$f":"\"\"","v":""},"COP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,2,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AG20:AG24)","v":0},0,0,0,null,1,null,"PTAC (New Construction)","PTAC80",0,8001,0,null,null,null,null,null,11.8]
[null,"Std Eff Option (Optional)",null,null,null,null,null,null,null,null,null,null,null,4,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"PTAC (New Construction)","PTAC105",8001,10501,0,null,null,null,null,null,11.4]
[null,null,null,null,null,null,null,"Project Cost",null,null,null,null,null,6,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"PTAC (New Construction)","PTAC135",10501,13501,0,null,null,null,null,null,10.7]
[null,1,null,null,null,{"$f":"IF($D28=\"\",\"\",FindIndex($D28,$E28,$G28,$I28,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D28=\"\",\"\",FindIndex($D28,$E28,$G28,$I28,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D28=\"\",\"\",FindIndex($D28,$E28,$G28,$I28,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D28=\"\",\"\",FindIndex($D28,$E28,$G28,$I28,K$18 &\" Units\"))","v":""},null,8,0,0,0,null,null,1,{"$f":"IF($D28=\"\",\"\",FindIndex($D28,$E28,$G28,$I28,T$17))","v":""},{"$f":"IF(AND(E28=\"\",$D28=\"\"),\"\",FindIndex($D28,$E28,$G28,$I28,V$17))","v":""},{"$f":"IF(AND(E28=\"\",$D28=\"\"),\"\",FindIndex($D28,$E28,$G28,$I28,W$17))","v":""},{"$f":"IF(AND(E28=\"\",$D28=\"\"),\"\",FindIndex($D28,$E28,$G28,$I28,X$17))","v":""},{"$f":"IF(AND(H28=\"\",$D28=\"\"),\"\",FindIndex($D28,$E28,$G28,$I28,Y$17))","v":""},{"$f":"IF(AND(H28=\"\",$D28=\"\"),\"\",FindIndex($D28,$E28,$G28,$I28,Z$17))","v":""},{"$f":"IF(AND(H28=\"\",$D28=\"\"),\"\",FindIndex($D28,$E28,$G28,$I28,AA$17))","v":""},{"$f":"IF(AND(K28=\"\",$D28=\"\"),\"\",FindIndex($D28,$E28,$G28,$I28,AB$17))","v":""},{"$f":"IF(AND(K28=\"\",$D28=\"\"),\"\",FindIndex($D28,$E28,$G28,$I28,AC$17))","v":""},{"$f":"IF(AND(K28=\"\",$D28=\"\"),\"\",FindIndex($D28,$E28,$G28,$I28,AD$17))","v":""},{"$f":"IF($U28=\"\",\"\",usage($C28,$E28,$V28,$H28,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U28=\"\",\"\",usage($C28,$E28,$W28,$J28,EFLCH,EFLHH,$AH$19)+ IF($X28=\"\",0,usage($C28,$E28,$X28,$L28,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF($U28=\"\",\"\",usage($C28,$E28,$G28,$H28,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U28=\"\",\"\",usage($C28,$E28,$I28,$J28,EFLCH,EFLHH,$AH$19)+ IF($K28=\"\",0,usage($C28,$E28,$K28,$L28,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF(AG28=\"\",\"\",AG28*DperKW*12+AH28*DperKWH)","v":""},{"$f":"IF(AH28=\"\",\"\",rebate(C28,D28,E28,G28,I28,K28,U28,AE28-AG28,AF28-AH28,Y28,Z28,AA28,AB28,AC28,AD28))","v":""},null,1,null,"PTAC (New Construction)","PTACL",13501,1000000,0,null,null,null,null,null,10]
[null,2,null,null,null,{"$f":"IF($D29=\"\",\"\",FindIndex($D29,$E29,$G29,$I29,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D29=\"\",\"\",FindIndex($D29,$E29,$G29,$I29,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D29=\"\",\"\",FindIndex($D29,$E29,$G29,$I29,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D29=\"\",\"\",FindIndex($D29,$E29,$G29,$I29,K$18 &\" Units\"))","v":""},null,10,0,0,0,null,null,2,{"$f":"IF($D29=\"\",\"\",FindIndex($D29,$E29,$G29,$I29,T$17))","v":""},{"$f":"IF(AND(E29=\"\",$D29=\"\"),\"\",FindIndex($D29,$E29,$G29,$I29,V$17))","v":""},{"$f":"IF(AND(E29=\"\",$D29=\"\"),\"\",FindIndex($D29,$E29,$G29,$I29,W$17))","v":""},{"$f":"IF(AND(E29=\"\",$D29=\"\"),\"\",FindIndex($D29,$E29,$G29,$I29,X$17))","v":""},{"$f":"IF(AND(H29=\"\",$D29=\"\"),\"\",FindIndex($D29,$E29,$G29,$I29,Y$17))","v":""},{"$f":"IF(AND(H29=\"\",$D29=\"\"),\"\",FindIndex($D29,$E29,$G29,$I29,Z$17))","v":""},{"$f":"IF(AND(H29=\"\",$D29=\"\"),\"\",FindIndex($D29,$E29,$G29,$I29,AA$17))","v":""},{"$f":"IF(AND(K29=\"\",$D29=\"\"),\"\",FindIndex($D29,$E29,$G29,$I29,AB$17))","v":""},{"$f":"IF(AND(K29=\"\",$D29=\"\"),\"\",FindIndex($D29,$E29,$G29,$I29,AC$17))","v":""},{"$f":"IF(AND(K29=\"\",$D29=\"\"),\"\",FindIndex($D29,$E29,$G29,$I29,AD$17))","v":""},{"$f":"IF($U29=\"\",\"\",usage($C29,$E29,$V29,$H29,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U29=\"\",\"\",usage($C29,$E29,$W29,$J29,EFLCH,EFLHH,$AH$19)+ IF($X29=\"\",0,usage($C29,$E29,$X29,$L29,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF($U29=\"\",\"\",usage($C29,$E29,$G29,$H29,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U29=\"\",\"\",usage($C29,$E29,$I29,$J29,EFLCH,EFLHH,$AH$19)+ IF($K29=\"\",0,usage($C29,$E29,$K29,$L29,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF(AG29=\"\",\"\",AG29*DperKW*12+AH29*DperKWH)","v":""},{"$f":"IF(AH29=\"\",\"\",rebate(C29,D29,E29,G29,I29,K29,U29,AE29-AG29,AF29-AH29,Y29,Z29,AA29,AB29,AC29,AD29))","v":""},null,1,null,"PTAC (Retrofit)","PTAC80",0,8001,0,null,null,null,null,null,{"$f":"AX25","v":11.8}]
[null,3,null,null,null,{"$f":"IF($D30=\"\",\"\",FindIndex($D30,$E30,$G30,$I30,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D30=\"\",\"\",FindIndex($D30,$E30,$G30,$I30,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D30=\"\",\"\",FindIndex($D30,$E30,$G30,$I30,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D30=\"\",\"\",FindIndex($D30,$E30,$G30,$I30,K$18 &\" Units\"))","v":""},null,null,null,null,null,null,null,3,{"$f":"IF($D30=\"\",\"\",FindIndex($D30,$E30,$G30,$I30,T$17))","v":""},{"$f":"IF(AND(E30=\"\",$D30=\"\"),\"\",FindIndex($D30,$E30,$G30,$I30,V$17))","v":""},{"$f":"IF(AND(E30=\"\",$D30=\"\"),\"\",FindIndex($D30,$E30,$G30,$I30,W$17))","v":""},{"$f":"IF(AND(E30=\"\",$D30=\"\"),\"\",FindIndex($D30,$E30,$G30,$I30,X$17))","v":""},{"$f":"IF(AND(H30=\"\",$D30=\"\"),\"\",FindIndex($D30,$E30,$G30,$I30,Y$17))","v":""},{"$f":"IF(AND(H30=\"\",$D30=\"\"),\"\",FindIndex($D30,$E30,$G30,$I30,Z$17))","v":""},{"$f":"IF(AND(H30=\"\",$D30=\"\"),\"\",FindIndex($D30,$E30,$G30,$I30,AA$17))","v":""},{"$f":"IF(AND(K30=\"\",$D30=\"\"),\"\",FindIndex($D30,$E30,$G30,$I30,AB$17))","v":""},{"$f":"IF(AND(K30=\"\",$D30=\"\"),\"\",FindIndex($D30,$E30,$G30,$I30,AC$17))","v":""},{"$f":"IF(AND(K30=\"\",$D30=\"\"),\"\",FindIndex($D30,$E30,$G30,$I30,AD$17))","v":""},{"$f":"IF($U30=\"\",\"\",usage($C30,$E30,$V30,$H30,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U30=\"\",\"\",usage($C30,$E30,$W30,$J30,EFLCH,EFLHH,$AH$19)+ IF($X30=\"\",0,usage($C30,$E30,$X30,$L30,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF($U30=\"\",\"\",usage($C30,$E30,$G30,$H30,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U30=\"\",\"\",usage($C30,$E30,$I30,$J30,EFLCH,EFLHH,$AH$19)+ IF($K30=\"\",0,usage($C30,$E30,$K30,$L30,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF(AG30=\"\",\"\",AG30*DperKW*12+AH30*DperKWH)","v":""},{"$f":"IF(AH30=\"\",\"\",rebate(C30,D30,E30,G30,I30,K30,U30,AE30-AG30,AF30-AH30,Y30,Z30,AA30,AB30,AC30,AD30))","v":""},null,1,null,"PTAC (Retrofit)","PTAC105",8001,10501,0,null,null,null,null,null,{"$f":"AX26","v":11.4}]
[null,4,null,null,null,{"$f":"IF($D31=\"\",\"\",FindIndex($D31,$E31,$G31,$I31,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D31=\"\",\"\",FindIndex($D31,$E31,$G31,$I31,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D31=\"\",\"\",FindIndex($D31,$E31,$G31,$I31,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D31=\"\",\"\",FindIndex($D31,$E31,$G31,$I31,K$18 &\" Units\"))","v":""},null,null,null,null,null,null,null,4,{"$f":"IF($D31=\"\",\"\",FindIndex($D31,$E31,$G31,$I31,T$17))","v":""},{"$f":"IF(AND(E31=\"\",$D31=\"\"),\"\",FindIndex($D31,$E31,$G31,$I31,V$17))","v":""},{"$f":"IF(AND(E31=\"\",$D31=\"\"),\"\",FindIndex($D31,$E31,$G31,$I31,W$17))","v":""},{"$f":"IF(AND(E31=\"\",$D31=\"\"),\"\",FindIndex($D31,$E31,$G31,$I31,X$17))","v":""},{"$f":"IF(AND(H31=\"\",$D31=\"\"),\"\",FindIndex($D31,$E31,$G31,$I31,Y$17))","v":""},{"$f":"IF(AND(H31=\"\",$D31=\"\"),\"\",FindIndex($D31,$E31,$G31,$I31,Z$17))","v":""},{"$f":"IF(AND(H31=\"\",$D31=\"\"),\"\",FindIndex($D31,$E31,$G31,$I31,AA$17))","v":""},{"$f":"IF(AND(K31=\"\",$D31=\"\"),\"\",FindIndex($D31,$E31,$G31,$I31,AB$17))","v":""},{"$f":"IF(AND(K31=\"\",$D31=\"\"),\"\",FindIndex($D31,$E31,$G31,$I31,AC$17))","v":""},{"$f":"IF(AND(K31=\"\",$D31=\"\"),\"\",FindIndex($D31,$E31,$G31,$I31,AD$17))","v":""},{"$f":"IF($U31=\"\",\"\",usage($C31,$E31,$V31,$H31,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U31=\"\",\"\",usage($C31,$E31,$W31,$J31,EFLCH,EFLHH,$AH$19)+ IF($X31=\"\",0,usage($C31,$E31,$X31,$L31,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF($U31=\"\",\"\",usage($C31,$E31,$G31,$H31,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U31=\"\",\"\",usage($C31,$E31,$I31,$J31,EFLCH,EFLHH,$AH$19)+ IF($K31=\"\",0,usage($C31,$E31,$K31,$L31,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF(AG31=\"\",\"\",AG31*DperKW*12+AH31*DperKWH)","v":""},{"$f":"IF(AH31=\"\",\"\",rebate(C31,D31,E31,G31,I31,K31,U31,AE31-AG31,AF31-AH31,Y31,Z31,AA31,AB31,AC31,AD31))","v":""},null,1,null,"PTAC (Retrofit)","PTAC135",10501,13501,0,null,null,null,null,null,{"$f":"AX27","v":10.7}]
[null,5,null,null,null,{"$f":"IF($D32=\"\",\"\",FindIndex($D32,$E32,$G32,$I32,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D32=\"\",\"\",FindIndex($D32,$E32,$G32,$I32,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D32=\"\",\"\",FindIndex($D32,$E32,$G32,$I32,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D32=\"\",\"\",FindIndex($D32,$E32,$G32,$I32,K$18 &\" Units\"))","v":""},null,null,null,null,null,null,null,5,{"$f":"IF($D32=\"\",\"\",FindIndex($D32,$E32,$G32,$I32,T$17))","v":""},{"$f":"IF(AND(E32=\"\",$D32=\"\"),\"\",FindIndex($D32,$E32,$G32,$I32,V$17))","v":""},{"$f":"IF(AND(E32=\"\",$D32=\"\"),\"\",FindIndex($D32,$E32,$G32,$I32,W$17))","v":""},{"$f":"IF(AND(E32=\"\",$D32=\"\"),\"\",FindIndex($D32,$E32,$G32,$I32,X$17))","v":""},{"$f":"IF(AND(H32=\"\",$D32=\"\"),\"\",FindIndex($D32,$E32,$G32,$I32,Y$17))","v":""},{"$f":"IF(AND(H32=\"\",$D32=\"\"),\"\",FindIndex($D32,$E32,$G32,$I32,Z$17))","v":""},{"$f":"IF(AND(H32=\"\",$D32=\"\"),\"\",FindIndex($D32,$E32,$G32,$I32,AA$17))","v":""},{"$f":"IF(AND(K32=\"\",$D32=\"\"),\"\",FindIndex($D32,$E32,$G32,$I32,AB$17))","v":""},{"$f":"IF(AND(K32=\"\",$D32=\"\"),\"\",FindIndex($D32,$E32,$G32,$I32,AC$17))","v":""},{"$f":"IF(AND(K32=\"\",$D32=\"\"),\"\",FindIndex($D32,$E32,$G32,$I32,AD$17))","v":""},{"$f":"IF($U32=\"\",\"\",usage($C32,$E32,$V32,$H32,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U32=\"\",\"\",usage($C32,$E32,$W32,$J32,EFLCH,EFLHH,$AH$19)+ IF($X32=\"\",0,usage($C32,$E32,$X32,$L32,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF($U32=\"\",\"\",usage($C32,$E32,$G32,$H32,EFLCH,EFLHH,$AG$19))","v":""},{"$f":"IF($U32=\"\",\"\",usage($C32,$E32,$I32,$J32,EFLCH,EFLHH,$AH$19)+ IF($K32=\"\",0,usage($C32,$E32,$K32,$L32,EFLCH,EFLHH,$AH$19)))","v":""},{"$f":"IF(AG32=\"\",\"\",AG32*DperKW*12+AH32*DperKWH)","v":""},{"$f":"IF(AH32=\"\",\"\",rebate(C32,D32,E32,G32,I32,K32,U32,AE32-AG32,AF32-AH32,Y32,Z32,AA32,AB32,AC32,AD32))","v":""},null,1,null,"PTAC (Retrofit)","PTACL",13501,1000000,0,null,null,null,null,null,{"$f":"AX28","v":10}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AE28:AE32)","v":0},{"$f":"SUM(AF28:AF32)","v":0},{"$f":"SUM(AG28:AG32)","v":0},{"$f":"SUM(AH28:AH32)","v":0},0,{"$f":"SUM(AJ28:AJ32)","v":0},null,1,null,"PTHP (New Construction)","PTHP80",0,8001,0,null,0,null,null,null,11.8,null,3.3]
[null,"Hi Eff Option (Required)",null,null,null,null,null,null,null,null,null,null,null,"Office Use Only",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"PTHP (New Construction)","PTHP105",8001,10501,0,null,0,null,null,null,11.4,null,3.2]
[null,null,null,null,null,null,null,"Project Cost",null,null,null,null,null,"Equipment Code","QTY","kW Savings","kWh Savings","Rebate",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AE36:AE40)","v":0},0,0,0,0,0,null,1,null,"PTHP (New Construction)","PTHP135",10501,13501,0,null,0,null,null,null,10.7,null,3.1]
[null,1,null,null,null,{"$f":"IF($D36=\"\",\"\",FindIndex($D36,$E36,$G36,$I36,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D36=\"\",\"\",FindIndex($D36,$E36,$G36,$I36,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D36=\"\",\"\",FindIndex($D36,$E36,$G36,$I36,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D36=\"\",\"\",FindIndex($D36,$E36,$G36,$I36,K$18 &\" Units\"))","v":""},null,{"$f":"U36","v":""},{"$f":"IF(N36=\"\",\"\",C36)","v":""},{"$f":" IF(O36=\"\", \"\", IF(OR(AND(H36<>\"\",G36 = \"\"),AND(J36<>\"\", I36 = \"\"),AND(K36=\"\",L36<>\"\")), \"Enter efficiency\", AE36-AG36))","v":""},{"$f":" IF(O36=\"\", \"\", IF(OR(AND(H36<>\"\",G36 = \"\"),AND(J36<>\"\", I36 = \"\"),AND(K36=\"\",L36<>\"\")), \"Enter efficiency\", AF36-AH36))","v":""},{"$f":"IF(Q36=\"\",\"\",IF(N36=\"NO CODE\", \"Not in catalogue\",IF(Q36=\"Enter efficiency\",\"Enter efficiency\",IF(N36=\"NO CODE\", \"Not in catalogue\",AJ36))))","v":""},null,1,{"$f":"IF($D36=\"\",\"\",FindIndex($D36,$E36,$G36,$I36,T$17))","v":""},{"$f":"IF(AND(E36=\"\",$D36=\"\"),\"\",FindIndex($D36,$E36,$G36,$I36,V$17))","v":""},{"$f":"IF(AND(E36=\"\",$D36=\"\"),\"\",FindIndex($D36,$E36,$G36,$I36,W$17))","v":""},{"$f":"IF(AND(E36=\"\",$D36=\"\"),\"\",FindIndex($D36,$E36,$G36,$I36,X$17))","v":""},{"$f":"IF(AND(H36=\"\",$D36=\"\"),\"\",FindIndex($D36,$E36,$G36,$I36,Y$17))","v":""},{"$f":"IF(AND(H36=\"\",$D36=\"\"),\"\",FindIndex($D36,$E36,$G36,$I36,Z$17))","v":""},{"$f":"IF(AND(H36=\"\",$D36=\"\"),\"\",FindIndex($D36,$E36,$G36,$I36,AA$17))","v":""},{"$f":"IF(AND(K36=\"\",$D36=\"\"),\"\",FindIndex($D36,$E36,$G36,$I36,AB$17))","v":""},{"$f":"IF(AND(K36=\"\",$D36=\"\"),\"\",FindIndex($D36,$E36,$G36,$I36,AC$17))","v":""},{"$f":"IF(AND(K36=\"\",$D36=\"\"),\"\",FindIndex($D36,$E36,$G36,$I36,AD$17))","v":""},{"$f":"IF($J36=\"SEER\",IF($U36=\"\",\"\",usage($C36,$E36,$W36,\"EER\",EFLCH,EFLHH,$AG$19)),IF($U36=\"\",\"\",usage($C36,$E36,$V36,$H36,EFLCH,EFLHH,$AG$19)))","v":""},{"$f":"IF(OR(D36=$AJ$55,D36=$AJ$56,D36=$AJ$57,D36=$AJ$58),IF($U36=\"\",\"\",usage($C36,$E36,$W36,\"IEER\",EFLCH,EFLHH,$AH$19)+ IF($X36=\"\",0,usage($C36,$E36,$X36,$L36,EFLCH,EFLHH,$AH$19))),IF($U36=\"\",\"\",usage($C36,$E36,$W36,$J36,EFLCH,EFLHH,$AH$19)+ IF($X36=\"\",0,usage($C36,$E36,$X36,$L36,EFLCH,EFLHH,$AH$19))))","v":""},{"$f":"IF(J36=\"SEER\",IF($U36=\"\",\"\",usage($C36,$E36,$I36,\"EER\",EFLCH,EFLHH,$AG$19)),IF($U36=\"\",\"\",usage($C36,$E36,$G36,$H36,EFLCH,EFLHH,$AG$19)))","v":""},{"$f":"IF(OR(D36=$AJ$55,D36=$AJ$56,D36=$AJ$57,D36=$AJ$58),IF($U36=\"\",\"\",usage($C36,$E36,$G36,\"IEER\",EFLCH,EFLHH,$AH$19)+ IF($K36=\"\",0,usage($C36,$E36,$K36,$L36,EFLCH,EFLHH,$AH$19))),IF($U36=\"\",\"\",usage($C36,$E36,$I36,$J36,EFLCH,EFLHH,$AH$19)+ IF($K36=\"\",0,usage($C36,$E36,$K36,$L36,EFLCH,EFLHH,$AH$19))))","v":""},{"$f":"IF(AG36=\"\",\"\",AG36*DperKW*12+AH36*DperKWH)","v":""},{"$f":"IF(AH36=\"\",\"\",rebate(C36,D36,E36,G36,I36,K36,U36,AE36-AG36,AF36-AH36,Y36,Z36,AA36,AB36,AC36,AD36))","v":""},null,1,null,"PTHP (New Construction)","PTHPL",13501,1000000,0,null,0,null,null,null,10,null,3]
[null,2,null,null,null,{"$f":"IF($D37=\"\",\"\",FindIndex($D37,$E37,$G37,$I37,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D37=\"\",\"\",FindIndex($D37,$E37,$G37,$I37,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D37=\"\",\"\",FindIndex($D37,$E37,$G37,$I37,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D37=\"\",\"\",FindIndex($D37,$E37,$G37,$I37,K$18 &\" Units\"))","v":""},null,{"$f":"U37","v":""},{"$f":"IF(N37=\"\",\"\",C37)","v":""},{"$f":" IF(O37=\"\", \"\", IF(OR(AND(H37<>\"\",G37 = \"\"),AND(J37<>\"\", I37 = \"\"),AND(K37=\"\",L37<>\"\")), \"Enter efficiency\", AE37-AG37))","v":""},{"$f":" IF(O37=\"\", \"\", IF(OR(AND(H37<>\"\",G37 = \"\"),AND(J37<>\"\", I37 = \"\"),AND(K37=\"\",L37<>\"\")), \"Enter efficiency\", AF37-AH37))","v":""},{"$f":"IF(Q37=\"\",\"\",IF(N37=\"NO CODE\", \"Not in catalogue\",IF(Q37=\"Enter efficiency\",\"Enter efficiency\",IF(N37=\"NO CODE\", \"Not in catalogue\",AJ37))))","v":""},null,2,{"$f":"IF($D37=\"\",\"\",FindIndex($D37,$E37,$G37,$I37,T$17))","v":""},{"$f":"IF(AND(E37=\"\",$D37=\"\"),\"\",FindIndex($D37,$E37,$G37,$I37,V$17))","v":""},{"$f":"IF(AND(E37=\"\",$D37=\"\"),\"\",FindIndex($D37,$E37,$G37,$I37,W$17))","v":""},{"$f":"IF(AND(E37=\"\",$D37=\"\"),\"\",FindIndex($D37,$E37,$G37,$I37,X$17))","v":""},{"$f":"IF(AND(H37=\"\",$D37=\"\"),\"\",FindIndex($D37,$E37,$G37,$I37,Y$17))","v":""},{"$f":"IF(AND(H37=\"\",$D37=\"\"),\"\",FindIndex($D37,$E37,$G37,$I37,Z$17))","v":""},{"$f":"IF(AND(H37=\"\",$D37=\"\"),\"\",FindIndex($D37,$E37,$G37,$I37,AA$17))","v":""},{"$f":"IF(AND(K37=\"\",$D37=\"\"),\"\",FindIndex($D37,$E37,$G37,$I37,AB$17))","v":""},{"$f":"IF(AND(K37=\"\",$D37=\"\"),\"\",FindIndex($D37,$E37,$G37,$I37,AC$17))","v":""},{"$f":"IF(AND(K37=\"\",$D37=\"\"),\"\",FindIndex($D37,$E37,$G37,$I37,AD$17))","v":""},{"$f":"IF($J37=\"SEER\",IF($U37=\"\",\"\",usage($C37,$E37,$W37,\"EER\",EFLCH,EFLHH,$AG$19)),IF($U37=\"\",\"\",usage($C37,$E37,$V37,$H37,EFLCH,EFLHH,$AG$19)))","v":""},{"$f":"IF(OR(D37=$AJ$55,D37=$AJ$56,D37=$AJ$57,D37=$AJ$58),IF($U37=\"\",\"\",usage($C37,$E37,$W37,\"IEER\",EFLCH,EFLHH,$AH$19)+ IF($X37=\"\",0,usage($C37,$E37,$X37,$L37,EFLCH,EFLHH,$AH$19))),IF($U37=\"\",\"\",usage($C37,$E37,$W37,$J37,EFLCH,EFLHH,$AH$19)+ IF($X37=\"\",0,usage($C37,$E37,$X37,$L37,EFLCH,EFLHH,$AH$19))))","v":""},{"$f":"IF(J37=\"SEER\",IF($U37=\"\",\"\",usage($C37,$E37,$I37,\"EER\",EFLCH,EFLHH,$AG$19)),IF($U37=\"\",\"\",usage($C37,$E37,$G37,$H37,EFLCH,EFLHH,$AG$19)))","v":""},{"$f":"IF(OR(D37=$AJ$55,D37=$AJ$56,D37=$AJ$57,D37=$AJ$58),IF($U37=\"\",\"\",usage($C37,$E37,$G37,\"IEER\",EFLCH,EFLHH,$AH$19)+ IF($K37=\"\",0,usage($C37,$E37,$K37,$L37,EFLCH,EFLHH,$AH$19))),IF($U37=\"\",\"\",usage($C37,$E37,$I37,$J37,EFLCH,EFLHH,$AH$19)+ IF($K37=\"\",0,usage($C37,$E37,$K37,$L37,EFLCH,EFLHH,$AH$19))))","v":""},{"$f":"IF(AG37=\"\",\"\",AG37*DperKW*12+AH37*DperKWH)","v":""},{"$f":"IF(AH37=\"\",\"\",rebate(C37,D37,E37,G37,I37,K37,U37,AE37-AG37,AF37-AH37,Y37,Z37,AA37,AB37,AC37,AD37))","v":""},null,1,null,"PTHP (Retrofit)","PTHP80",0,8001,0,null,0,null,null,null,{"$f":"AX33","v":11.8},null,{"$f":"AZ33","v":3.3}]
[null,3,null,null,null,{"$f":"IF($D38=\"\",\"\",FindIndex($D38,$E38,$G38,$I38,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D38=\"\",\"\",FindIndex($D38,$E38,$G38,$I38,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D38=\"\",\"\",FindIndex($D38,$E38,$G38,$I38,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D38=\"\",\"\",FindIndex($D38,$E38,$G38,$I38,K$18 &\" Units\"))","v":""},null,"","","","","",null,3,{"$f":"IF($D38=\"\",\"\",FindIndex($D38,$E38,$G38,$I38,T$17))","v":""},{"$f":"IF(AND(E38=\"\",$D38=\"\"),\"\",FindIndex($D38,$E38,$G38,$I38,V$17))","v":""},{"$f":"IF(AND(E38=\"\",$D38=\"\"),\"\",FindIndex($D38,$E38,$G38,$I38,W$17))","v":""},{"$f":"IF(AND(E38=\"\",$D38=\"\"),\"\",FindIndex($D38,$E38,$G38,$I38,X$17))","v":""},{"$f":"IF(AND(H38=\"\",$D38=\"\"),\"\",FindIndex($D38,$E38,$G38,$I38,Y$17))","v":""},{"$f":"IF(AND(H38=\"\",$D38=\"\"),\"\",FindIndex($D38,$E38,$G38,$I38,Z$17))","v":""},{"$f":"IF(AND(H38=\"\",$D38=\"\"),\"\",FindIndex($D38,$E38,$G38,$I38,AA$17))","v":""},{"$f":"IF(AND(K38=\"\",$D38=\"\"),\"\",FindIndex($D38,$E38,$G38,$I38,AB$17))","v":""},{"$f":"IF(AND(K38=\"\",$D38=\"\"),\"\",FindIndex($D38,$E38,$G38,$I38,AC$17))","v":""},{"$f":"IF(AND(K38=\"\",$D38=\"\"),\"\",FindIndex($D38,$E38,$G38,$I38,AD$17))","v":""},{"$f":"IF($J38=\"SEER\",IF($U38=\"\",\"\",usage($C38,$E38,$W38,\"EER\",EFLCH,EFLHH,$AG$19)),IF($U38=\"\",\"\",usage($C38,$E38,$V38,$H38,EFLCH,EFLHH,$AG$19)))","v":""},{"$f":"IF(OR(D38=$AJ$55,D38=$AJ$56,D38=$AJ$57,D38=$AJ$58),IF($U38=\"\",\"\",usage($C38,$E38,$W38,\"IEER\",EFLCH,EFLHH,$AH$19)+ IF($X38=\"\",0,usage($C38,$E38,$X38,$L38,EFLCH,EFLHH,$AH$19))),IF($U38=\"\",\"\",usage($C38,$E38,$W38,$J38,EFLCH,EFLHH,$AH$19)+ IF($X38=\"\",0,usage($C38,$E38,$X38,$L38,EFLCH,EFLHH,$AH$19))))","v":""},{"$f":"IF(J38=\"SEER\",IF($U38=\"\",\"\",usage($C38,$E38,$I38,\"EER\",EFLCH,EFLHH,$AG$19)),IF($U38=\"\",\"\",usage($C38,$E38,$G38,$H38,EFLCH,EFLHH,$AG$19)))","v":""},{"$f":"IF(OR(D38=$AJ$55,D38=$AJ$56,D38=$AJ$57,D38=$AJ$58),IF($U38=\"\",\"\",usage($C38,$E38,$G38,\"IEER\",EFLCH,EFLHH,$AH$19)+ IF($K38=\"\",0,usage($C38,$E38,$K38,$L38,EFLCH,EFLHH,$AH$19))),IF($U38=\"\",\"\",usage($C38,$E38,$I38,$J38,EFLCH,EFLHH,$AH$19)+ IF($K38=\"\",0,usage($C38,$E38,$K38,$L38,EFLCH,EFLHH,$AH$19))))","v":""},{"$f":"IF(AG38=\"\",\"\",AG38*DperKW*12+AH38*DperKWH)","v":""},{"$f":"IF(AH38=\"\",\"\",rebate(C38,D38,E38,G38,I38,K38,U38,AE38-AG38,AF38-AH38,Y38,Z38,AA38,AB38,AC38,AD38))","v":""},null,1,null,"PTHP (Retrofit)","PTHP105",8001,10501,0,null,0,null,null,null,{"$f":"AX34","v":11.4},null,{"$f":"AZ34","v":3.2}]
[null,4,null,null,null,{"$f":"IF($D39=\"\",\"\",FindIndex($D39,$E39,$G39,$I39,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D39=\"\",\"\",FindIndex($D39,$E39,$G39,$I39,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D39=\"\",\"\",FindIndex($D39,$E39,$G39,$I39,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D39=\"\",\"\",FindIndex($D39,$E39,$G39,$I39,K$18 &\" Units\"))","v":""},null,"","","","","",null,4,{"$f":"IF($D39=\"\",\"\",FindIndex($D39,$E39,$G39,$I39,T$17))","v":""},{"$f":"IF(AND(E39=\"\",$D39=\"\"),\"\",FindIndex($D39,$E39,$G39,$I39,V$17))","v":""},{"$f":"IF(AND(E39=\"\",$D39=\"\"),\"\",FindIndex($D39,$E39,$G39,$I39,W$17))","v":""},{"$f":"IF(AND(E39=\"\",$D39=\"\"),\"\",FindIndex($D39,$E39,$G39,$I39,X$17))","v":""},{"$f":"IF(AND(H39=\"\",$D39=\"\"),\"\",FindIndex($D39,$E39,$G39,$I39,Y$17))","v":""},{"$f":"IF(AND(H39=\"\",$D39=\"\"),\"\",FindIndex($D39,$E39,$G39,$I39,Z$17))","v":""},{"$f":"IF(AND(H39=\"\",$D39=\"\"),\"\",FindIndex($D39,$E39,$G39,$I39,AA$17))","v":""},{"$f":"IF(AND(K39=\"\",$D39=\"\"),\"\",FindIndex($D39,$E39,$G39,$I39,AB$17))","v":""},{"$f":"IF(AND(K39=\"\",$D39=\"\"),\"\",FindIndex($D39,$E39,$G39,$I39,AC$17))","v":""},{"$f":"IF(AND(K39=\"\",$D39=\"\"),\"\",FindIndex($D39,$E39,$G39,$I39,AD$17))","v":""},{"$f":"IF($J39=\"SEER\",IF($U39=\"\",\"\",usage($C39,$E39,$W39,\"EER\",EFLCH,EFLHH,$AG$19)),IF($U39=\"\",\"\",usage($C39,$E39,$V39,$H39,EFLCH,EFLHH,$AG$19)))","v":""},{"$f":"IF(OR(D39=$AJ$55,D39=$AJ$56,D39=$AJ$57,D39=$AJ$58),IF($U39=\"\",\"\",usage($C39,$E39,$W39,\"IEER\",EFLCH,EFLHH,$AH$19)+ IF($X39=\"\",0,usage($C39,$E39,$X39,$L39,EFLCH,EFLHH,$AH$19))),IF($U39=\"\",\"\",usage($C39,$E39,$W39,$J39,EFLCH,EFLHH,$AH$19)+ IF($X39=\"\",0,usage($C39,$E39,$X39,$L39,EFLCH,EFLHH,$AH$19))))","v":""},{"$f":"IF(J39=\"SEER\",IF($U39=\"\",\"\",usage($C39,$E39,$I39,\"EER\",EFLCH,EFLHH,$AG$19)),IF($U39=\"\",\"\",usage($C39,$E39,$G39,$H39,EFLCH,EFLHH,$AG$19)))","v":""},{"$f":"IF(OR(D39=$AJ$55,D39=$AJ$56,D39=$AJ$57,D39=$AJ$58),IF($U39=\"\",\"\",usage($C39,$E39,$G39,\"IEER\",EFLCH,EFLHH,$AH$19)+ IF($K39=\"\",0,usage($C39,$E39,$K39,$L39,EFLCH,EFLHH,$AH$19))),IF($U39=\"\",\"\",usage($C39,$E39,$I39,$J39,EFLCH,EFLHH,$AH$19)+ IF($K39=\"\",0,usage($C39,$E39,$K39,$L39,EFLCH,EFLHH,$AH$19))))","v":""},{"$f":"IF(AG39=\"\",\"\",AG39*DperKW*12+AH39*DperKWH)","v":""},{"$f":"IF(AH39=\"\",\"\",rebate(C39,D39,E39,G39,I39,K39,U39,AE39-AG39,AF39-AH39,Y39,Z39,AA39,AB39,AC39,AD39))","v":""},null,1,null,"PTHP (Retrofit)","PTHP135",10501,13501,0,null,0,null,null,null,{"$f":"AX35","v":10.7},null,{"$f":"AZ35","v":3.1}]
[null,5,null,null,null,{"$f":"IF($D40=\"\",\"\",FindIndex($D40,$E40,$G40,$I40,E$19 &\" Units\"))","v":""},null,{"$f":"IF($D40=\"\",\"\",FindIndex($D40,$E40,$G40,$I40,G$18 &\" Units\"))","v":""},null,{"$f":"IF($D40=\"\",\"\",FindIndex($D40,$E40,$G40,$I40,I$18 &\" Units\"))","v":""},null,{"$f":"IF($D40=\"\",\"\",FindIndex($D40,$E40,$G40,$I40,K$18 &\" Units\"))","v":""},null,"","","","","",null,5,{"$f":"IF($D40=\"\",\"\",FindIndex($D40,$E40,$G40,$I40,T$17))","v":""},{"$f":"IF(AND(E40=\"\",$D40=\"\"),\"\",FindIndex($D40,$E40,$G40,$I40,V$17))","v":""},{"$f":"IF(AND(E40=\"\",$D40=\"\"),\"\",FindIndex($D40,$E40,$G40,$I40,W$17))","v":""},{"$f":"IF(AND(E40=\"\",$D40=\"\"),\"\",FindIndex($D40,$E40,$G40,$I40,X$17))","v":""},{"$f":"IF(AND(H40=\"\",$D40=\"\"),\"\",FindIndex($D40,$E40,$G40,$I40,Y$17))","v":""},{"$f":"IF(AND(H40=\"\",$D40=\"\"),\"\",FindIndex($D40,$E40,$G40,$I40,Z$17))","v":""},{"$f":"IF(AND(H40=\"\",$D40=\"\"),\"\",FindIndex($D40,$E40,$G40,$I40,AA$17))","v":""},{"$f":"IF(AND(K40=\"\",$D40=\"\"),\"\",FindIndex($D40,$E40,$G40,$I40,AB$17))","v":""},{"$f":"IF(AND(K40=\"\",$D40=\"\"),\"\",FindIndex($D40,$E40,$G40,$I40,AC$17))","v":""},{"$f":"IF(AND(K40=\"\",$D40=\"\"),\"\",FindIndex($D40,$E40,$G40,$I40,AD$17))","v":""},{"$f":"IF($J40=\"SEER\",IF($U40=\"\",\"\",usage($C40,$E40,$W40,\"EER\",EFLCH,EFLHH,$AG$19)),IF($U40=\"\",\"\",usage($C40,$E40,$V40,$H40,EFLCH,EFLHH,$AG$19)))","v":""},{"$f":"IF(OR(D40=$AJ$55,D40=$AJ$56,D40=$AJ$57,D40=$AJ$58),IF($U40=\"\",\"\",usage($C40,$E40,$W40,\"IEER\",EFLCH,EFLHH,$AH$19)+ IF($X40=\"\",0,usage($C40,$E40,$X40,$L40,EFLCH,EFLHH,$AH$19))),IF($U40=\"\",\"\",usage($C40,$E40,$W40,$J40,EFLCH,EFLHH,$AH$19)+ IF($X40=\"\",0,usage($C40,$E40,$X40,$L40,EFLCH,EFLHH,$AH$19))))","v":""},{"$f":"IF(J40=\"SEER\",IF($U40=\"\",\"\",usage($C40,$E40,$I40,\"EER\",EFLCH,EFLHH,$AG$19)),IF($U40=\"\",\"\",usage($C40,$E40,$G40,$H40,EFLCH,EFLHH,$AG$19)))","v":""},{"$f":"IF(OR(D40=$AJ$55,D40=$AJ$56,D40=$AJ$57,D40=$AJ$58),IF($U40=\"\",\"\",usage($C40,$E40,$G40,\"IEER\",EFLCH,EFLHH,$AH$19)+ IF($K40=\"\",0,usage($C40,$E40,$K40,$L40,EFLCH,EFLHH,$AH$19))),IF($U40=\"\",\"\",usage($C40,$E40,$I40,$J40,EFLCH,EFLHH,$AH$19)+ IF($K40=\"\",0,usage($C40,$E40,$K40,$L40,EFLCH,EFLHH,$AH$19))))","v":""},{"$f":"IF(AG40=\"\",\"\",AG40*DperKW*12+AH40*DperKWH)","v":""},{"$f":"IF(AH40=\"\",\"\",rebate(C40,D40,E40,G40,I40,K40,U40,AE40-AG40,AF40-AH40,Y40,Z40,AA40,AB40,AC40,AD40))","v":""},null,1,null,"PTHP (Retrofit)","PTHPL",13501,1000000,0,null,0,null,null,null,{"$f":"AX36","v":10},null,{"$f":"AZ36","v":3}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,">= 65,000 BTU/HR HP and AC",null,null,"BTUh",null,"EER","IEER","COP",null,null,null,"EER","IEER","COP","EER","IEER","COP"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(SEER2/HSPF2) 3 Phase Heat Pump Single Package",null,1,null,"3 Phase Unitary AC Single Package","AC3SP135",{"$f":"AQ14","v":65000},135000,11.2,11.4,null,null,null,null,{"$f":"AR42","v":11.2},{"$f":"AS42","v":11.4}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(SEER2/HSPF2) 3 Phase Heat Pump Split System",null,1,null,"3 Phase Unitary AC Single Package","AC3SP240",{"$f":"AQ42","v":135000},240000,11,11.2,null,null,null,null,{"$f":"AR43","v":11},{"$f":"AS43","v":11.2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(SEER2) 3 Phase Unitary AC Single Package",null,1,null,"3 Phase Unitary AC Single Package","AC3SP760",{"$f":"AQ43","v":240000},760000,10,10.1,null,null,null,null,10,10.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(SEER2) 3 Phase Unitary AC Split System",null,1,null,"3 Phase Unitary AC Single Package","AC3SPL",{"$f":"AQ44","v":760000},1000000,9.6999999999999993,9.8000000000000007,null,null,null,null,9.6999999999999993,9.8000000000000007]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(SEER2) VRF/Mini-Split AC",null,1,null,"3 Phase Unitary AC Split System","AC3SS135",{"$f":"AQ14","v":65000},135000,11.2,11.4,null,null,null,null,11.2,11.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(SEER2/HSPF2) VRF/Mini-Split HP",null,1,null,"3 Phase Unitary AC Split System","AC3SS240",{"$f":"AQ46","v":135000},240000,11,11.2,null,null,null,null,11,11.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 Phase Heat Pump Single Package",null,1,null,"3 Phase Unitary AC Split System","AC3SS760",{"$f":"AQ47","v":240000},760000,10,10.1,null,null,null,null,10,10.1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 Phase Heat Pump Split System",null,1,null,"3 Phase Unitary AC Split System","AC3SSL",{"$f":"AQ48","v":760000},1000000,9.6999999999999993,9.8000000000000007,null,null,null,null,9.6999999999999993,9.8000000000000007]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 Phase Unitary AC Single Package",null,1,null,"3 Phase Heat Pump Single Package","HP3SP135",65000,135000,11,11.2,3.3,null,null,null,{"$f":"AR50","v":11},11.2,3.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3 Phase Unitary AC Split System",null,1,null,"3 Phase Heat Pump Single Package","HP3SP170",135000,170000,10.6,10.7,3.2,null,null,null,10.6,10.7,3.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VRF/Mini-Split AC",null,1,null,"3 Phase Heat Pump Single Package","HP3SP240",{"$f":"AQ51","v":170000},240000,10.6,10.7,3.2,null,null,null,10.6,10.7,3.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VRF/Mini-Split HP",null,1,null,"3 Phase Heat Pump Single Package","HP3SPL",{"$f":"AQ52","v":240000},1000000,9.5,9.6,3.2,null,null,null,9.5,9.6,3.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VRF/Mini-Split HP W/ Heat Recovery",null,1,null,"3 Phase Heat Pump Split System","HP3SS135",{"$f":"AQ12","v":65000},135000,11,11.2,3.3,null,null,null,11,11.2,3.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PTAC (New Construction)",null,1,null,"3 Phase Heat Pump Split System","HP3SS170",{"$f":"AQ54","v":135000},170000,10.6,10.7,3.2,null,null,null,10.6,10.7,3.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PTAC (Retrofit)",null,1,null,"3 Phase Heat Pump Split System","HP3SS240",{"$f":"AQ55","v":170000},240000,10.6,10.7,3.2,null,null,null,10.6,10.7,3.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PTHP (New Construction)",null,1,null,"3 Phase Heat Pump Split System","HP3SSL",{"$f":"AQ56","v":240000},1000000,9.5,9.6,3.2,null,null,null,9.5,9.6,3.2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PTHP (Retrofit)",null,1,null,"VRF/Mini-Split AC","ACVRF135",65000,135000,11.2,13.1,null,null,null,null,11.3,15.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1 Phase Heat Pump Single Package",null,1,null,"VRF/Mini-Split AC","ACVRF240",135000,240000,11,12.9,null,null,null,null,11.1,15.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1 Phase Heat Pump Split System",null,1,null,"VRF/Mini-Split AC","ACVRFL",240000,1000000,10,11.6,null,null,null,null,10.3,13.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Air Cooled Chiller w/ Condenser",null,1,null,"VRF/Mini-Split HP","HPVRF135",65000,135000,11,12.9,3.3,null,null,null,11.1,15.9,3.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Air Cooled Chiller w/o Condenser",null,1,null,"VRF/Mini-Split HP","HPVRF240",135000,240000,10.6,12.3,3.2,null,null,null,10.7,15.4,3.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Water Cooled Chiller Non-Centrifugal",null,1,null,"VRF/Mini-Split HP W/ Heat Recovery","HPVRF240R",135000,240000,10.4,12.1,3.2,null,null,null,10.5,16.3,3.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Water Cooled Chiller Reciprocating",null,1,null,"VRF/Mini-Split HP","HPVRFL",240000,1000000,9.5,11,3.2,null,null,null,10.3,13.3,3.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Water Cooled Chiller Centrifugal",null,1,null,"VRF/Mini-Split HP W/ Heat Recovery","HPVRFLR",240000,1000000,9.3000000000000007,10.8,3.2,null,null,null,10.3,13.3,3.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Water Chilling Packages",null,null,"Tons",null,"kW/Ton","kW/Ton",null,"kW/Ton","kW/Ton",null,"kW/Ton","kW/Ton",null,"kW/Ton","kW/Ton"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Air Cooled Chiller w/ Condenser","ACCC150",0,150,1.2549675800041833,0.96,null,null,null,null,1.2,0.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Air Cooled Chiller w/ Condenser","ACCCL",{"$f":"AQ67","v":150},1000000,1.2549675800041833,0.94117647058823528,null,null,null,null,1.2,0.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Air Cooled Chiller w/o Condenser","ACC150",0,150,1.2549675800041833,0.96,null,null,null,null,1.2,0.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Air Cooled Chiller w/o Condenser","ACCL",{"$f":"AQ69","v":150},1000000,1.2549675800041833,0.94117647058823528,null,null,null,null,1.2,0.9]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Water Cooled Chiller Non-Centrifugal","WCCRSS75",0,75,0.78,0.63,null,0.8,0.6,null,0.73,0.6,null,0.75,0.56999999999999995]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Water Cooled Chiller Non-Centrifugal","WCCRSS150",{"$f":"AQ71","v":75},150,0.77500000000000002,0.61499999999999999,null,0.79,0.58599999999999997,null,0.73,0.57999999999999996,null,0.75,0.55000000000000004]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Water Cooled Chiller Non-Centrifugal","WCCRSS300",{"$f":"AQ72","v":150},300,0.68,0.57999999999999996,null,0.71799999999999997,0.54,null,0.63,0.55000000000000004,null,0.67,0.51]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Water Cooled Chiller Non-Centrifugal","WCCRSSL",{"$f":"AQ73","v":300},1000000,0.62,0.54,null,0.63900000000000001,0.49,null,0.57999999999999996,0.51,null,0.6,0.46]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Water Cooled Chiller Reciprocating","WCCR75",0,75,0.78,0.63,null,{"$f":"AU71","v":0.8},{"$f":"AV71","v":0.6},null,{"$f":"AX71","v":0.73},{"$f":"AY71","v":0.6},null,{"$f":"BA71","v":0.75},0.56999999999999995]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Water Cooled Chiller Reciprocating","WCCR150",{"$f":"AQ75","v":75},150,0.77500000000000002,0.61499999999999999,null,{"$f":"AU72","v":0.79},0.58599999999999997,null,{"$f":"AX72","v":0.73},0.57999999999999996,null,0.75,0.55000000000000004]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Water Cooled Chiller Reciprocating","WCCR300",{"$f":"AQ76","v":150},300,0.68,0.57999999999999996,null,0.71799999999999997,0.54,null,0.63,0.55000000000000004,null,0.67,0.51]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Water Cooled Chiller Reciprocating","WCCRL",{"$f":"AQ77","v":300},1000000,0.62,0.54,null,0.63900000000000001,0.49,null,0.57999999999999996,0.51,null,0.6,0.46]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Water Cooled Chiller Centrifugal","WCCC150",0,150,0.63400000000000001,0.59599999999999997,null,0.63900000000000001,0.45,null,0.6,0.56000000000000005,null,0.61,0.42]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Water Cooled Chiller Centrifugal","WCCC300",{"$f":"AQ79","v":150},300,0.63400000000000001,0.59599999999999997,null,0.63900000000000001,0.45,null,0.6,0.56000000000000005,null,0.61,0.42]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Water Cooled Chiller Centrifugal","WCCC600",{"$f":"AQ80","v":300},600,0.57599999999999996,0.54900000000000004,null,0.6,0.4,null,0.54,0.52,null,0.56000000000000005,0.38]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"Water Cooled Chiller Centrifugal","WCCCL",{"$f":"AQ81","v":600},1000000,0.56999999999999995,0.53900000000000003,null,0.59,0.4,null,0.54,0.51,null,0.56000000000000005,0.38]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,"?",null,"?","?","?","?","?","?","?","?","?","?","?","?"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,"NO CODE","NO CODE"]

{"sheet":"Warning","index":6,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":false,"merged":[[0,0,0,2],[1,0,4,0]]}
["You must enable macros."]
["If you just opened this workbook, you must enable macros and re-open this file.",null,"If you just saved this workbook, click here to continue."]
[null,null,"Customer Information"]

{"sheet":"Appendix E (Ref. Table)","index":7,"n_rows":70,"n_cols":8,"rows_kept":70,"cut":false,"hidden":true,"merged":[]}
[null,null,null,null,null,null,null,"Reference"]
[null,null,"BTUh (>=)","BTUh (<)","EER","SEER","HSPF","Baseline Reference"]
["1 Phase Heat Pump Single Package","HP1SP65",0,65000,"Not in Code",14,8,"Code of Federal Regulations\nkW savings is calculated bsaed on SEER & EFLH"]
["1 Phase Heat Pump Split System","HP1SS65",0,65000,"Not in Code",14,8.1999999999999993,"Code of Federal Regulations\nkW savings is calculated bsaed on SEER & EFLH"]
["3 Phase Heat Pump Single Package","HP3SP65",0,65000,"Not in Code",13,7.7,"IECC 2012\nkW savings is calculated bsaed on SEER & EFLH"]
["3 Phase Heat Pump Split System","HP3SS65",0,65000,"Not in Code",13,7.7,"IECC 2012\nkW savings is calculated bsaed on SEER & EFLH"]
["3 Phase Unitary AC Single Package","AC3SP65",0,65000,"Not in Code",13,"NA","IECC 2012\nkW savings is calculated bsaed on SEER & EFLH"]
["3 Phase Unitary AC Split System","AC3SS65",0,65000,"Not in Code",13,"NA","IECC 2012\nkW savings is calculated bsaed on SEER & EFLH"]
["VRF/Mini-Split AC","ACVRF65",0,65000,"Not in Standard",13,"NA","ASHRAE 90.1-2010\nkW savings is calculated bsaed on SEER & EFLH"]
["VRF/Mini-Split HP","HPVRF65",0,65000,"Not in Standard",13,7.7,"ASHRAE 90.1-2010\nkW savings is calculated bsaed on SEER & EFLH"]
[null,null,"BTUh (>=)","BTUh (<)","EER","SEER","COP","Baseline Reference"]
["PTAC (New Construction)","PTAC80",0,8001,"12.5-0.213cap/1000","Not in Code","NA","IECC 2009\nkWh savings is calculated bsaed on EER & EFLH"]
["PTAC (New Construction)","PTAC105",8001,10501,"12.5-0.213cap/1000","Not in Code","NA","IECC 2009\nkWh savings is calculated bsaed on EER & EFLH"]
["PTAC (New Construction)","PTAC135",10501,13501,"12.5-0.213cap/1000","Not in Code","NA","IECC 2009\nkWh savings is calculated bsaed on EER & EFLH"]
["PTAC (New Construction)","PTACL",13501,1000000,"12.5-0.213cap/1000","Not in Code","NA","IECC 2009\nkWh savings is calculated bsaed on EER & EFLH"]
["PTAC (Retrofit)","PTAC80",0,8001,"10.9-0.213cap/1000","Not in Code","NA","IECC 2009\nkWh savings is calculated bsaed on EER & EFLH"]
["PTAC (Retrofit)","PTAC105",8001,10501,"10.9-0.213cap/1000","Not in Code","NA","IECC 2009\nkWh savings is calculated bsaed on EER & EFLH"]
["PTAC (Retrofit)","PTAC135",10501,13501,"10.9-0.213cap/1000","Not in Code","NA","IECC 2009\nkWh savings is calculated bsaed on EER & EFLH"]
["PTAC (Retrofit)","PTACL",13501,1000000,"10.9-0.213cap/1000","Not in Code","NA","IECC 2009\nkWh savings is calculated bsaed on EER & EFLH"]
["PTHP (New Construction)","PTHP80",0,8001,"12.3-0.213cap/1000","Not in Code","3.2-0.026cap/1000","IECC 2009\nkWh savings is calculated bsaed on EER, COP, & EFLH"]
["PTHP (New Construction)","PTHP105",8001,10501,"12.3-0.213cap/1000","Not in Code","3.2-0.026cap/1000","IECC 2009\nkWh savings is calculated bsaed on EER, COP, & EFLH"]
["PTHP (New Construction)","PTHP135",10501,13501,"12.3-0.213cap/1000","Not in Code","3.2-0.026cap/1000","IECC 2009\nkWh savings is calculated bsaed on EER, COP, & EFLH"]
["PTHP (New Construction)","PTHPL",13501,1000000,"12.3-0.213cap/1000","Not in Code","3.2-0.026cap/1000","IECC 2009\nkWh savings is calculated bsaed on EER, COP, & EFLH"]
["PTHP (Retrofit)","PTHP80",0,8001,"10.8-0.213cap/1000","Not in Code","2.9-0.026cap/1000","IECC 2009\nkWh savings is calculated bsaed on EER, COP, & EFLH"]
["PTHP (Retrofit)","PTHP105",8001,10501,"10.8-0.213cap/1000","Not in Code","2.9-0.026cap/1000","IECC 2009\nkWh savings is calculated bsaed on EER, COP, & EFLH"]
["PTHP (Retrofit)","PTHP135",10501,13501,"10.8-0.213cap/1000","Not in Code","2.9-0.026cap/1000","IECC 2009\nkWh savings is calculated bsaed on EER, COP, & EFLH"]
["PTHP (Retrofit)","PTHPL",13501,1000000,"10.8-0.213cap/1000","Not in Code","2.9-0.026cap/1000","IECC 2009\nkWh savings is calculated bsaed on EER, COP, & EFLH"]
[null,null,"BTUh (>=)","BTUh (<)","EER","IEER","COP","Baseline Reference"]
["3 Phase Unitary AC Single Package","AC3SP135",65000,135000,11.2,11.4,"NA","IECC 2012"]
["3 Phase Unitary AC Single Package","AC3SP240",135000,240000,11,11.2,"NA","IECC 2012"]
["3 Phase Unitary AC Single Package","AC3SP760",240000,760000,10,10.1,"NA","IECC 2012"]
["3 Phase Unitary AC Single Package","AC3SPL",760000,1000000,9.6999999999999993,9.8000000000000007,"NA","IECC 2012"]
["3 Phase Unitary AC Split System","AC3SS135",65000,135000,11.2,11.4,"NA","IECC 2012"]
["3 Phase Unitary AC Split System","AC3SS240",135000,240000,11,11.2,"NA","IECC 2012"]
["3 Phase Unitary AC Split System","AC3SS760",240000,760000,10,10.1,"NA","IECC 2012"]
["3 Phase Unitary AC Split System","AC3SSL",760000,1000000,9.6999999999999993,9.8000000000000007,"NA","IECC 2012"]
["3 Phase Heat Pump Single Package","HP3SP135",65000,135000,11,11.2,3.3,"IECC 2012"]
["3 Phase Heat Pump Single Package","HP3SP170",135000,170000,10.6,10.7,3.2,"IECC 2012"]
["3 Phase Heat Pump Single Package","HP3SP240",170000,240000,10.6,10.7,3.2,"IECC 2012"]
["3 Phase Heat Pump Single Package","HP3SPL",240000,1000000,9.5,9.6,3.2,"IECC 2012"]
["3 Phase Heat Pump Split System","HP3SS135",65000,135000,11,11.2,3.3,"IECC 2012"]
["3 Phase Heat Pump Split System","HP3SS170",135000,170000,10.6,10.7,3.2,"IECC 2012"]
["3 Phase Heat Pump Split System","HP3SS240",170000,240000,10.6,10.7,3.2,"IECC 2012"]
["3 Phase Heat Pump Split System","HP3SSL",240000,1000000,9.5,9.6,3.2,"IECC 2012"]
["VRF/Mini-Split AC","ACVRF135",65000,135000,11.2,13.1,"NA","ASHRAE 90.1-2010"]
["VRF/Mini-Split AC","ACVRF240",135000,240000,11,12.9,"NA","ASHRAE 90.1-2010"]
["VRF/Mini-Split AC","ACVRFL",240000,1000000,10,11.6,"NA","ASHRAE 90.1-2010"]
["VRF/Mini-Split HP","HPVRF135",65000,135000,11,12.9,3.3,"ASHRAE 90.1-2010"]
["VRF/Mini-Split HP W/ Heat Recovery",null,65000,135000,10.8,12.7,3.3,"ASHRAE 90.1-2010"]
["VRF/Mini-Split HP","HPVRF240",135000,240000,10.6,12.3,3.2,"ASHRAE 90.1-2010"]
["VRF/Mini-Split HP W/ Heat Recovery","HPVRF240R",135000,240000,10.4,12.1,3.2,"ASHRAE 90.1-2010"]
["VRF/Mini-Split HP","HPVRFL",240000,1000000,9.5,11,3.2,"ASHRAE 90.1-2010"]
["VRF/Mini-Split HP W/ Heat Recovery","HPVRFLR",240000,1000000,9.3000000000000007,10.8,3.2,"ASHRAE 90.1-2010"]
[null,null,"Tons",null,"kW/Ton","kW/Ton","-","-"]
["Air Cooled Chiller w/ Condenser","ACCC150",0,150,{"$f":"12/9.562","v":1.2549675800041833},{"$f":"12/12.5","v":0.96},"-","IECC 2009"]
["Air Cooled Chiller w/ Condenser","ACCCL",150,1000000,{"$f":"12/9.562","v":1.2549675800041833},{"$f":"12/12.75","v":0.94117647058823528},"-","IECC 2009"]
["Air Cooled Chiller w/o Condenser","ACC150",0,150,{"$f":"E55","v":1.2549675800041833},{"$f":"F55","v":0.96},"-","IECC 2009"]
["Air Cooled Chiller w/o Condenser","ACCL",150,1000000,{"$f":"E56","v":1.2549675800041833},{"$f":"F56","v":0.94117647058823528},"-","IECC 2009"]
["Water Cooled Chiller Non-Centrifugal","WCCRSS75",0,75,{"$f":"E63","v":0.78},{"$f":"F63","v":0.63},"-","IECC 2009"]
["Water Cooled Chiller Non-Centrifugal","WCCRSS150",75,150,{"$f":"E64","v":0.77500000000000002},0.61499999999999999,"-","IECC 2009"]
["Water Cooled Chiller Non-Centrifugal","WCCRSS300",150,300,0.68,0.57999999999999996,"-","IECC 2009"]
["Water Cooled Chiller Non-Centrifugal","WCCRSSL",300,1000000,0.62,0.54,"-","IECC 2009"]
["Water Cooled Chiller Reciprocating","WCCR75",0,75,0.78,0.63,"-","IECC 2009"]
["Water Cooled Chiller Reciprocating","WCCR150",75,150,0.77500000000000002,0.61499999999999999,"-","IECC 2009"]
["Water Cooled Chiller Reciprocating","WCCR300",150,300,0.68,0.57999999999999996,"-","IECC 2009"]
["Water Cooled Chiller Reciprocating","WCCRL",300,1000000,0.62,0.54,"-","IECC 2009"]
["Water Cooled Chiller Centrifugal","WCCC150",0,150,0.63400000000000001,0.59599999999999997,"-","IECC 2009"]
["Water Cooled Chiller Centrifugal","WCCC300",150,300,0.63400000000000001,0.59599999999999997,"-","IECC 2009"]
["Water Cooled Chiller Centrifugal","WCCC600",300,600,0.57599999999999996,0.54900000000000004,"-","IECC 2009"]
["Water Cooled Chiller Centrifugal","WCCCL",600,1000000,0.56999999999999995,0.53900000000000003,"-","IECC 2009"]

{"sheet":"Change Log","index":8,"n_rows":6,"n_cols":3,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["Date","Engineer","Change"]
["2022-02-18","Brian Ng & Hang Zhang","Update 1: Only provide rebate for 3-ph equipment that generate kWh savings and >=0 kW savings. 2022 Program Manual states that rebate is calculated based on $0.3/kWh saved.\nUpdate 2: Rebate will not be calculated if user did not enter all the required efficiencies. “Enter efficiency” message will be shown in the calculator.\nUpdate 3: Checked and update code efficiencies are per IECC 2009 except \no\t3-phase AC & HP to follow IECC 2012 as stated in 2022 SC Program Manual and \no\tVRF/Mini-Split to follow ASHRAE 90.1-2010 because IECC 2009 and 2012 do not have VRF efficiency\nUpdate 4: Tier 1 & 2 efficiencies are checked to align with 2022 SC Program Manual\nUpdate 5: Fixed the PTAC and PTHP capacity categorization errors. For example, the program manual says <= 8000 btuh, but the calculator pushing 8000 btuh unit to the next category up. \nUpdate 6: Checked and observed that the majority of the Tier 1 efficiencies are equal to code, but some are above (mostly VRF). \nUpdate 7: Checked no code requirement for the orange highlighted efficiencies.\nUpdate 8: Added a \"Change log\" tab in the calculator as a hidden tab"]
["2022-02-28","Brian Ng & Hang Zhang","Update 1: Removed EER for units<65000 btuh (not listed in code/standard). Use SEER and EFLH to calculate kW savings\nUpdate 2: Removed SEER for PTAS & PTHP (not listed in code/standard). Use EER and EFLH to calculate kWh savings\nUpdate 3: Added \"Appendix E (Ref. Table)\" tab"]
["2024-04-02","Mancel Fincher","Added measures for SEER2/HSPF2; efficiency ratings based on eCFR, Table Table 19 to § 431.97(h)."]
["2024-08-29","Mancel Fincher","Reviewed to ensure the current energy code is used. Updated the version.\nAdded \"VRF/Mini-Split HP W/ Heat Recovery\" for the 65-135 kBtu/h range (measure is missing)."]
["2024-10-02","Mancel Fincher","Updated the Empower Business logo."]